;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##;"►qol##OTHER##"""
AGAT CLEAN SLIGHT LED 2600 OPTICS-1L SH IP65 E 34 840 / 600X600;Clean luminaires - recessed;19.3188.0001.34;595 x 595 x 35;mounted in module ceilings;14.4;1908;133;4000;4000;0.7291;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_SH (transparent hardened glass);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 106,6° / 86,8°;IP65;IK08;I;0;0.95;595;595;35;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/19.3188.0001.34/;19.3188.0001.34.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
AGAT CLEAN SLIGHT LED 2600 OPTICS-2L SH IP65 E 34 840 / 600X600;Clean luminaires - recessed;19.3188.0002.34;595 x 595 x 35;mounted in module ceilings;14.4;2199;153;4000;4000;0.8403;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_SH (transparent hardened glass);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 56,4° / 92,6°;IP65;IK08;I;0;0.95;595;595;35;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/19.3188.0002.34/;19.3188.0002.34.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
AGAT CLEAN SLIGHT LED 2600 OPTICS-3L SH IP65 E 34 840 / 600X600;Clean luminaires - recessed;19.3188.0003.34;595 x 595 x 35;mounted in module ceilings;14.4;1967;137;4000;4000;0.7516;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_SH (transparent hardened glass);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;Rozsył asymetryczny - Imax=-24°;IP65;IK08;I;0;0.95;595;595;35;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/19.3188.0003.34/;19.3188.0003.34.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
AGAT CLEAN SLIGHT LED 3900 OPTICS-1L SH IP65 E 34 840 / 600X600;Clean luminaires - recessed;19.3188.0004.34;595 x 595 x 35;mounted in module ceilings;21.7;2862;132;4000;4000;0.7291;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_SH (transparent hardened glass);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 106,6° / 86,8°;IP65;IK08;I;0;0.95;595;595;35;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/19.3188.0004.34/;19.3188.0004.34.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;3
AGAT CLEAN SLIGHT LED 3900 OPTICS-2L SH IP65 E 34 840 / 600X600;Clean luminaires - recessed;19.3188.0005.34;595 x 595 x 35;mounted in module ceilings;21.7;3299;152;4000;4000;0.8403;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_SH (transparent hardened glass);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 56,4° / 92,6°;IP65;IK08;I;0;0.95;595;595;35;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/19.3188.0005.34/;19.3188.0005.34.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;3
AGAT CLEAN SLIGHT LED 3900 OPTICS-3L SH IP65 E 34 840 / 600X600;Clean luminaires - recessed;19.3188.0006.34;595 x 595 x 35;mounted in module ceilings;21.7;2951;136;4000;4000;0.7516;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_SH (transparent hardened glass);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;Rozsył asymetryczny - Imax=-24°;IP65;IK08;I;0;0.95;595;595;35;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/19.3188.0006.34/;19.3188.0006.34.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;3
AGAT CLEAN SLIGHT LED 4400 OPTICS-1L SH IP65 E 34 840 / 600X600;Clean luminaires - recessed;19.3188.0007.34;595 x 595 x 35;mounted in module ceilings;24.7;3328;135;4000;4000;0.7291;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_SH (transparent hardened glass);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 106,6° / 86,8°;IP65;IK08;I;0;0.95;595;595;35;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/19.3188.0007.34/;19.3188.0007.34.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
AGAT CLEAN SLIGHT LED 4400 OPTICS-2L SH IP65 E 34 840 / 600X600;Clean luminaires - recessed;19.3188.0008.34;595 x 595 x 35;mounted in module ceilings;24.7;3836;155;4000;4000;0.8403;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_SH (transparent hardened glass);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 56,4° / 92,6°;IP65;IK08;I;0;0.95;595;595;35;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/19.3188.0008.34/;19.3188.0008.34.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
AGAT CLEAN SLIGHT LED 4400 OPTICS-3L SH IP65 E 34 840 / 600X600;Clean luminaires - recessed;19.3188.0009.34;595 x 595 x 35;mounted in module ceilings;24.7;3431;139;4000;4000;0.7516;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_SH (transparent hardened glass);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;Rozsył asymetryczny - Imax=-24°;IP65;IK08;I;0;0.95;595;595;35;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/19.3188.0009.34/;19.3188.0009.34.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
AGAT CLEAN SLIGHT LED 5200 OPTICS-2L SH IP65 E 34 840 / 600X600;Clean luminaires - recessed;19.3188.0010.34;595 x 595 x 35;mounted in module ceilings;28.2;4398;156;4000;4000;0.8403;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_SH (transparent hardened glass);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 56,4° / 92,6°;IP65;IK08;I;0;0.95;595;595;35;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/19.3188.0010.34/;19.3188.0010.34.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;4
AGAT CLEAN SLIGHT LED 5200 OPTICS-3L SH IP65 E 34 840 / 600X600;Clean luminaires - recessed;19.3188.0011.34;595 x 595 x 35;mounted in module ceilings;28.2;3934;139;4000;4000;0.7516;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_SH (transparent hardened glass);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;Rozsył asymetryczny - Imax=-24°;IP65;IK08;I;0;0.95;595;595;35;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/19.3188.0011.34/;19.3188.0011.34.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;4
AGAT CLEAN SLIGHT LED 6600 OPTICS-1L SH IP65 E 34 840 / 600X600;Clean luminaires - recessed;19.3188.0012.34;595 x 595 x 35;mounted in module ceilings;35.3;4993;141;4000;4000;0.7291;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_SH (transparent hardened glass);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 106,6° / 86,8°;IP65;IK08;I;0;0.95;595;595;35;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/19.3188.0012.34/;19.3188.0012.34.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;3
AGAT CLEAN SLIGHT LED 6600 OPTICS-2L SH IP65 E 34 840 / 600X600;Clean luminaires - recessed;19.3188.0013.34;595 x 595 x 35;mounted in module ceilings;35.3;5754;163;4000;4000;0.8403;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_SH (transparent hardened glass);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 56,4° / 92,6°;IP65;IK08;I;0;0.95;595;595;35;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/19.3188.0013.34/;19.3188.0013.34.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;3
AGAT CLEAN SLIGHT LED 6600 OPTICS-3L SH IP65 E 34 840 / 600X600;Clean luminaires - recessed;19.3188.0014.34;595 x 595 x 35;mounted in module ceilings;35.3;5147;146;4000;4000;0.7516;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_SH (transparent hardened glass);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;Rozsył asymetryczny - Imax=-24°;IP65;IK08;I;0;0.95;595;595;35;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/19.3188.0014.34/;19.3188.0014.34.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;3
AGAT CLEAN SLIGHT LED 8800 OPTICS-1L SH IP65 E 34 840 / 600X600;Clean luminaires - recessed;19.3188.0015.34;595 x 595 x 35;mounted in module ceilings;49.1;6657;136;4000;4000;0.7291;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_SH (transparent hardened glass);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 106,6° / 86,8°;IP65;IK08;I;0;0.95;595;595;35;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/19.3188.0015.34/;19.3188.0015.34.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;4
AGAT CLEAN SLIGHT LED 8800 OPTICS-2L SH IP65 E 34 840 / 600X600;Clean luminaires - recessed;19.3188.0016.34;595 x 595 x 35;mounted in module ceilings;49.1;7672;156;4000;4000;0.8403;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_SH (transparent hardened glass);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 56,4° / 92,6°;IP65;IK08;I;0;0.95;595;595;35;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/19.3188.0016.34/;19.3188.0016.34.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;4
AGAT CLEAN SLIGHT LED 8800 OPTICS-3L SH IP65 E 34 840 / 600X600;Clean luminaires - recessed;19.3188.0017.34;595 x 595 x 35;mounted in module ceilings;49.1;6862;140;4000;4000;0.7516;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_SH (transparent hardened glass);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;Rozsył asymetryczny - Imax=-24°;IP65;IK08;I;0;0.95;595;595;35;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/agat-clean-slight-led/19.3188.0017.34/;19.3188.0017.34.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;4
