;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
AGAT SLIM LED 2600 PLX E 34 830;Recessed luminaires;19.3043.0110.34;591 x 115 x 88;mounted in module ceilings;14.4;1946;135;3000;3000;0.7706;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 101,2° / 103,2°;IP20;IK04;I;0;0,95;591;115;88;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/19.3043.0110.34/;19.3043.0110.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
AGAT SLIM LED 2600 PLX E 34 840;Recessed luminaires;19.3043.0109.34;591 x 115 x 88;mounted in module ceilings;14.4;2017;140;4000;4000;0.7706;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 101,2° / 103,2°;IP20;IK04;I;0;0,95;591;115;88;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/19.3043.0109.34/;19.3043.0109.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
AGAT SLIM LED 2600 PLX EDD 34 830;Recessed luminaires;19.3043.0111.34;591 x 115 x 88;mounted in module ceilings;14.4;1946;135;3000;3000;0.7706;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 101,2° / 103,2°;IP20;IK04;I;0;0,95;591;115;88;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/19.3043.0111.34/;19.3043.0111.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
AGAT SLIM LED 2600 PLX EDD 34 840;Recessed luminaires;19.3043.0117.34;591 x 115 x 88;mounted in module ceilings;14.4;2017;140;4000;4000;0.7706;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 101,2° / 103,2°;IP20;IK04;I;0;0,95;591;115;88;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/19.3043.0117.34/;19.3043.0117.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
AGAT SLIM LED 4400 PLX E 34 830;Recessed luminaires;19.3043.0124.34;591 x 115 x 88;mounted in module ceilings;24.7;3395;137;3000;3000;0.7706;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 101,2° / 103,2°;IP20;IK04;I;0;0,95;591;115;88;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/19.3043.0124.34/;19.3043.0124.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
AGAT SLIM LED 4400 PLX E 34 840;Recessed luminaires;19.3043.0123.34;591 x 115 x 88;mounted in module ceilings;24.7;3518;142;4000;4000;0.7706;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 101,2° / 103,2°;IP20;IK04;I;0;0,95;591;115;88;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/19.3043.0123.34/;19.3043.0123.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
AGAT SLIM LED 4400 PLX EDD 34 830;Recessed luminaires;19.3043.0131.34;591 x 115 x 88;mounted in module ceilings;24.7;3395;137;3000;3000;0.7706;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 101,2° / 103,2°;IP20;IK04;I;0;0,95;591;115;88;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/19.3043.0131.34/;19.3043.0131.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
AGAT SLIM LED 4400 PLX EDD 34 840;Recessed luminaires;19.3043.0130.34;591 x 115 x 88;mounted in module ceilings;24.7;3518;142;4000;4000;0.7706;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 101,2° / 103,2°;IP20;IK04;I;0;0,95;591;115;88;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/19.3043.0130.34/;19.3043.0130.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
AGAT SLIM LED 5200 PLX E 34 830 / L-1200;Recessed luminaires;19.3043.0212.34;1196 x 115 x 88;mounted in module ceilings;28.2;3892;138;3000;3000;0.7706;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 101,2° / 103,2°;IP20;IK04;I;0;0,95;1196;115;88;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/19.3043.0212.34/;19.3043.0212.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
AGAT SLIM LED 5200 PLX E 34 840 / L-1200;Recessed luminaires;19.3043.0211.34;1196 x 115 x 88;mounted in module ceilings;28.2;4033;143;4000;4000;0.7706;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 101,2° / 103,2°;IP20;IK04;I;0;0,95;1196;115;88;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/19.3043.0211.34/;19.3043.0211.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
AGAT SLIM LED 5200 PLX EDD 34 830 / L-1200;Recessed luminaires;19.3043.0214.34;1196 x 115 x 88;mounted in module ceilings;28.2;3892;138;3000;3000;0.7706;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 101,2° / 103,2°;IP20;IK04;I;0;0,95;1196;115;88;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/19.3043.0214.34/;19.3043.0214.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
AGAT SLIM LED 5200 PLX EDD 34 840 / L-1200;Recessed luminaires;19.3043.0213.34;1196 x 115 x 88;mounted in module ceilings;28.2;4033;143;4000;4000;0.7706;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 101,2° / 103,2°;IP20;IK04;I;0;0,95;1196;115;88;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/agat-slim-led/19.3043.0213.34/;19.3043.0213.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
