;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
ANGLE 2500 20° E 21 830;Recessed luminaires;19.3201.0001.21;?151 x 125;mounted in suspended ceiling;18.4;2520;137;3000;3000;0.8347;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 22,4° / 22,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0001.21/;19.3201.0001.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 20° E 21 840;Recessed luminaires;19.3201.0002.21;?151 x 125;mounted in suspended ceiling;18.4;2594;141;4000;4000;0.8347;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 22,4° / 22,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0002.21/;19.3201.0002.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 20° E 33 830;Recessed luminaires;19.3201.0001.33;?151 x 125;mounted in suspended ceiling;21;2043;97;3000;3000;0.8347;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 22,4° / 22,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0001.33/;19.3201.0001.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 20° E 33 840;Recessed luminaires;19.3201.0002.33;?151 x 125;mounted in suspended ceiling;21;2104;100;4000;4000;0.8347;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 22,4° / 22,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0002.33/;19.3201.0002.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 20° EDD 21 830;Recessed luminaires;19.3201.0003.21;?151 x 125;mounted in suspended ceiling;18.4;2520;137;3000;3000;0.8347;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 22,4° / 22,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0003.21/;19.3201.0003.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 20° EDD 21 840;Recessed luminaires;19.3201.0004.21;?151 x 125;mounted in suspended ceiling;18.4;2594;141;4000;4000;0.8347;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 22,4° / 22,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0004.21/;19.3201.0004.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 20° EDD 33 830;Recessed luminaires;19.3201.0003.33;?151 x 125;mounted in suspended ceiling;21;2043;97;3000;3000;0.8347;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 22,4° / 22,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0003.33/;19.3201.0003.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 20° EDD 33 840;Recessed luminaires;19.3201.0004.33;?151 x 125;mounted in suspended ceiling;21;2104;100;4000;4000;0.8347;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 22,4° / 22,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0004.33/;19.3201.0004.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 40° E 21 830;Recessed luminaires;19.3201.0005.21;?151 x 125;mounted in suspended ceiling;18.4;2531;138;3000;3000;0.8385;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 33,4° / 33,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0005.21/;19.3201.0005.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 40° E 21 840;Recessed luminaires;19.3201.0006.21;?151 x 125;mounted in suspended ceiling;18.4;2606;142;4000;4000;0.8385;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 33,4° / 33,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0006.21/;19.3201.0006.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 40° E 33 830;Recessed luminaires;19.3201.0005.33;?151 x 125;mounted in suspended ceiling;21;2053;98;3000;3000;0.8385;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 33,4° / 33,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0005.33/;19.3201.0005.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 40° E 33 840;Recessed luminaires;19.3201.0006.33;?151 x 125;mounted in suspended ceiling;21;2114;101;4000;4000;0.8385;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 33,4° / 33,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0006.33/;19.3201.0006.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 40° EDD 21 830;Recessed luminaires;19.3201.0007.21;?151 x 125;mounted in suspended ceiling;18.4;2531;138;3000;3000;0.8385;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 33,4° / 33,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0007.21/;19.3201.0007.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 40° EDD 21 840;Recessed luminaires;19.3201.0008.21;?151 x 125;mounted in suspended ceiling;18.4;2606;142;4000;4000;0.8385;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 33,4° / 33,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0008.21/;19.3201.0008.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 40° EDD 33 830;Recessed luminaires;19.3201.0007.33;?151 x 125;mounted in suspended ceiling;21;2053;98;3000;3000;0.8385;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 33,4° / 33,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0007.33/;19.3201.0007.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 40° EDD 33 840;Recessed luminaires;19.3201.0008.33;?151 x 125;mounted in suspended ceiling;21;2114;101;4000;4000;0.8385;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 33,4° / 33,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0008.33/;19.3201.0008.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 60° E 21 830;Recessed luminaires;19.3201.0009.21;?151 x 125;mounted in suspended ceiling;18.4;2398;130;3000;3000;0.7944;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 53,2° / 53,2°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0009.21/;19.3201.0009.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 60° E 21 840;Recessed luminaires;19.3201.0010.21;?151 x 125;mounted in suspended ceiling;18.4;2469;134;4000;4000;0.7944;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 53,2° / 53,2°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0010.21/;19.3201.0010.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 60° E 33 830;Recessed luminaires;19.3201.0009.33;?151 x 125;mounted in suspended ceiling;21;1945;93;3000;3000;0.7944;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 53,2° / 53,2°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0009.33/;19.3201.0009.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 60° E 33 840;Recessed luminaires;19.3201.0010.33;?151 x 125;mounted in suspended ceiling;21;2003;95;4000;4000;0.7944;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 53,2° / 53,2°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0010.33/;19.3201.0010.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 60° EDD 21 830;Recessed luminaires;19.3201.0011.21;?151 x 125;mounted in suspended ceiling;18.4;2398;130;3000;3000;0.7944;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 53,2° / 53,2°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0011.21/;19.3201.0011.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 60° EDD 21 840;Recessed luminaires;19.3201.0012.21;?151 x 125;mounted in suspended ceiling;18.4;2469;134;4000;4000;0.7944;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 53,2° / 53,2°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0012.21/;19.3201.0012.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 60° EDD 33 830;Recessed luminaires;19.3201.0011.33;?151 x 125;mounted in suspended ceiling;21;1945;93;3000;3000;0.7944;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 53,2° / 53,2°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0011.33/;19.3201.0011.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 2500 60° EDD 33 840;Recessed luminaires;19.3201.0012.33;?151 x 125;mounted in suspended ceiling;21;2003;95;4000;4000;0.7944;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 53,2° / 53,2°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0012.33/;19.3201.0012.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 20° E 21 830;Recessed luminaires;19.3201.0013.21;?151 x 125;mounted in suspended ceiling;26.4;3335;126;3000;3000;0.8347;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 22,4° / 22,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0013.21/;19.3201.0013.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 20° E 21 840;Recessed luminaires;19.3201.0014.21;?151 x 125;mounted in suspended ceiling;26.4;3431;130;4000;4000;0.8347;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 22,4° / 22,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0014.21/;19.3201.0014.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 20° E 33 830;Recessed luminaires;19.3201.0013.33;?151 x 125;mounted in suspended ceiling;28;3025;108;3000;3000;0.8347;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 22,4° / 22,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0013.33/;19.3201.0013.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 20° E 33 840;Recessed luminaires;19.3201.0014.33;?151 x 125;mounted in suspended ceiling;28;3114;111;4000;4000;0.8347;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 22,4° / 22,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0014.33/;19.3201.0014.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 20° EDD 21 830;Recessed luminaires;19.3201.0015.21;?151 x 125;mounted in suspended ceiling;26.4;3335;126;3000;3000;0.8347;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 22,4° / 22,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0015.21/;19.3201.0015.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 20° EDD 21 840;Recessed luminaires;19.3201.0016.21;?151 x 125;mounted in suspended ceiling;26.4;3431;130;4000;4000;0.8347;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 22,4° / 22,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0016.21/;19.3201.0016.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 20° EDD 33 830;Recessed luminaires;19.3201.0015.33;?151 x 125;mounted in suspended ceiling;28;3025;108;3000;3000;0.8347;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 22,4° / 22,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0015.33/;19.3201.0015.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 20° EDD 33 840;Recessed luminaires;19.3201.0016.33;?151 x 125;mounted in suspended ceiling;28;3114;111;4000;4000;0.8347;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 22,4° / 22,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0016.33/;19.3201.0016.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 40° E 21 830;Recessed luminaires;19.3201.0017.21;?151 x 125;mounted in suspended ceiling;26.4;3350;127;3000;3000;0.8385;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 33,4° / 33,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0017.21/;19.3201.0017.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 40° E 21 840;Recessed luminaires;19.3201.0018.21;?151 x 125;mounted in suspended ceiling;26.4;3447;131;4000;4000;0.8385;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 33,4° / 33,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0018.21/;19.3201.0018.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 40° E 33 830;Recessed luminaires;19.3201.0017.33;?151 x 125;mounted in suspended ceiling;28;3039;109;3000;3000;0.8385;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 33,4° / 33,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0017.33/;19.3201.0017.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 40° E 33 840;Recessed luminaires;19.3201.0018.33;?151 x 125;mounted in suspended ceiling;28;3128;112;4000;4000;0.8385;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 33,4° / 33,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0018.33/;19.3201.0018.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 40° EDD 21 830;Recessed luminaires;19.3201.0019.21;?151 x 125;mounted in suspended ceiling;26.4;3350;127;3000;3000;0.8385;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 33,4° / 33,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0019.21/;19.3201.0019.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 40° EDD 21 840;Recessed luminaires;19.3201.0020.21;?151 x 125;mounted in suspended ceiling;26.4;3447;131;4000;4000;0.8385;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 33,4° / 33,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0020.21/;19.3201.0020.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 40° EDD 33 830;Recessed luminaires;19.3201.0019.33;?151 x 125;mounted in suspended ceiling;28;3039;109;3000;3000;0.8385;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 33,4° / 33,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0019.33/;19.3201.0019.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 40° EDD 33 840;Recessed luminaires;19.3201.0020.33;?151 x 125;mounted in suspended ceiling;28;3128;112;4000;4000;0.8385;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 33,4° / 33,4°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0020.33/;19.3201.0020.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 60° E 21 830;Recessed luminaires;19.3201.0021.21;?151 x 125;mounted in suspended ceiling;26.4;3174;120;3000;3000;0.7944;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 53,2° / 53,2°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0021.21/;19.3201.0021.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 60° E 21 840;Recessed luminaires;19.3201.0022.21;?151 x 125;mounted in suspended ceiling;26.4;3266;124;4000;4000;0.7944;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 53,2° / 53,2°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0022.21/;19.3201.0022.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 60° E 33 830;Recessed luminaires;19.3201.0021.33;?151 x 125;mounted in suspended ceiling;28;2879;103;3000;3000;0.7944;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 53,2° / 53,2°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0021.33/;19.3201.0021.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 60° E 33 840;Recessed luminaires;19.3201.0022.33;?151 x 125;mounted in suspended ceiling;28;2964;106;4000;4000;0.7944;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 53,2° / 53,2°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0022.33/;19.3201.0022.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 60° EDD 21 830;Recessed luminaires;19.3201.0023.21;?151 x 125;mounted in suspended ceiling;26.4;3174;120;3000;3000;0.7944;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 53,2° / 53,2°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0023.21/;19.3201.0023.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 60° EDD 21 840;Recessed luminaires;19.3201.0024.21;?151 x 125;mounted in suspended ceiling;26.4;3266;124;4000;4000;0.7944;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_hardened transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 53,2° / 53,2°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0024.21/;19.3201.0024.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 60° EDD 33 830;Recessed luminaires;19.3201.0023.33;?151 x 125;mounted in suspended ceiling;28;2879;103;3000;3000;0.7944;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 53,2° / 53,2°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0023.33/;19.3201.0023.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ANGLE 3700 60° EDD 33 840;Recessed luminaires;19.3201.0024.33;?151 x 125;mounted in suspended ceiling;28;2964;106;4000;4000;0.7944;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_hardened transparent glass;LED;5 ÷ 30;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 53,2° / 53,2°;IP20/44;IK04;II;0;0.95;125;151;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/;https://luxiona.pl/oferta/oprawy-do-wbudowania/angle/19.3201.0024.33/;19.3201.0024.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
