;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
ARTSHAPE SIX LED SMALL FULL UP&DOWN 2800/5500 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3004.1021.34;650 x 592 x 85;surface mounted on slings;68.0;6567;97;4000;4000;0.7881;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;35000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP20;IK04;I;0;0,95;650;592;85;0;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.1021.34/;19.3004.1021.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE SIX LED MEDIUM FULL UP&DOWN 4000/12000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3004.2015.34;900 x 809 x 85;surface mounted on slings;135.0;13110;97;4000;4000;0.7722;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;35000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP20;IK04;I;0;0,95;900;809;85;0;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.2015.34/;19.3004.2015.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE SIX LED LARGE FULL UP&DOWN 5000/21000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3004.3013.34;1170 x 1043 x 85;surface mounted on slings;218.0;20738;95;4000;4000;0.7652;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;35000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP20;IK04;I;0;0,95;1170;1043;85;0;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.3013.34/;19.3004.3013.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA