;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##;LSDepth##LENGTH##MILLIMETERS
ATENA LINE NEW LED INDUSTRY 18000 SH MEDIUM E IP65 04 850 / HT50;Industrial luminaires;19.3126.0001.04;465 x 201 x 150;directly mounted to ceiling construction or surface mounted on slings;110;14568;132;5000;5000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 50;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;465;201;150;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/19.3126.0001.04/;19.3126.0001.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW LED INDUSTRY 18000 SH WIDE E IP65 04 850 / HT50;Industrial luminaires;19.3126.0002.04;465 x 201 x 150;directly mounted to ceiling construction or surface mounted on slings;110;14968;136;5000;5000;0.8727;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 50;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;465;201;150;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/19.3126.0002.04/;19.3126.0002.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW LED INDUSTRY 18000 SH WIDE ODB E IP65 04 850 / HT50;Industrial luminaires;19.3126.0003.04;465 x 201 x 150;directly mounted to ceiling construction or surface mounted on slings;110;13604;124;5000;5000;0.7932;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 50;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;465;201;150;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/19.3126.0003.04/;19.3126.0003.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45
ATENA LINE NEW LED INDUSTRY 24000 SH MEDIUM E IP65 04 850 / HT50;Industrial luminaires;19.3126.0004.04;680 x 201 x 150;directly mounted to ceiling construction or surface mounted on slings;146;18939;130;5000;5000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 50;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;680;201;150;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/19.3126.0004.04/;19.3126.0004.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW LED INDUSTRY 24000 SH WIDE E IP65 04 850 / HT50;Industrial luminaires;19.3126.0005.04;680 x 201 x 150;directly mounted to ceiling construction or surface mounted on slings;146;19459;133;5000;5000;0.8727;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 50;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;680;201;150;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/19.3126.0005.04/;19.3126.0005.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW LED INDUSTRY 24000 SH WIDE ODB E IP65 04 850 / HT50;Industrial luminaires;19.3126.0006.04;680 x 201 x 150;directly mounted to ceiling construction or surface mounted on slings;146;17686;121;5000;5000;0.7932;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 50;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;680;201;150;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/19.3126.0006.04/;19.3126.0006.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45
ATENA LINE NEW LED INDUSTRY 30000 SH MEDIUM E IP65 04 850 / HT50;Industrial luminaires;19.3126.0007.04;785 x 201 x 150;directly mounted to ceiling construction or surface mounted on slings;195;24475;126;5000;5000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 50;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;785;201;150;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/19.3126.0007.04/;19.3126.0007.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW LED INDUSTRY 30000 SH WIDE E IP65 04 850 / HT50;Industrial luminaires;19.3126.0008.04;785 x 201 x 150;directly mounted to ceiling construction or surface mounted on slings;195;25146;129;5000;5000;0.8727;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 50;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;785;201;150;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/19.3126.0008.04/;19.3126.0008.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW LED INDUSTRY 30000 SH WIDE ODB E IP65 04 850 / HT50;Industrial luminaires;19.3126.0009.04;785 x 201 x 150;directly mounted to ceiling construction or surface mounted on slings;195;22855;117;5000;5000;0.7932;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 50;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;785;201;150;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/19.3126.0009.04/;19.3126.0009.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45
ATENA LINE NEW LED INDUSTRY 36000 SH MEDIUM E IP65 04 850 / HT50;Industrial luminaires;19.3126.0010.04;885 x 201 x 150;directly mounted to ceiling construction or surface mounted on slings;233;29137;125;5000;5000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 50;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;885;201;150;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/19.3126.0010.04/;19.3126.0010.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW LED INDUSTRY 36000 SH WIDE E IP65 04 850 / HT50;Industrial luminaires;19.3126.0011.04;885 x 201 x 150;directly mounted to ceiling construction or surface mounted on slings;233;29936;128;5000;5000;0.8727;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 50;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;885;201;150;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/19.3126.0011.04/;19.3126.0011.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW LED INDUSTRY 36000 SH WIDE ODB E IP65 04 850 / HT50;Industrial luminaires;19.3126.0012.04;885 x 201 x 150;directly mounted to ceiling construction or surface mounted on slings;233;27209;117;5000;5000;0.7932;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 50;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;885;201;150;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-led-industry/19.3126.0012.04/;19.3126.0012.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45
