;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##;LSDepth##LENGTH##MILLIMETERS
ATENA LINE NEW OUTDOOR LED 12000 SH MEDIUM E IP65 04 840;Outdoor luminaires;19.3138.0003.04;430 x 201 x 150;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";83;10050;121;4000;4000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;430;201;150;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0003.04/;19.3138.0003.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW OUTDOOR LED 12000 SH MEDIUM E IP65 04 840 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0004.04;430 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";83;10050;121;4000;4000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;430;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0004.04/;19.3138.0004.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW OUTDOOR LED 12000 SH MEDIUM E IP65 04 850;Outdoor luminaires;19.3138.0001.04;430 x 201 x 150;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";81;10198;126;5000;5000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;430;201;150;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0001.04/;19.3138.0001.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW OUTDOOR LED 12000 SH MEDIUM E IP65 04 850 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0002.04;430 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";81;10198;126;5000;5000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;430;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0002.04/;19.3138.0002.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW OUTDOOR LED 12000 SH WIDE ODB E IP65 04 840 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0006.04;430 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";83;9385;113;4000;4000;0.7932;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;430;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0006.04/;19.3138.0006.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45
ATENA LINE NEW OUTDOOR LED 12000 SH WIDE ODB E IP65 04 850 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0005.04;430 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";81;9523;118;5000;5000;0.7932;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;430;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0005.04/;19.3138.0005.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45
ATENA LINE NEW OUTDOOR LED 18000 SH MEDIUM E IP65 04 840;Outdoor luminaires;19.3138.0009.04;430 x 201 x 150;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";105;15829;151;4000;4000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;430;201;150;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0009.04/;19.3138.0009.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW OUTDOOR LED 18000 SH MEDIUM E IP65 04 840 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0010.04;430 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";105;15829;151;4000;4000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;430;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0010.04/;19.3138.0010.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW OUTDOOR LED 18000 SH MEDIUM E IP65 04 850;Outdoor luminaires;19.3138.0007.04;430 x 201 x 150;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";105;16061;153;5000;5000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;430;201;150;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0007.04/;19.3138.0007.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW OUTDOOR LED 18000 SH MEDIUM E IP65 04 850 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0008.04;430 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";105;16061;153;5000;5000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;430;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0008.04/;19.3138.0008.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW OUTDOOR LED 18000 SH WIDE ODB E IP65 04 840 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0012.04;430 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";105;14781;141;4000;4000;0.7932;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;430;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0012.04/;19.3138.0012.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45
ATENA LINE NEW OUTDOOR LED 18000 SH WIDE ODB E IP65 04 850 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0011.04;430 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";105;14999;143;5000;5000;0.7932;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;430;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0011.04/;19.3138.0011.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45
ATENA LINE NEW OUTDOOR LED 24000 SH MEDIUM E IP65 04 840;Outdoor luminaires;19.3138.0015.04;465 x 201 x 150;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";138;21105;153;4000;4000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;465;201;150;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0015.04/;19.3138.0015.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW OUTDOOR LED 24000 SH MEDIUM E IP65 04 840 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0016.04;465 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";138;21105;153;4000;4000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;465;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0016.04/;19.3138.0016.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW OUTDOOR LED 24000 SH MEDIUM E IP65 04 850;Outdoor luminaires;19.3138.0013.04;465 x 201 x 150;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";138;21416;155;5000;5000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;465;201;150;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0013.04/;19.3138.0013.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW OUTDOOR LED 24000 SH MEDIUM E IP65 04 850 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0014.04;465 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";138;21416;155;5000;5000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;465;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0014.04/;19.3138.0014.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
ATENA LINE NEW OUTDOOR LED 24000 SH WIDE ODB E IP65 04 840 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0018.04;465 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";138;19709;143;4000;4000;0.7932;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;465;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0018.04/;19.3138.0018.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45
ATENA LINE NEW OUTDOOR LED 24000 SH WIDE ODB E IP65 04 850 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0017.04;465 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";138;19999;145;5000;5000;0.7932;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;465;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0017.04/;19.3138.0017.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45
