;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
ATENA LINE NEW OUTDOOR LED 12000 SH ASY E IP65 04 840;Outdoor luminaires;19.3138.0019.04;430 x 201 x 150;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";83;8713;105;4000;4000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;430;201;150;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0019.04/;19.3138.0019.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ATENA LINE NEW OUTDOOR LED 12000 SH ASY E IP65 04 840 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0020.04;430 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";83;8713;105;4000;4000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;430;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0020.04/;19.3138.0020.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ATENA LINE NEW OUTDOOR LED 12000 SH ASY E IP65 04 850;Outdoor luminaires;19.3138.0021.04;430 x 201 x 150;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";81;8841;109;5000;5000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;430;201;150;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0021.04/;19.3138.0021.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ATENA LINE NEW OUTDOOR LED 12000 SH ASY E IP65 04 850 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0022.04;430 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";81;8841;109;5000;5000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;430;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0022.04/;19.3138.0022.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ATENA LINE NEW OUTDOOR LED 18000 SH ASY E IP65 04 840;Outdoor luminaires;19.3138.0023.04;430 x 201 x 150;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";105;13723;131;4000;4000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;430;201;150;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0023.04/;19.3138.0023.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ATENA LINE NEW OUTDOOR LED 18000 SH ASY E IP65 04 840 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0024.04;430 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";105;13723;131;4000;4000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;430;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0024.04/;19.3138.0024.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ATENA LINE NEW OUTDOOR LED 18000 SH ASY E IP65 04 850;Outdoor luminaires;19.3138.0025.04;430 x 201 x 150;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";105;13925;133;5000;5000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;430;201;150;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0025.04/;19.3138.0025.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ATENA LINE NEW OUTDOOR LED 18000 SH ASY E IP65 04 850 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0026.04;430 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";105;13925;133;5000;5000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;430;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0026.04/;19.3138.0026.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ATENA LINE NEW OUTDOOR LED 24000 SH ASY E IP65 04 840;Outdoor luminaires;19.3138.0027.04;465 x 201 x 150;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";138;18297;133;4000;4000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;465;201;150;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0027.04/;19.3138.0027.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ATENA LINE NEW OUTDOOR LED 24000 SH ASY E IP65 04 840 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0028.04;465 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";138;18297;133;4000;4000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;465;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0028.04/;19.3138.0028.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ATENA LINE NEW OUTDOOR LED 24000 SH ASY E IP65 04 850;Outdoor luminaires;19.3138.0029.04;465 x 201 x 150;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";138;18567;135;5000;5000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;465;201;150;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0029.04/;19.3138.0029.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ATENA LINE NEW OUTDOOR LED 24000 SH ASY E IP65 04 850 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0030.04;465 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";138;18567;135;5000;5000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;465;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0030.04/;19.3138.0030.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ATENA LINE NEW OUTDOOR LED 30000 SH ASY E IP65 04 840;Outdoor luminaires;19.3138.0031.04;588 x 201 x 150;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";177;22872;129;4000;4000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;588;201;150;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0031.04/;19.3138.0031.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ATENA LINE NEW OUTDOOR LED 30000 SH ASY E IP65 04 840 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0032.04;588 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";177;23208;131;4000;4000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;588;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0032.04/;19.3138.0032.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ATENA LINE NEW OUTDOOR LED 30000 SH ASY E IP65 04 850;Outdoor luminaires;19.3138.0033.04;588 x 201 x 150;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";177;23208;131;5000;5000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;588;201;150;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0033.04/;19.3138.0033.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ATENA LINE NEW OUTDOOR LED 30000 SH ASY E IP65 04 850 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0034.04;588 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";177;23208;131;5000;5000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;588;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0034.04/;19.3138.0034.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ATENA LINE NEW OUTDOOR LED 36000 SH ASY E IP65 04 840;Outdoor luminaires;19.3138.0035.04;680 x 201 x 150;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";210;27446;131;4000;4000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;680;201;150;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0035.04/;19.3138.0035.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ATENA LINE NEW OUTDOOR LED 36000 SH ASY E IP65 04 840 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0036.04;680 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";210;27446;131;4000;4000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;680;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0036.04/;19.3138.0036.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ATENA LINE NEW OUTDOOR LED 36000 SH ASY E IP65 04 850;Outdoor luminaires;19.3138.0037.04;680 x 201 x 150;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";210;27850;133;5000;5000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;680;201;150;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0037.04/;19.3138.0037.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ATENA LINE NEW OUTDOOR LED 36000 SH ASY E IP65 04 850 / UCHWYT OBROTOWY;Outdoor luminaires;19.3138.0038.04;680 x 201 x 190;"mounted on poles; directly mounted to ceiling construction or surface mounted on slings";210;27850;133;5000;5000;0.7364;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;asymmetric light distribution - Imax=-54°;IP65;IK08;I;0;0,95;680;201;190;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/;https://luxiona.pl/en/oferta/oprawy-zewnetrzne/atena-line-new-outdoor-led/19.3138.0038.04/;19.3138.0038.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
