;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##;LSDepth##LENGTH##MILLIMETERS;Grate##OTHER##
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH MEDIUM E IP65 04 850;Industrial luminaires;19.3181.0001.04;596 x 250 x 200;mounted in suspended ceiling/board;81;10198;126;5000;5000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0001.04/;19.3181.0001.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH MEDIUM E IP65 04 850 / KRATA;Industrial luminaires;19.3181.0009.04;596 x 250 x 200;mounted in suspended ceiling/board;81;9637;119;5000;5000;0.8027;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0009.04/;19.3181.0009.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH MEDIUM EDD IP65 04 850;Industrial luminaires;19.3181.0002.04;596 x 250 x 200;mounted in suspended ceiling/board;81;10198;126;5000;5000;0.8494;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0002.04/;19.3181.0002.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH MEDIUM EDD IP65 04 850 / KRATA;Industrial luminaires;19.3181.0010.04;596 x 250 x 200;mounted in suspended ceiling/board;81;9637;119;5000;5000;0.8027;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0010.04/;19.3181.0010.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH NARROW E IP65 04 850;Industrial luminaires;19.3181.0003.04;596 x 250 x 200;mounted in suspended ceiling/board;81;9829;121;5000;5000;0.8187;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0003.04/;19.3181.0003.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH NARROW E IP65 04 850 / KRATA;Industrial luminaires;19.3181.0011.04;596 x 250 x 200;mounted in suspended ceiling/board;81;9248;114;5000;5000;0.7703;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0011.04/;19.3181.0011.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH NARROW EDD IP65 04 850;Industrial luminaires;19.3181.0004.04;596 x 250 x 200;mounted in suspended ceiling/board;81;9829;121;5000;5000;0.8187;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0004.04/;19.3181.0004.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH NARROW EDD IP65 04 850 / KRATA;Industrial luminaires;19.3181.0012.04;596 x 250 x 200;mounted in suspended ceiling/board;81;9248;114;5000;5000;0.7703;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0012.04/;19.3181.0012.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH WIDE E IP65 04 850;Industrial luminaires;19.3181.0005.04;596 x 250 x 200;mounted in suspended ceiling/board;81;10478;129;5000;5000;0.8727;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0005.04/;19.3181.0005.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH WIDE E IP65 04 850 / KRATA;Industrial luminaires;19.3181.0013.04;596 x 250 x 200;mounted in suspended ceiling/board;81;9901;122;5000;5000;0.8247;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0013.04/;19.3181.0013.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH WIDE EDD IP65 04 850;Industrial luminaires;19.3181.0006.04;596 x 250 x 200;mounted in suspended ceiling/board;81;10478;129;5000;5000;0.8727;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0006.04/;19.3181.0006.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH WIDE EDD IP65 04 850 / KRATA;Industrial luminaires;19.3181.0014.04;596 x 250 x 200;mounted in suspended ceiling/board;81;9901;122;5000;5000;0.8247;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0014.04/;19.3181.0014.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH WIDE ODB E IP65 04 850;Industrial luminaires;19.3181.0007.04;596 x 250 x 200;mounted in suspended ceiling/board;81;9523;118;5000;5000;0.7932;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0007.04/;19.3181.0007.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;0
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH WIDE ODB E IP65 04 850 / KRATA;Industrial luminaires;19.3181.0015.04;596 x 250 x 200;mounted in suspended ceiling/board;81;8998;111;5000;5000;0.7495;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0015.04/;19.3181.0015.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;1
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH WIDE ODB EDD IP65 04 850;Industrial luminaires;19.3181.0008.04;596 x 250 x 200;mounted in suspended ceiling/board;81;9523;118;5000;5000;0.7932;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0008.04/;19.3181.0008.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;0
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH WIDE ODB EDD IP65 04 850 / KRATA;Industrial luminaires;19.3181.0016.04;596 x 250 x 200;mounted in suspended ceiling/board;81;8998;111;5000;5000;0.7495;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0016.04/;19.3181.0016.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;1
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH MEDIUM E IP65 04 850;Industrial luminaires;19.3181.0017.04;596 x 250 x 200;mounted in suspended ceiling/board;105;16061;153;5000;5000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0017.04/;19.3181.0017.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH MEDIUM E IP65 04 850 / KRATA;Industrial luminaires;19.3181.0025.04;596 x 250 x 200;mounted in suspended ceiling/board;105;15178;145;5000;5000;0.8027;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0025.04/;19.3181.0025.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH MEDIUM EDD IP65 04 850;Industrial luminaires;19.3181.0018.04;596 x 250 x 200;mounted in suspended ceiling/board;105;16061;153;5000;5000;0.8494;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0018.04/;19.3181.0018.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH MEDIUM EDD IP65 04 850 / KRATA;Industrial luminaires;19.3181.0026.04;596 x 250 x 200;mounted in suspended ceiling/board;105;15178;145;5000;5000;0.8027;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0026.04/;19.3181.0026.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH NARROW E IP65 04 850;Industrial luminaires;19.3181.0019.04;596 x 250 x 200;mounted in suspended ceiling/board;105;15481;147;5000;5000;0.8187;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0019.04/;19.3181.0019.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH NARROW E IP65 04 850 / KRATA;Industrial luminaires;19.3181.0027.04;596 x 250 x 200;mounted in suspended ceiling/board;105;14566;139;5000;5000;0.7703;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0027.04/;19.3181.0027.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH NARROW EDD IP65 04 850;Industrial luminaires;19.3181.0020.04;596 x 250 x 200;mounted in suspended ceiling/board;105;15481;147;5000;5000;0.8187;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0020.04/;19.3181.0020.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH NARROW EDD IP65 04 850 / KRATA;Industrial luminaires;19.3181.0028.04;596 x 250 x 200;mounted in suspended ceiling/board;105;14566;139;5000;5000;0.7703;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0028.04/;19.3181.0028.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH WIDE E IP65 04 850;Industrial luminaires;19.3181.0021.04;596 x 250 x 200;mounted in suspended ceiling/board;105;16502;157;5000;5000;0.8727;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0021.04/;19.3181.0021.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH WIDE E IP65 04 850 / KRATA;Industrial luminaires;19.3181.0029.04;596 x 250 x 200;mounted in suspended ceiling/board;105;15594;149;5000;5000;0.8247;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0029.04/;19.3181.0029.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH WIDE EDD IP65 04 850;Industrial luminaires;19.3181.0022.04;596 x 250 x 200;mounted in suspended ceiling/board;105;16502;157;5000;5000;0.8727;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0022.04/;19.3181.0022.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH WIDE EDD IP65 04 850 / KRATA;Industrial luminaires;19.3181.0030.04;596 x 250 x 200;mounted in suspended ceiling/board;105;15594;149;5000;5000;0.8247;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0030.04/;19.3181.0030.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH WIDE ODB E IP65 04 850;Industrial luminaires;19.3181.0023.04;596 x 250 x 200;mounted in suspended ceiling/board;105;14999;143;5000;5000;0.7932;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0023.04/;19.3181.0023.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;0
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH WIDE ODB E IP65 04 850 / KRATA;Industrial luminaires;19.3181.0031.04;596 x 250 x 200;mounted in suspended ceiling/board;105;14172;135;5000;5000;0.7495;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0031.04/;19.3181.0031.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;1
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH WIDE ODB EDD IP65 04 850;Industrial luminaires;19.3181.0024.04;596 x 250 x 200;mounted in suspended ceiling/board;105;14999;143;5000;5000;0.7932;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0024.04/;19.3181.0024.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;0
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH WIDE ODB EDD IP65 04 850 / KRATA;Industrial luminaires;19.3181.0032.04;596 x 250 x 200;mounted in suspended ceiling/board;105;14172;135;5000;5000;0.7495;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;596;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0032.04/;19.3181.0032.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;1
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH MEDIUM E IP65 04 850;Industrial luminaires;19.3181.0033.04;616 x 250 x 200;mounted in suspended ceiling/board;138;21416;155;5000;5000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;616;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0033.04/;19.3181.0033.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH MEDIUM E IP65 04 850 / KRATA;Industrial luminaires;19.3181.0041.04;616 x 250 x 200;mounted in suspended ceiling/board;138;20238;147;5000;5000;0.8027;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;616;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0041.04/;19.3181.0041.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH MEDIUM EDD IP65 04 850;Industrial luminaires;19.3181.0034.04;616 x 250 x 200;mounted in suspended ceiling/board;138;21416;155;5000;5000;0.8494;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;616;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0034.04/;19.3181.0034.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH MEDIUM EDD IP65 04 850 / KRATA;Industrial luminaires;19.3181.0042.04;616 x 250 x 200;mounted in suspended ceiling/board;138;20238;147;5000;5000;0.8027;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;616;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0042.04/;19.3181.0042.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH NARROW E IP65 04 850;Industrial luminaires;19.3181.0035.04;616 x 250 x 200;mounted in suspended ceiling/board;138;20642;150;5000;5000;0.8187;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;616;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0035.04/;19.3181.0035.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH NARROW E IP65 04 850 / KRATA;Industrial luminaires;19.3181.0043.04;616 x 250 x 200;mounted in suspended ceiling/board;138;19422;141;5000;5000;0.7703;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;616;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0043.04/;19.3181.0043.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH NARROW EDD IP65 04 850;Industrial luminaires;19.3181.0036.04;616 x 250 x 200;mounted in suspended ceiling/board;138;20642;150;5000;5000;0.8187;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;616;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0036.04/;19.3181.0036.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH NARROW EDD IP65 04 850 / KRATA;Industrial luminaires;19.3181.0044.04;616 x 250 x 200;mounted in suspended ceiling/board;138;19422;141;5000;5000;0.7703;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;616;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0044.04/;19.3181.0044.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH WIDE E IP65 04 850;Industrial luminaires;19.3181.0037.04;616 x 250 x 200;mounted in suspended ceiling/board;138;22003;159;5000;5000;0.8727;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;616;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0037.04/;19.3181.0037.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH WIDE E IP65 04 850 / KRATA;Industrial luminaires;19.3181.0045.04;616 x 250 x 200;mounted in suspended ceiling/board;138;20793;151;5000;5000;0.8247;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;616;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0045.04/;19.3181.0045.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH WIDE EDD IP65 04 850;Industrial luminaires;19.3181.0038.04;616 x 250 x 200;mounted in suspended ceiling/board;138;22003;159;5000;5000;0.8727;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;616;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0038.04/;19.3181.0038.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH WIDE EDD IP65 04 850 / KRATA;Industrial luminaires;19.3181.0046.04;616 x 250 x 200;mounted in suspended ceiling/board;138;20793;151;5000;5000;0.8247;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;616;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0046.04/;19.3181.0046.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH WIDE ODB E IP65 04 850;Industrial luminaires;19.3181.0039.04;616 x 250 x 200;mounted in suspended ceiling/board;138;19999;145;5000;5000;0.7932;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;616;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0039.04/;19.3181.0039.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;0
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH WIDE ODB E IP65 04 850 / KRATA;Industrial luminaires;19.3181.0047.04;616 x 250 x 200;mounted in suspended ceiling/board;138;18897;137;5000;5000;0.7495;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;616;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0047.04/;19.3181.0047.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;1
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH WIDE ODB EDD IP65 04 850;Industrial luminaires;19.3181.0040.04;616 x 250 x 200;mounted in suspended ceiling/board;138;19999;145;5000;5000;0.7932;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;616;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0040.04/;19.3181.0040.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;0
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH WIDE ODB EDD IP65 04 850 / KRATA;Industrial luminaires;19.3181.0048.04;616 x 250 x 200;mounted in suspended ceiling/board;138;18897;137;5000;5000;0.7495;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;616;250;200;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/;https://luxiona.pl/en/oferta/oprawy-przemyslowe/atena-line-new-outdoor-recessed-led/19.3181.0048.04/;19.3181.0048.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;1
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH MEDIUM E IP65 04 850_outdoor;Outdoor luminaires;19.3181.0001.04 ;596 x 250 x 200;mounted in suspended ceiling/board;81;10198;126;5000;5000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0001.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH MEDIUM E IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0009.04 ;596 x 250 x 200;mounted in suspended ceiling/board;81;9637;119;5000;5000;0.8027;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0009.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH MEDIUM EDD IP65 04 850_outdoor;Outdoor luminaires;19.3181.0002.04 ;596 x 250 x 200;mounted in suspended ceiling/board;81;10198;126;5000;5000;0.8494;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0002.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH MEDIUM EDD IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0010.04 ;596 x 250 x 200;mounted in suspended ceiling/board;81;9637;119;5000;5000;0.8027;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0010.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH NARROW E IP65 04 850_outdoor;Outdoor luminaires;19.3181.0003.04 ;596 x 250 x 200;mounted in suspended ceiling/board;81;9829;121;5000;5000;0.8187;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0003.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH NARROW E IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0011.04 ;596 x 250 x 200;mounted in suspended ceiling/board;81;9248;114;5000;5000;0.7703;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0011.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH NARROW EDD IP65 04 850_outdoor;Outdoor luminaires;19.3181.0004.04 ;596 x 250 x 200;mounted in suspended ceiling/board;81;9829;121;5000;5000;0.8187;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0004.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH NARROW EDD IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0012.04 ;596 x 250 x 200;mounted in suspended ceiling/board;81;9248;114;5000;5000;0.7703;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0012.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH WIDE E IP65 04 850_outdoor;Outdoor luminaires;19.3181.0005.04 ;596 x 250 x 200;mounted in suspended ceiling/board;81;10478;129;5000;5000;0.8727;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0005.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH WIDE E IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0013.04 ;596 x 250 x 200;mounted in suspended ceiling/board;81;9901;122;5000;5000;0.8247;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0013.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH WIDE EDD IP65 04 850_outdoor;Outdoor luminaires;19.3181.0006.04 ;596 x 250 x 200;mounted in suspended ceiling/board;81;10478;129;5000;5000;0.8727;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0006.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH WIDE EDD IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0014.04 ;596 x 250 x 200;mounted in suspended ceiling/board;81;9901;122;5000;5000;0.8247;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0014.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH WIDE ODB E IP65 04 850_outdoor;Outdoor luminaires;19.3181.0007.04 ;596 x 250 x 200;mounted in suspended ceiling/board;81;9523;118;5000;5000;0.7932;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0007.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;0
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH WIDE ODB E IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0015.04 ;596 x 250 x 200;mounted in suspended ceiling/board;81;8998;111;5000;5000;0.7495;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0015.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;1
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH WIDE ODB EDD IP65 04 850_outdoor;Outdoor luminaires;19.3181.0008.04 ;596 x 250 x 200;mounted in suspended ceiling/board;81;9523;118;5000;5000;0.7932;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0008.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;0
ATENA LINE NEW OUTDOOR RECESSED LED 12000 SH WIDE ODB EDD IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0016.04 ;596 x 250 x 200;mounted in suspended ceiling/board;81;8998;111;5000;5000;0.7495;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0016.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;1
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH MEDIUM E IP65 04 850_outdoor;Outdoor luminaires;19.3181.0017.04 ;596 x 250 x 200;mounted in suspended ceiling/board;105;16061;153;5000;5000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0017.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH MEDIUM E IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0025.04 ;596 x 250 x 200;mounted in suspended ceiling/board;105;15178;145;5000;5000;0.8027;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0025.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH MEDIUM EDD IP65 04 850_outdoor;Outdoor luminaires;19.3181.0018.04 ;596 x 250 x 200;mounted in suspended ceiling/board;105;16061;153;5000;5000;0.8494;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0018.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH MEDIUM EDD IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0026.04 ;596 x 250 x 200;mounted in suspended ceiling/board;105;15178;145;5000;5000;0.8027;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0026.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH NARROW E IP65 04 850_outdoor;Outdoor luminaires;19.3181.0019.04 ;596 x 250 x 200;mounted in suspended ceiling/board;105;15481;147;5000;5000;0.8187;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0019.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH NARROW E IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0027.04 ;596 x 250 x 200;mounted in suspended ceiling/board;105;14566;139;5000;5000;0.7703;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0027.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH NARROW EDD IP65 04 850_outdoor;Outdoor luminaires;19.3181.0020.04 ;596 x 250 x 200;mounted in suspended ceiling/board;105;15481;147;5000;5000;0.8187;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0020.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH NARROW EDD IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0028.04 ;596 x 250 x 200;mounted in suspended ceiling/board;105;14566;139;5000;5000;0.7703;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0028.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH WIDE E IP65 04 850_outdoor;Outdoor luminaires;19.3181.0021.04 ;596 x 250 x 200;mounted in suspended ceiling/board;105;16502;157;5000;5000;0.8727;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0021.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH WIDE E IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0029.04 ;596 x 250 x 200;mounted in suspended ceiling/board;105;15594;149;5000;5000;0.8247;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0029.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH WIDE EDD IP65 04 850_outdoor;Outdoor luminaires;19.3181.0022.04 ;596 x 250 x 200;mounted in suspended ceiling/board;105;16502;157;5000;5000;0.8727;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0022.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH WIDE EDD IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0030.04 ;596 x 250 x 200;mounted in suspended ceiling/board;105;15594;149;5000;5000;0.8247;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0030.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH WIDE ODB E IP65 04 850_outdoor;Outdoor luminaires;19.3181.0023.04 ;596 x 250 x 200;mounted in suspended ceiling/board;105;14999;143;5000;5000;0.7932;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0023.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;0
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH WIDE ODB E IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0031.04 ;596 x 250 x 200;mounted in suspended ceiling/board;105;14172;135;5000;5000;0.7495;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0031.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;1
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH WIDE ODB EDD IP65 04 850_outdoor;Outdoor luminaires;19.3181.0024.04 ;596 x 250 x 200;mounted in suspended ceiling/board;105;14999;143;5000;5000;0.7932;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0024.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;0
ATENA LINE NEW OUTDOOR RECESSED LED 18000 SH WIDE ODB EDD IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0032.04 ;596 x 250 x 200;mounted in suspended ceiling/board;105;14172;135;5000;5000;0.7495;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;596;250;200;#N/D;#N/D;19.3181.0032.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;1
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH MEDIUM E IP65 04 850_outdoor;Outdoor luminaires;19.3181.0033.04 ;616 x 250 x 200;mounted in suspended ceiling/board;138;21416;155;5000;5000;0.8494;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;616;250;200;#N/D;#N/D;19.3181.0033.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH MEDIUM E IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0041.04 ;616 x 250 x 200;mounted in suspended ceiling/board;138;20238;147;5000;5000;0.8027;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;616;250;200;#N/D;#N/D;19.3181.0041.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH MEDIUM EDD IP65 04 850_outdoor;Outdoor luminaires;19.3181.0034.04 ;616 x 250 x 200;mounted in suspended ceiling/board;138;21416;155;5000;5000;0.8494;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;616;250;200;#N/D;#N/D;19.3181.0034.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH MEDIUM EDD IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0042.04 ;616 x 250 x 200;mounted in suspended ceiling/board;138;20238;147;5000;5000;0.8027;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 57,6° / 56,2°;IP65;IK08;I;0;0,95;616;250;200;#N/D;#N/D;19.3181.0042.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH NARROW E IP65 04 850_outdoor;Outdoor luminaires;19.3181.0035.04 ;616 x 250 x 200;mounted in suspended ceiling/board;138;20642;150;5000;5000;0.8187;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;616;250;200;#N/D;#N/D;19.3181.0035.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH NARROW E IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0043.04 ;616 x 250 x 200;mounted in suspended ceiling/board;138;19422;141;5000;5000;0.7703;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;616;250;200;#N/D;#N/D;19.3181.0043.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH NARROW EDD IP65 04 850_outdoor;Outdoor luminaires;19.3181.0036.04 ;616 x 250 x 200;mounted in suspended ceiling/board;138;20642;150;5000;5000;0.8187;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;616;250;200;#N/D;#N/D;19.3181.0036.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH NARROW EDD IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0044.04 ;616 x 250 x 200;mounted in suspended ceiling/board;138;19422;141;5000;5000;0.7703;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 21,8° / 22°;IP65;IK08;I;0;0,95;616;250;200;#N/D;#N/D;19.3181.0044.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH WIDE E IP65 04 850_outdoor;Outdoor luminaires;19.3181.0037.04 ;616 x 250 x 200;mounted in suspended ceiling/board;138;22003;159;5000;5000;0.8727;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;616;250;200;#N/D;#N/D;19.3181.0037.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH WIDE E IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0045.04 ;616 x 250 x 200;mounted in suspended ceiling/board;138;20793;151;5000;5000;0.8247;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;616;250;200;#N/D;#N/D;19.3181.0045.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH WIDE EDD IP65 04 850_outdoor;Outdoor luminaires;19.3181.0038.04 ;616 x 250 x 200;mounted in suspended ceiling/board;138;22003;159;5000;5000;0.8727;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;616;250;200;#N/D;#N/D;19.3181.0038.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH WIDE EDD IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0046.04 ;616 x 250 x 200;mounted in suspended ceiling/board;138;20793;151;5000;5000;0.8247;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 93,8° / 89,6°;IP65;IK08;I;0;0,95;616;250;200;#N/D;#N/D;19.3181.0046.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH WIDE ODB E IP65 04 850_outdoor;Outdoor luminaires;19.3181.0039.04 ;616 x 250 x 200;mounted in suspended ceiling/board;138;19999;145;5000;5000;0.7932;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;616;250;200;#N/D;#N/D;19.3181.0039.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;0
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH WIDE ODB E IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0047.04 ;616 x 250 x 200;mounted in suspended ceiling/board;138;18897;137;5000;5000;0.7495;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;616;250;200;#N/D;#N/D;19.3181.0047.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;1
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH WIDE ODB EDD IP65 04 850_outdoor;Outdoor luminaires;19.3181.0040.04 ;616 x 250 x 200;mounted in suspended ceiling/board;138;19999;145;5000;5000;0.7932;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;616;250;200;#N/D;#N/D;19.3181.0040.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;0
ATENA LINE NEW OUTDOOR RECESSED LED 24000 SH WIDE ODB EDD IP65 04 850 / KRATA_outdoor;Outdoor luminaires;19.3181.0048.04 ;616 x 250 x 200;mounted in suspended ceiling/board;138;18897;137;5000;5000;0.7495;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_SH (transparent hardened glass);LED;-25 ÷ 40;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 103,2° / 104,4°;IP65;IK08;I;0;0,95;616;250;200;#N/D;#N/D;19.3181.0048.04 .IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;45;1
