;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
BERYL LED NK 1500 PLX 34 830;Surface mounted luminaires;19.3072.0001.34;200 x 200 x 110;surface mounted on ceiling;10;1175;117;3000;3000;0.7831;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 79,4° / 79,2°;IP20;IK06;I;0;0.95;200;200;110;https://luxiona.pl/oferta/oprawy-nastropowe/beryl-led-nk/;https://luxiona.pl/oferta/oprawy-nastropowe/beryl-led-nk/19.3072.0001.34/;19.3072.0001.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL LED NK 1500 PLX 34 840;Surface mounted luminaires;19.3072.0002.34;200 x 200 x 110;surface mounted on ceiling;10;1175;117;4000;4000;0.7831;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 79,4° / 79,2°;IP20;IK06;I;0;0.95;200;200;110;https://luxiona.pl/oferta/oprawy-nastropowe/beryl-led-nk/;https://luxiona.pl/oferta/oprawy-nastropowe/beryl-led-nk/19.3072.0002.34/;19.3072.0002.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL LED NK 2200 PLX E 34 830;Surface mounted luminaires;19.3072.0003.34;200 x 200 x 110;surface mounted on ceiling;16;1717;107;3000;3000;0.7831;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 79,4° / 79,2°;IP20;IK06;I;0;0.95;200;200;110;https://luxiona.pl/oferta/oprawy-nastropowe/beryl-led-nk/;https://luxiona.pl/oferta/oprawy-nastropowe/beryl-led-nk/19.3072.0003.34/;19.3072.0003.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL LED NK 2200 PLX E 34 840;Surface mounted luminaires;19.3072.0004.34;200 x 200 x 110;surface mounted on ceiling;16;1828;114;4000;4000;0.7831;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 79,4° / 79,2°;IP20;IK06;I;0;0.95;200;200;110;https://luxiona.pl/oferta/oprawy-nastropowe/beryl-led-nk/;https://luxiona.pl/oferta/oprawy-nastropowe/beryl-led-nk/19.3072.0004.34/;19.3072.0004.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL LED NK 3000 PLX 34 830;Surface mounted luminaires;19.3072.0005.34;200 x 200 x 110;surface mounted on ceiling;21;2186;104;3000;3000;0.7831;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 79,4° / 79,2°;IP20;IK06;I;0;0.95;200;200;110;https://luxiona.pl/oferta/oprawy-nastropowe/beryl-led-nk/;https://luxiona.pl/oferta/oprawy-nastropowe/beryl-led-nk/19.3072.0005.34/;19.3072.0005.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL LED NK 3000 PLX 34 840;Surface mounted luminaires;19.3072.0006.34;200 x 200 x 110;surface mounted on ceiling;21;2326;111;4000;4000;0.7831;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 79,4° / 79,2°;IP20;IK06;I;0;0.95;200;200;110;https://luxiona.pl/oferta/oprawy-nastropowe/beryl-led-nk/;https://luxiona.pl/oferta/oprawy-nastropowe/beryl-led-nk/19.3072.0006.34/;19.3072.0006.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
