;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
BERYL NEW LED O-1 1000 E 33 IP20/44 830;Recessed luminaires;19.3051.1102.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;9.8;1001;102;3000;3000;0.7749;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent PMMA;LED;5 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 41° / 40,4°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.1102.33/;19.3051.1102.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1000 E 33 IP20/44 840;Recessed luminaires;19.3051.1101.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;9.8;1029;105;4000;4000;0.7749;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent PMMA;LED;5 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 41° / 40,4°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.1101.33/;19.3051.1101.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1000 EDD 33 IP20/44 830;Recessed luminaires;19.3051.1104.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;9.8;1001;102;3000;3000;0.7749;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent PMMA;LED;5 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 41° / 40,4°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.1104.33/;19.3051.1104.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1000 EDD 33 IP20/44 840;Recessed luminaires;19.3051.1103.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;9.8;1029;105;4000;4000;0.7749;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent PMMA;LED;5 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 41° / 40,4°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.1103.33/;19.3051.1103.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1000 MICRO-PRM E 33 IP20/44 830;Recessed luminaires;19.3051.1302.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;9.8;954;97;3000;3000;0.7384;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 89,2° / 87,4°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.1302.33/;19.3051.1302.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1000 MICRO-PRM E 33 IP20/44 840;Recessed luminaires;19.3051.1301.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;9.8;981;100;4000;4000;0.7384;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 89,2° / 87,4°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.1301.33/;19.3051.1301.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1000 MICRO-PRM EDD 33 IP20/44 830;Recessed luminaires;19.3051.1304.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;9.8;954;97;3000;3000;0.7384;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 89,2° / 87,4°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.1304.33/;19.3051.1304.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1000 MICRO-PRM EDD 33 IP20/44 840;Recessed luminaires;19.3051.1303.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;9.8;981;100;4000;4000;0.7384;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 89,2° / 87,4°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.1303.33/;19.3051.1303.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1000 PLX E 33 IP20/44 830;Recessed luminaires;19.3051.1202.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;9.8;852;87;3000;3000;0.6592;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 81,6° / 81,6°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.1202.33/;19.3051.1202.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1000 PLX E 33 IP20/44 840;Recessed luminaires;19.3051.1201.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;9.8;875;89;4000;4000;0.6592;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 81,6° / 81,6°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.1201.33/;19.3051.1201.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1000 PLX EDD 33 IP20/44 830;Recessed luminaires;19.3051.1204.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;9.8;852;87;3000;3000;0.6592;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 81,6° / 81,6°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.1204.33/;19.3051.1204.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1000 PLX EDD 33 IP20/44 840;Recessed luminaires;19.3051.1203.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;9.8;875;89;4000;4000;0.6592;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 81,6° / 81,6°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.1203.33/;19.3051.1203.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1800 E 33 IP20/44 830;Recessed luminaires;19.3051.2102.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;12.8;1550;121;3000;3000;0.7749;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent PMMA;LED;5 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 41° / 40,4°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.2102.33/;19.3051.2102.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1800 E 33 IP20/44 840;Recessed luminaires;19.3051.2101.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;12.8;1595;125;4000;4000;0.7749;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent PMMA;LED;5 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 41° / 40,4°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.2101.33/;19.3051.2101.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1800 EDD 33 IP20/44 830;Recessed luminaires;19.3051.2104.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;12.8;1550;121;3000;3000;0.7749;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent PMMA;LED;5 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 41° / 40,4°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.2104.33/;19.3051.2104.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1800 EDD 33 IP20/44 840;Recessed luminaires;19.3051.2103.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;12.8;1595;125;4000;4000;0.7749;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent PMMA;LED;5 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 41° / 40,4°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.2103.33/;19.3051.2103.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1800 MICRO-PRM E 33 IP20/44 830;Recessed luminaires;19.3051.2302.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;12.8;1477;115;3000;3000;0.7384;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 89,2° / 87,4°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.2302.33/;19.3051.2302.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1800 MICRO-PRM E 33 IP20/44 840;Recessed luminaires;19.3051.2301.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;12.8;1520;119;4000;4000;0.7384;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 89,2° / 87,4°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.2301.33/;19.3051.2301.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1800 MICRO-PRM EDD 33 IP20/44 830;Recessed luminaires;19.3051.2304.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;12.8;1477;115;3000;3000;0.7384;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 89,2° / 87,4°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.2304.33/;19.3051.2304.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1800 MICRO-PRM EDD 33 IP20/44 840;Recessed luminaires;19.3051.2303.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;12.8;1520;119;4000;4000;0.7384;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 89,2° / 87,4°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.2303.33/;19.3051.2303.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1800 PLX E 33 IP20/44 830;Recessed luminaires;19.3051.2202.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;12.8;1318;103;3000;3000;0.6592;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 81,6° / 81,6°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.2202.33/;19.3051.2202.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1800 PLX E 33 IP20/44 840;Recessed luminaires;19.3051.2201.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;12.8;1357;106;4000;4000;0.6592;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 81,6° / 81,6°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.2201.33/;19.3051.2201.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1800 PLX EDD 33 IP20/44 830;Recessed luminaires;19.3051.2204.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;12.8;1318;103;3000;3000;0.6592;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 81,6° / 81,6°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.2204.33/;19.3051.2204.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-1 1800 PLX EDD 33 IP20/44 840;Recessed luminaires;19.3051.2203.33;?100 x 75;mounted in module ceilings, as well as plasterboard ceilings;12.8;1357;106;4000;4000;0.6592;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 81,6° / 81,6°;IP20/44;IK04;II;RG0;0,95;0;0;75;100;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.2203.33/;19.3051.2203.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
