;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
BERYL NEW LED O-2 2800 E 33 IP20/44 830;Recessed luminaires;19.3051.3102.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;18.4;2156;117;3000;3000;0.7141;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent glass;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 72° / 73°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.3102.33/;19.3051.3102.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 2800 E 33 IP20/44 840;Recessed luminaires;19.3051.3101.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;18.4;2219;121;4000;4000;0.7141;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent glass;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 72° / 73°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.3101.33/;19.3051.3101.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 2800 MICRO-PRM E 33 IP20/44 830;Recessed luminaires;19.3051.3302.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;18.4;2009;109;3000;3000;0.6655;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 113,2° / 110,8°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.3302.33/;19.3051.3302.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 2800 MICRO-PRM E 33 IP20/44 840;Recessed luminaires;19.3051.3301.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;18.4;2068;112;4000;4000;0.6655;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 113,2° / 110,8°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.3301.33/;19.3051.3301.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 2800 MICRO-PRM EDD 33 IP20/44 830;Recessed luminaires;19.3051.3304.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;18.4;2009;109;3000;3000;0.6655;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 113,2° / 110,8°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.3304.33/;19.3051.3304.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 2800 MICRO-PRM EDD 33 IP20/44 840;Recessed luminaires;19.3051.3303.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;18.4;2068;112;4000;4000;0.6655;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 113,2° / 110,8°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.3303.33/;19.3051.3303.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 2800 PLX E 33 IP20/44 830;Recessed luminaires;19.3051.3202.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;18.4;1948;106;3000;3000;0.6453;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 93,4° / 93,4°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.3202.33/;19.3051.3202.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 2800 PLX E 33 IP20/44 840;Recessed luminaires;19.3051.3201.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;18.4;2006;109;4000;4000;0.6453;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 93,4° / 93,4°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.3201.33/;19.3051.3201.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 2800 PLX EDD 33 IP20/44 830;Recessed luminaires;19.3051.3204.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;18.4;1948;106;3000;3000;0.6453;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 93,4° / 93,4°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.3204.33/;19.3051.3204.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 2800 PLX EDD 33 IP20/44 840;Recessed luminaires;19.3051.3203.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;18.4;2006;109;4000;4000;0.6453;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 93,4° / 93,4°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.3203.33/;19.3051.3203.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 3600 E 33 IP20/44 830;Recessed luminaires;19.3051.4102.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;25.5;2984;117;3000;3000;0.7141;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 72° / 73°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.4102.33/;19.3051.4102.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 3600 E 33 IP20/44 840;Recessed luminaires;19.3051.4101.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;25.5;3074;121;4000;4000;0.7141;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 72° / 73°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.4101.33/;19.3051.4101.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 3600 EDD 33 IP20/44 830;Recessed luminaires;19.3051.4104.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;25.5;2984;117;3000;3000;0.7141;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 72° / 73°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.4104.33/;19.3051.4104.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 3600 EDD 33 IP20/44 840;Recessed luminaires;19.3051.4103.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;25.5;3074;121;4000;4000;0.7141;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 72° / 73°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.4103.33/;19.3051.4103.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 3600 MICRO-PRM E 33 IP20/44 830;Recessed luminaires;19.3051.4302.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;25.5;2781;109;3000;3000;0.6655;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 113,2° / 110,8°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.4302.33/;19.3051.4302.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 3600 MICRO-PRM E 33 IP20/44 840;Recessed luminaires;19.3051.4301.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;25.5;2865;112;4000;4000;0.6655;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 113,2° / 110,8°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.4301.33/;19.3051.4301.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 3600 MICRO-PRM EDD 33 IP20/44 830;Recessed luminaires;19.3051.4304.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;25.5;2781;109;3000;3000;0.6655;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 113,2° / 110,8°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.4304.33/;19.3051.4304.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 3600 MICRO-PRM EDD 33 IP20/44 840;Recessed luminaires;19.3051.4303.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;25.5;2865;112;4000;4000;0.6655;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 113,2° / 110,8°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.4303.33/;19.3051.4303.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 3600 PLX E 33 IP20/44 830;Recessed luminaires;19.3051.4202.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;25.5;2697;106;3000;3000;0.6453;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 93,4° / 93,4°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.4202.33/;19.3051.4202.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 3600 PLX E 33 IP20/44 840;Recessed luminaires;19.3051.4201.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;25.5;2778;109;4000;4000;0.6453;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 93,4° / 93,4°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.4201.33/;19.3051.4201.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 3600 PLX EDD 33 IP20/44 840;Recessed luminaires;19.3051.4203.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;25.5;2778;109;4000;4000;0.6453;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 93,4° / 93,4°;IP20/44;IK04;II;RG0;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.4203.33/;19.3051.4203.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2/M21 3600 E 34 IP20/44 840;Recessed luminaires;19.3051.8101.34;?190 x 101;mounted in module ceilings, as well as plasterboard ceilings;25.5;3074;121;4000;4000;0.7141;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 72° / 73°;IP20/44;IK04;II;RG0;0,95;0;0;101;190;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.8101.34/;19.3051.8101.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2/M21 3600 MICRO-PRM E 34 IP20/44 840;Recessed luminaires;19.3051.8301.34;?190 x 101;mounted in module ceilings, as well as plasterboard ceilings;25.5;2865;112;4000;4000;0.6655;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 113,2° / 110,8°;IP20/44;IK04;II;RG0;0,95;0;0;101;190;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.8301.34/;19.3051.8301.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2/M21 3600 PLX E 34 IP20/44 840;Recessed luminaires;19.3051.8201.34;?190 x 101;mounted in module ceilings, as well as plasterboard ceilings;25.5;2778;109;4000;4000;0.6453;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 93,4° / 93,4°;IP20/44;IK04;II;RG0;0,95;0;0;101;190;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.8201.34/;19.3051.8201.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 1800 EDD 33 IP20/44 / TUNABLE WHITE;Recessed luminaires;19.3051.0101.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;16.0;1425;89;4000;2450 ÷ 7000;0.7141;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent glass;LED;5 ÷ 30;95000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);>85;0;(C0-C180) / (C90-C270) - 72° / 73°;IP20/44;IK04;II;-;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.0101.33/;19.3051.0101.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 1800 MICRO-PRM EDD 33 IP20/44 / TUNABLE WHITE;Recessed luminaires;19.3051.0301.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;16.0;1328;83;4000;2450 ÷ 7000;0.6655;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;95000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);>85;0;(C0-C180) / (C90-C270) - 113,2° / 110,8°;IP20/44;IK04;II;-;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.0301.33/;19.3051.0301.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-2 1800 PLX EDD 33 IP20/44 / TUNABLE WHITE;Recessed luminaires;19.3051.0201.33;?165 x 100;mounted in module ceilings, as well as plasterboard ceilings;16.0;1287;80;4000;2450 ÷ 7000;0.6453;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;95000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);>85;0;(C0-C180) / (C90-C270) - 93,4° / 93,4°;IP20/44;IK04;II;-;0,95;0;0;100;165;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.0201.33/;19.3051.0201.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 2800 E 33 IP20/44 830;Recessed luminaires;19.3051.5102.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;18.4;2316;126;3000;3000;0.7672;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent glass;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.5102.33/;19.3051.5102.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 2800 E 33 IP20/44 840;Recessed luminaires;19.3051.5101.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;18.4;2384;130;4000;4000;0.7672;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent glass;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.5101.33/;19.3051.5101.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 2800 EDD 33 IP20/44 830;Recessed luminaires;19.3051.5104.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;18.4;2316;126;3000;3000;0.7672;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent glass;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.5104.33/;19.3051.5104.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 2800 EDD 33 IP20/44 840;Recessed luminaires;19.3051.5103.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;18.4;2384;130;4000;4000;0.7672;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent glass;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.5103.33/;19.3051.5103.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 2800 MICRO-PRM E 33 IP20/44 830;Recessed luminaires;19.3051.5302.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;18.4;2139;116;3000;3000;0.7085;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 103° / 101,6°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.5302.33/;19.3051.5302.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 2800 MICRO-PRM E 33 IP20/44 840;Recessed luminaires;19.3051.5301.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;18.4;2202;120;4000;4000;0.7085;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 103° / 101,6°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.5301.33/;19.3051.5301.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 2800 MICRO-PRM EDD 33 IP20/44 830;Recessed luminaires;19.3051.5304.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;18.4;2139;116;3000;3000;0.7085;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 103° / 101,6°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.5304.33/;19.3051.5304.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 2800 MICRO-PRM EDD 33 IP20/44 840;Recessed luminaires;19.3051.5303.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;18.4;2202;120;4000;4000;0.7085;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 103° / 101,6°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.5303.33/;19.3051.5303.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 2800 PLX E 33 IP20/44 830;Recessed luminaires;19.3051.5202.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;18.4;1983;108;3000;3000;0.6568;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 94,6° / 94,4°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.5202.33/;19.3051.5202.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 2800 PLX E 33 IP20/44 840;Recessed luminaires;19.3051.5201.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;18.4;2041;111;4000;4000;0.6568;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 94,6° / 94,4°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.5201.33/;19.3051.5201.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 2800 PLX EDD 33 IP20/44 830;Recessed luminaires;19.3051.5204.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;18.4;1983;108;3000;3000;0.6568;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 94,6° / 94,4°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.5204.33/;19.3051.5204.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 2800 PLX EDD 33 IP20/44 840;Recessed luminaires;19.3051.5203.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;18.4;2041;111;4000;4000;0.6568;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;91000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 94,6° / 94,4°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.5203.33/;19.3051.5203.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 3600 E 33 IP20/44 830;Recessed luminaires;19.3051.6102.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;25.5;3206;126;3000;3000;0.7672;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.6102.33/;19.3051.6102.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 3600 E 33 IP20/44 840;Recessed luminaires;19.3051.6101.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;25.5;3303;130;4000;4000;0.7672;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.6101.33/;19.3051.6101.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 3600 EDD 33 IP20/44 830;Recessed luminaires;19.3051.6104.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;25.5;3206;126;3000;3000;0.7672;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.6104.33/;19.3051.6104.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 3600 EDD 33 IP20/44 840;Recessed luminaires;19.3051.6103.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;25.5;3303;130;4000;4000;0.7672;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent glass;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.6103.33/;19.3051.6103.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 3600 MICRO-PRM E 33 IP20/44 830;Recessed luminaires;19.3051.6302.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;25.5;2961;116;3000;3000;0.7085;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 103° / 101,6°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.6302.33/;19.3051.6302.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 3600 MICRO-PRM E 33 IP20/44 840;Recessed luminaires;19.3051.6301.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;25.5;3050;120;4000;4000;0.7085;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 103° / 101,6°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.6301.33/;19.3051.6301.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 3600 MICRO-PRM EDD 33 IP20/44 830;Recessed luminaires;19.3051.6304.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;25.5;2961;116;3000;3000;0.7085;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 103° / 101,6°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.6304.33/;19.3051.6304.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 3600 MICRO-PRM EDD 33 IP20/44 840;Recessed luminaires;19.3051.6303.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;25.5;3050;120;4000;4000;0.7085;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 103° / 101,6°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.6303.33/;19.3051.6303.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 3600 PLX E 33 IP20/44 830;Recessed luminaires;19.3051.6202.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;25.5;2745;108;3000;3000;0.6568;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 94,6° / 94,4°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.6202.33/;19.3051.6202.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 3600 PLX E 33 IP20/44 840;Recessed luminaires;19.3051.6201.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;25.5;2828;111;4000;4000;0.6568;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 94,6° / 94,4°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.6201.33/;19.3051.6201.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 3600 PLX EDD 33 IP20/44 830;Recessed luminaires;19.3051.6204.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;25.5;2745;108;3000;3000;0.6568;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 94,6° / 94,4°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.6204.33/;19.3051.6204.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 3600 PLX EDD 33 IP20/44 840;Recessed luminaires;19.3051.6203.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;25.5;2828;111;4000;4000;0.6568;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);80;2;(C0-C180) / (C90-C270) - 94,6° / 94,4°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.6203.33/;19.3051.6203.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 5400 E 33 IP20/44 840;Recessed luminaires;19.3051.7101.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;39.3;4982;127;4000;4000;0.7672;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent glass;LED;5 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.7101.33/;19.3051.7101.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 5400 EDD 33 IP20/44 840;Recessed luminaires;19.3051.7103.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;39.3;4982;127;4000;4000;0.7672;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent glass;LED;5 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.7103.33/;19.3051.7103.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 5400 PLX E 33 IP20/44 840;Recessed luminaires;19.3051.7201.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;39.0;4080;105;4000;4000;0.6568;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;83000;L90/B10;85;3;(C0-C180) / (C90-C270) - 94,6° / 94,4°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.7201.33/;19.3051.7201.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3/M22 5400 E 34 IP20/44 840;Recessed luminaires;19.3051.9701.34;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;39.3;4982;127;4000;4000;0.7672;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent glass;LED;5 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20/44;IK04;II;RG0;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.9701.34/;19.3051.9701.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3/M22 5400 EDD 34 IP20/44 840;Recessed luminaires;19.3051.9703.34;?216 x 111;mounted in module ceilings, as well as plasterboard ceilings;39.3;4982;127;4000;4000;0.7672;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent glass;LED;5 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20/44;IK04;II;RG0;0,95;0;0;111;216;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.9703.34/;19.3051.9703.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3/M22 5400 MICRO-PRM E 34 IP20/44 840;Recessed luminaires;19.3051.9901.34;?216 x 111;mounted in module ceilings, as well as plasterboard ceilings;39.3;4601;117;4000;4000;0.7085;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 103° / 101,6°;IP20/44;IK04;II;RG0;0,95;0;0;111;216;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.9901.34/;19.3051.9901.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3/M22 5400 PLX E 34 IP20/44 840;Recessed luminaires;19.3051.9801.34;?216 x 111;mounted in module ceilings, as well as plasterboard ceilings;39.3;4265;109;4000;4000;0.6568;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 94,6° / 94,4°;IP20/44;IK04;II;RG0;0,95;0;0;111;216;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.9801.34/;19.3051.9801.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 3000 EDD 33 IP20/44 / TUNABLE WHITE;Recessed luminaires;19.3051.0401.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;30.0;2529;84;4000;2450 ÷ 7000;0.7672;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_transparent glass;LED;5 ÷ 30;82000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);>85;0;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20/44;IK04;II;-;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.0401.33/;19.3051.0401.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 3000 MICRO-PRM EDD 33 IP20/44 / TUNABLE WHITE;Recessed luminaires;19.3051.0601.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;30.0;2336;78;4000;2450 ÷ 7000;0.7085;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;82000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);>85;0;(C0-C180) / (C90-C270) - 103° / 101,6°;IP20/44;IK04;II;-;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.0601.33/;19.3051.0601.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL NEW LED O-3 3000 PLX EDD 33 IP20/44 / TUNABLE WHITE;Recessed luminaires;19.3051.0501.33;?195 x 110;mounted in module ceilings, as well as plasterboard ceilings;30.0;2165;72;4000;2450 ÷ 7000;0.6568;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;82000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);>85;0;(C0-C180) / (C90-C270) - 94,6° / 94,4°;IP20/44;IK04;II;-;0,95;0;0;110;195;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/;https://luxiona.pl/oferta/oprawy-do-wbudowania/beryl-new-led-o-ip20-44/19.3051.0501.33/;19.3051.0501.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA

