;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
BERYL SURFACE NEW LED O-2 2800 E 34 830;Surface mounted luminaires;19.3078.0023.34;?185 x 156;surface mounted on ceiling;18.6;2044;110;3000;3000;0.7141;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent glass;LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 72° / 73°;IP20;IK04;II;RG0;0,95;0;0;156;185;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0023.34/;19.3078.0023.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-2 2800 E 34 840;Surface mounted luminaires;19.3078.0024.34;?185 x 156;surface mounted on ceiling;18.6;2104;113;4000;4000;0.7141;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent glass;LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 72° / 73°;IP20;IK04;II;RG0;0,95;0;0;156;185;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0024.34/;19.3078.0024.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-2 2800 MICRO-PRM E 34 830;Surface mounted luminaires;19.3078.0025.34;?185 x 156;surface mounted on ceiling;18.6;1905;102;3000;3000;0.6655;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 113,2° / 110,8°;IP20;IK04;II;RG0;0,95;0;0;156;185;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0025.34/;19.3078.0025.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-2 2800 MICRO-PRM E 34 840;Surface mounted luminaires;19.3078.0026.34;?185 x 156;surface mounted on ceiling;18.6;1961;105;4000;4000;0.6655;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 113,2° / 110,8°;IP20;IK04;II;RG0;0,95;0;0;156;185;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0026.34/;19.3078.0026.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-2 2800 PLX E 34 830;Surface mounted luminaires;19.3078.0027.34;?185 x 156;surface mounted on ceiling;18.6;1847;99;3000;3000;0.6453;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 93,4° / 93,4°;IP20;IK04;II;RG0;0,95;0;0;156;185;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0027.34/;19.3078.0027.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-2 2800 PLX E 34 840;Surface mounted luminaires;19.3078.0028.34;?185 x 156;surface mounted on ceiling;18.6;1902;102;4000;4000;0.6453;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 93,4° / 93,4°;IP20;IK04;II;RG0;0,95;0;0;156;185;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0028.34/;19.3078.0028.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-2 3600 E 34 840;Surface mounted luminaires;19.3078.0029.34;?185 x 156;surface mounted on ceiling;25.3;2929;116;4000;4000;0.7141;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent glass;LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 72° / 73°;IP20;IK04;II;RG0;0,95;0;0;156;185;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0029.34/;19.3078.0029.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-2 3600 EDD 34 840;Surface mounted luminaires;19.3078.0030.34;?185 x 156;surface mounted on ceiling;25.3;2929;116;4000;4000;0.7141;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent glass;LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 72° / 73°;IP20;IK04;II;RG0;0,95;0;0;156;185;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0030.34/;19.3078.0030.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-2 3600 MICRO-PRM E 34 840;Surface mounted luminaires;19.3078.0031.34;?185 x 156;surface mounted on ceiling;25.3;2730;108;4000;4000;0.6655;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 113,2° / 110,8°;IP20;IK04;II;RG0;0,95;0;0;156;185;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0031.34/;19.3078.0031.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-2 3600 MICRO-PRM EDD 34 840;Surface mounted luminaires;19.3078.0032.34;?185 x 156;surface mounted on ceiling;25.3;2730;108;4000;4000;0.6655;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 113,2° / 110,8°;IP20;IK04;II;RG0;0,95;0;0;156;185;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0032.34/;19.3078.0032.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-2 3600 PLX E 34 830;Surface mounted luminaires;19.3078.0033.34;?185 x 156;surface mounted on ceiling;25.3;2571;102;3000;3000;0.6453;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 93,4° / 93,4°;IP20;IK04;II;RG0;0,95;0;0;156;185;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0033.34/;19.3078.0033.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-2 3600 PLX E 34 840;Surface mounted luminaires;19.3078.0034.34;?185 x 156;surface mounted on ceiling;25.3;2647;105;4000;4000;0.6453;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 93,4° / 93,4°;IP20;IK04;II;RG0;0,95;0;0;156;185;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0034.34/;19.3078.0034.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-2 3600 PLX EDD 34 830;Surface mounted luminaires;19.3078.0035.34;?185 x 156;surface mounted on ceiling;25.3;2571;102;3000;3000;0.6453;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 93,4° / 93,4°;IP20;IK04;II;RG0;0,95;0;0;156;185;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0035.34/;19.3078.0035.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-2 3600 PLX EDD 34 840;Surface mounted luminaires;19.3078.0036.34;?185 x 156;surface mounted on ceiling;25.3;2647;105;4000;4000;0.6453;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 93,4° / 93,4°;IP20;IK04;II;RG0;0,95;0;0;156;185;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0036.34/;19.3078.0036.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-2 3600 SHM E 34 840;Surface mounted luminaires;19.3078.0037.34;?185 x 156;surface mounted on ceiling;25.3;2875;114;4000;4000;0.7008;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_SHM (hardened mat glass);LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 71,6° / 71,6°;IP20;IK04;II;RG0;0,95;0;0;156;185;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0037.34/;19.3078.0037.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 2800 E 34 830;Surface mounted luminaires;19.3078.0038.34;?215 x 166;surface mounted on ceiling;18.6;2196;118;3000;3000;0.7672;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_SHM (hardened mat glass);LED;5 ÷ 30;83000;L90/B10;80;2;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0038.34/;19.3078.0038.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 2800 E 34 840;Surface mounted luminaires;19.3078.0039.34;?215 x 166;surface mounted on ceiling;18.6;2261;122;4000;4000;0.7672;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_SHM (hardened mat glass);LED;5 ÷ 30;83000;L90/B10;80;2;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0039.34/;19.3078.0039.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 2800 EDD 34 830;Surface mounted luminaires;19.3078.0040.34;?215 x 166;surface mounted on ceiling;18.6;2196;118;3000;3000;0.7672;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_SHM (hardened mat glass);LED;5 ÷ 30;83000;L90/B10;80;2;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0040.34/;19.3078.0040.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 2800 EDD 34 840;Surface mounted luminaires;19.3078.0041.34;?215 x 166;surface mounted on ceiling;18.6;2261;122;4000;4000;0.7672;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_SHM (hardened mat glass);LED;5 ÷ 30;83000;L90/B10;80;2;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0041.34/;19.3078.0041.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 2800 MICRO-PRM E 34 830;Surface mounted luminaires;19.3078.0042.34;?215 x 166;surface mounted on ceiling;18.6;2028;109;3000;3000;0.7085;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_SHM (hardened mat glass);LED;5 ÷ 30;83000;L90/B10;80;2;(C0-C180) / (C90-C270) - 103° / 101,6°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0042.34/;19.3078.0042.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 2800 MICRO-PRM E 34 840;Surface mounted luminaires;19.3078.0043.34;?215 x 166;surface mounted on ceiling;18.6;2088;112;4000;4000;0.7085;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_SHM (hardened mat glass);LED;5 ÷ 30;83000;L90/B10;80;2;(C0-C180) / (C90-C270) - 103° / 101,6°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0043.34/;19.3078.0043.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 2800 MICRO-PRM EDD 34 830;Surface mounted luminaires;19.3078.0044.34;?215 x 166;surface mounted on ceiling;18.6;2028;109;3000;3000;0.7085;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_SHM (hardened mat glass);LED;5 ÷ 30;83000;L90/B10;80;2;(C0-C180) / (C90-C270) - 103° / 101,6°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0044.34/;19.3078.0044.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 2800 MICRO-PRM EDD 34 840;Surface mounted luminaires;19.3078.0045.34;?215 x 166;surface mounted on ceiling;18.6;2088;112;4000;4000;0.7085;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_SHM (hardened mat glass);LED;5 ÷ 30;83000;L90/B10;80;2;(C0-C180) / (C90-C270) - 103° / 101,6°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0045.34/;19.3078.0045.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 2800 PLX E 34 830;Surface mounted luminaires;19.3078.0046.34;?215 x 166;surface mounted on ceiling;18.6;1880;101;3000;3000;0.6568;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;83000;L90/B10;80;2;(C0-C180) / (C90-C270) - 94,6° / 94,4°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0046.34/;19.3078.0046.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 2800 PLX E 34 840;Surface mounted luminaires;19.3078.0047.34;?215 x 166;surface mounted on ceiling;18.6;1936;104;4000;4000;0.6568;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;83000;L90/B10;80;2;(C0-C180) / (C90-C270) - 94,6° / 94,4°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0047.34/;19.3078.0047.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 2800 PLX EDD 34 830;Surface mounted luminaires;19.3078.0048.34;?215 x 166;surface mounted on ceiling;18.6;1880;101;3000;3000;0.6568;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;83000;L90/B10;80;2;(C0-C180) / (C90-C270) - 94,6° / 94,4°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0048.34/;19.3078.0048.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 2800 PLX EDD 34 840;Surface mounted luminaires;19.3078.0049.34;?215 x 166;surface mounted on ceiling;18.6;1936;104;4000;4000;0.6568;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;83000;L90/B10;80;2;(C0-C180) / (C90-C270) - 94,6° / 94,4°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0049.34/;19.3078.0049.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 3600 E 34 830;Surface mounted luminaires;19.3078.0050.34;?215 x 166;surface mounted on ceiling;25.3;3057;121;3000;3000;0.7672;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_SHM (hardened mat glass);LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0050.34/;19.3078.0050.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 3600 E 34 840;Surface mounted luminaires;19.3078.0051.34;?215 x 166;surface mounted on ceiling;25.3;3147;124;4000;4000;0.7672;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_SHM (hardened mat glass);LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0051.34/;19.3078.0051.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 3600 EDD 34 830;Surface mounted luminaires;19.3078.0052.34;?215 x 166;surface mounted on ceiling;25.3;3057;121;3000;3000;0.7672;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_SHM (hardened mat glass);LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0052.34/;19.3078.0052.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 3600 EDD 34 840;Surface mounted luminaires;19.3078.0053.34;?215 x 166;surface mounted on ceiling;25.3;3147;124;4000;4000;0.7672;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_SHM (hardened mat glass);LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 74,2° / 73,6°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0053.34/;19.3078.0053.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 3600 MICRO-PRM E 34 830;Surface mounted luminaires;19.3078.0054.34;?215 x 166;surface mounted on ceiling;25.3;2823;112;3000;3000;0.7085;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_SHM (hardened mat glass);LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 103° / 101,6°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0054.34/;19.3078.0054.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 3600 MICRO-PRM E 34 840;Surface mounted luminaires;19.3078.0055.34;?215 x 166;surface mounted on ceiling;25.3;2906;115;4000;4000;0.7085;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_SHM (hardened mat glass);LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 103° / 101,6°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0055.34/;19.3078.0055.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 3600 MICRO-PRM EDD 34 830;Surface mounted luminaires;19.3078.0056.34;?215 x 166;surface mounted on ceiling;25.3;2823;112;3000;3000;0.7085;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_SHM (hardened mat glass);LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 103° / 101,6°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0056.34/;19.3078.0056.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 3600 MICRO-PRM EDD 34 840;Surface mounted luminaires;19.3078.0057.34;?215 x 166;surface mounted on ceiling;25.3;2906;115;4000;4000;0.7085;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_SHM (hardened mat glass);LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 103° / 101,6°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0057.34/;19.3078.0057.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 3600 PLX E 34 840;Surface mounted luminaires;19.3078.0058.34;?215 x 166;surface mounted on ceiling;25.3;2694;106;4000;4000;0.6568;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 94,6° / 94,4°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0058.34/;19.3078.0058.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 3600 PLX EDD 34 830;Surface mounted luminaires;19.3078.0059.34;?215 x 166;surface mounted on ceiling;25.3;2617;103;3000;3000;0.6568;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 94,6° / 94,4°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0059.34/;19.3078.0059.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-3 3600 PLX EDD 34 840;Surface mounted luminaires;19.3078.0060.34;?215 x 166;surface mounted on ceiling;25.3;2694;106;4000;4000;0.6568;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;84000;L90/B10;80;2;(C0-C180) / (C90-C270) - 94,6° / 94,4°;IP20;IK04;II;RG0;0,95;0;0;166;215;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0060.34/;19.3078.0060.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
