;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
BERYL SURFACE NEW LED O-1 1000 E 34 830;Surface mounted luminaires;19.3078.0001.34;?135 x 136;surface mounted on ceiling;8;755;94;3000;3000;0.7749;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent PMMA;LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 41° / 40,4°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0001.34/;19.3078.0001.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1000 E 34 840;Surface mounted luminaires;19.3078.0002.34;?135 x 136;surface mounted on ceiling;8;777;97;4000;4000;0.7749;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent PMMA;LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 41° / 40,4°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0002.34/;19.3078.0002.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1000 EDD 34 830;Surface mounted luminaires;19.3078.0003.34;?135 x 136;surface mounted on ceiling;8;755;94;3000;3000;0.7749;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent PMMA;LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 41° / 40,4°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0003.34/;19.3078.0003.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1000 EDD 34 840;Surface mounted luminaires;19.3078.0004.34;?135 x 136;surface mounted on ceiling;8;777;97;4000;4000;0.7749;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent PMMA;LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 41° / 40,4°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0004.34/;19.3078.0004.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1000 MICRO-PRM E 34 830;Surface mounted luminaires;19.3078.0005.34;?135 x 136;surface mounted on ceiling;8;719;90;3000;3000;0.7384;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 89,2° / 87,4°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0005.34/;19.3078.0005.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1000 MICRO-PRM E 34 840;Surface mounted luminaires;19.3078.0006.34;?135 x 136;surface mounted on ceiling;8;741;93;4000;4000;0.7384;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 89,2° / 87,4°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0006.34/;19.3078.0006.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1000 MICRO-PRM EDD 34 830;Surface mounted luminaires;19.3078.0007.34;?135 x 136;surface mounted on ceiling;8;719;90;3000;3000;0.7384;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 89,2° / 87,4°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0007.34/;19.3078.0007.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1000 MICRO-PRM EDD 34 840;Surface mounted luminaires;19.3078.0008.34;?135 x 136;surface mounted on ceiling;8;741;93;4000;4000;0.7384;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 89,2° / 87,4°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0008.34/;19.3078.0008.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1000 PLX E 34 830;Surface mounted luminaires;19.3078.0009.34;?135 x 136;surface mounted on ceiling;8;642;80;3000;3000;0.6592;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 81,6° / 81,6°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0009.34/;19.3078.0009.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1000 PLX E 34 840;Surface mounted luminaires;19.3078.0010.34;?135 x 136;surface mounted on ceiling;8;661;83;4000;4000;0.6592;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 81,6° / 81,6°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0010.34/;19.3078.0010.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1000 PLX EDD 34 830;Surface mounted luminaires;19.3078.0011.34;?135 x 136;surface mounted on ceiling;8;642;80;3000;3000;0.6592;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 81,6° / 81,6°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0011.34/;19.3078.0011.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1000 PLX EDD 34 840;Surface mounted luminaires;19.3078.0012.34;?135 x 136;surface mounted on ceiling;8;661;83;4000;4000;0.6592;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 81,6° / 81,6°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0012.34/;19.3078.0012.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1800 E 34 830;Surface mounted luminaires;19.3078.0013.34;?135 x 136;surface mounted on ceiling;13.2;1473;112;3000;3000;0.7749;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent PMMA;LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 41° / 40,4°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0013.34/;19.3078.0013.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1800 E 34 840;Surface mounted luminaires;19.3078.0014.34;?135 x 136;surface mounted on ceiling;13.2;1516;115;4000;4000;0.7749;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent PMMA;LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 41° / 40,4°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0014.34/;19.3078.0014.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1800 EDD 34 830;Surface mounted luminaires;19.3078.0015.34;?135 x 136;surface mounted on ceiling;13.2;1473;112;3000;3000;0.7749;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent PMMA;LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 41° / 40,4°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0015.34/;19.3078.0015.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1800 EDD 34 840;Surface mounted luminaires;19.3078.0016.34;?135 x 136;surface mounted on ceiling;13.2;1516;115;4000;4000;0.7749;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent PMMA;LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 41° / 40,4°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0016.34/;19.3078.0016.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1800 MICRO-PRM E 34 830;Surface mounted luminaires;19.3078.0017.34;?135 x 136;surface mounted on ceiling;13.2;1403;106;3000;3000;0.7384;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 89,2° / 87,4°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0017.34/;19.3078.0017.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1800 MICRO-PRM E 34 840;Surface mounted luminaires;19.3078.0018.34;?135 x 136;surface mounted on ceiling;13.2;1445;109;4000;4000;0.7384;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 89,2° / 87,4°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0018.34/;19.3078.0018.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1800 MICRO-PRM EDD 34 840;Surface mounted luminaires;19.3078.0019.34;?135 x 136;surface mounted on ceiling;13.2;1445;109;4000;4000;0.7384;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 89,2° / 87,4°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0019.34/;19.3078.0019.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1800 PLX E 34 830;Surface mounted luminaires;19.3078.0020.34;?135 x 136;surface mounted on ceiling;13.2;1253;95;3000;3000;0.6592;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 81,6° / 81,6°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0020.34/;19.3078.0020.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1800 PLX E 34 840;Surface mounted luminaires;19.3078.0021.34;?135 x 136;surface mounted on ceiling;13.2;1290;98;4000;4000;0.6592;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 81,6° / 81,6°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0021.34/;19.3078.0021.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BERYL SURFACE NEW LED O-1 1800 PLX EDD 34 840;Surface mounted luminaires;19.3078.0022.34;?135 x 136;surface mounted on ceiling;13.2;1290;98;4000;4000;0.6592;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;83000;L90/B10;85;2;(C0-C180) / (C90-C270) - 81,6° / 81,6°;IP20;IK04;II;RG0;0,95;0;0;136;135;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/;https://luxiona.pl/en/oferta/oprawy-nastropowe/beryl-surface-new-led-o/19.3078.0022.34/;19.3078.0022.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
