;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
BHU LINEMED TRIANGLE LED P-2600-1300-ON-2-B-B-3-B E OPTICS-3L/PLX 53 830 L=1250MM;Clean luminaires - surface;19.3191.0001.33;1250 x 130 x 110;mounted on wall;26.0;2961;114;3000;3000;0.7316;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9003 (white);LUXIONA_OPTICS/PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;Rozsył asymetryczny;IP40;IK04;I;0;0,95;1250;130;110;0;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/19.3191.0001.33/;19.3191.0001.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BHU LINEMED TRIANGLE LED P-2600-1300-ON-2-B-B-3-B E OPTICS-3L/PLX 53 840 L=1250MM;Clean luminaires - surface;19.3191.0002.33;1250 x 130 x 110;mounted on wall;26.0;3117;120;4000;4000;0.7316;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9003 (white);LUXIONA_OPTICS/PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;Rozsył asymetryczny;IP40;IK04;I;0;0,95;1250;130;110;0;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/19.3191.0002.33/;19.3191.0002.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BHU LINEMED TRIANGLE LED P-4400-2200-ON-2-B-B-3-B E OPTICS-3L/PLX 53 830 L=1250MM;Clean luminaires - surface;19.3191.0003.33;1250 x 130 x 110;mounted on wall;42.0;4840;115;3000;3000;0.7316;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9003 (white);LUXIONA_OPTICS/PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;Rozsył asymetryczny;IP40;IK04;I;0;0,95;1250;130;110;0;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/19.3191.0003.33/;19.3191.0003.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BHU LINEMED TRIANGLE LED P-4400-2200-ON-2-B-B-3-B E OPTICS-3L/PLX 53 840 L=1250MM;Clean luminaires - surface;19.3191.0004.33;1250 x 130 x 110;mounted on wall;42.0;5096;121;4000;4000;0.7316;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9003 (white);LUXIONA_OPTICS/PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;Rozsył asymetryczny;IP40;IK04;I;0;0,95;1250;130;110;0;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/19.3191.0004.33/;19.3191.0004.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BHU LINEMED TRIANGLE LED P-5200-1300-ON-2-B-B-3-B E PLX/PLX 53 830 L=1250MM;Clean luminaires - surface;19.3191.0005.33;1250 x 130 x 110;mounted on wall;43.0;4993;116;3000;3000;0.7403;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9003 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;Rozsył asymetryczny;IP40;IK04;I;0;0,95;1250;130;110;0;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/19.3191.0005.33/;19.3191.0005.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BHU LINEMED TRIANGLE LED P-5200-1300-ON-2-B-B-3-B E PLX/PLX 53 840 L=1250MM;Clean luminaires - surface;19.3191.0006.33;1250 x 130 x 110;mounted on wall;43.0;5256;122;4000;4000;0.7403;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9003 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;Rozsył asymetryczny;IP40;IK04;I;0;0,95;1250;130;110;0;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/19.3191.0006.33/;19.3191.0006.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BHU LINEMED TRIANGLE LED P-8000-2000-ON-2-B-B-3-B E OPTICS-3L/PLX 53 830 L=1250MM;Clean luminaires - surface;19.3191.0007.33;1250 x 130 x 110;mounted on wall;71.0;7393;104;3000;3000;0.7345;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9003 (white);LUXIONA_OPTICS/PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;Rozsył asymetryczny;IP40;IK04;I;0;0,95;1250;130;110;0;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/19.3191.0007.33/;19.3191.0007.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BHU LINEMED TRIANGLE LED P-8000-2000-ON-2-B-B-3-B E OPTICS-3L/PLX 53 840 L=1250MM;Clean luminaires - surface;19.3191.0008.33;1250 x 130 x 110;mounted on wall;71.0;7648;108;4000;4000;0.7345;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9003 (white);LUXIONA_OPTICS/PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;Rozsył asymetryczny;IP40;IK04;I;0;0,95;1250;130;110;0;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/19.3191.0008.33/;19.3191.0008.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BHU LINEMED TRIANGLE LED P-8800-2200-ON-2-B-B-3-B E PLX/PLX 53 830 L=1250MM;Clean luminaires - surface;19.3191.0009.33;1250 x 130 x 110;mounted on wall;70.0;8162;117;3000;3000;0.7403;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9003 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;Rozsył asymetryczny;IP40;IK04;I;0;0,95;1250;130;110;0;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/19.3191.0009.33/;19.3191.0009.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
BHU LINEMED TRIANGLE LED P-8800-2200-ON-2-B-B-3-B E PLX/PLX 53 840 L=1250MM;Clean luminaires - surface;19.3191.0010.33;1250 x 130 x 110;mounted on wall;70.0;8595;123;4000;4000;0.7403;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9003 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;Rozsył asymetryczny;IP40;IK04;I;0;0,95;1250;130;110;0;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/;https://luxiona.pl/oferta/oprawy-clean-nastropowe/bhu-linemed-triangle-led/19.3191.0010.33/;19.3191.0010.33.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA

