;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
DOMINO CLEAN LOW UGR LED 6300 SH RASTER DAISY-BLACK-WIDE E 34 IP65 830 / 592X592;Clean luminaires - recessed;19.3182.1006.34;592 x 592 x 50;mounted in module ceilings;40;4496;112;3000;3000;0.7608;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 71,6° / 75,6°;IP65;IK08;II;0;0,95;592;592;50;0;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/domino-clean-low-ugr-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/domino-clean-low-ugr-led/19.3182.1006.34/;19.3182.1006.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
DOMINO CLEAN LOW UGR LED 6300 SH RASTER DAISY-BLACK-WIDE E 34 IP65 840 / 592X592;Clean luminaires - recessed;19.3182.1005.34;592 x 592 x 50;mounted in module ceilings;40;4738;118;4000;4000;0.7608;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 71,6° / 75,6°;IP65;IK08;II;0;0,95;592;592;50;0;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/domino-clean-low-ugr-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/domino-clean-low-ugr-led/19.3182.1005.34/;19.3182.1005.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
DOMINO CLEAN LOW UGR LED 6300 SH RASTER DAISY-BLACK-WIDE EDD 34 IP65 830 / 592X592;Clean luminaires - recessed;19.3182.1008.34;592 x 592 x 50;mounted in module ceilings;40;4496;112;3000;3000;0.7608;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 71,6° / 75,6°;IP65;IK08;II;0;0,95;592;592;50;0;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/domino-clean-low-ugr-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/domino-clean-low-ugr-led/19.3182.1008.34/;19.3182.1008.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
DOMINO CLEAN LOW UGR LED 6300 SH RASTER DAISY-BLACK-WIDE EDD 34 IP65 840 / 592X592;Clean luminaires - recessed;19.3182.1007.34;592 x 592 x 50;mounted in module ceilings;40;4738;118;4000;4000;0.7608;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 71,6° / 75,6°;IP65;IK08;II;0;0,95;592;592;50;0;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/domino-clean-low-ugr-led/;https://luxiona.pl/oferta/oprawy-clean-do-wbudowania/domino-clean-low-ugr-led/19.3182.1007.34/;19.3182.1007.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
