;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##;LinLight##OTHER##
DOMINO LOW UGR LED 2100 RASTER DAISY-BLACK-WIDE E 34 830 / 596X296;Recessed luminaires;19.3200.3005.34;596 x 296 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;13;1635;126;3000;3000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;596;296;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.3005.34/;19.3200.3005.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1
DOMINO LOW UGR LED 2100 RASTER DAISY-BLACK-WIDE E 34 840 / 596X296;Recessed luminaires;19.3200.3001.34;596 x 296 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;13;1723;133;4000;4000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;596;296;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.3001.34/;19.3200.3001.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1
DOMINO LOW UGR LED 2100 RASTER DAISY-BLACK-WIDE EDD 34 830 / 596X296;Recessed luminaires;19.3200.3007.34;596 x 296 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;13;1635;126;3000;3000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;596;296;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.3007.34/;19.3200.3007.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1
DOMINO LOW UGR LED 2100 RASTER DAISY-BLACK-WIDE EDD 34 840 / 596X296;Recessed luminaires;19.3200.3003.34;596 x 296 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;13;1723;133;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;596;296;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.3003.34/;19.3200.3003.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1
DOMINO LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE E 34 830 / 1196X296;Recessed luminaires;19.3200.2005.34;1196 x 296 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;26;3269;126;3000;3000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;1196;296;2;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.2005.34/;19.3200.2005.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1
DOMINO LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE E 34 830 / 596X296;Recessed luminaires;19.3200.3006.34;596 x 296 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;26;3269;126;3000;3000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;596;296;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.3006.34/;19.3200.3006.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
DOMINO LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE E 34 830 / 596X596;Recessed luminaires;19.3200.1005.34;596 x 596 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;26;3269;126;3000;3000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;596;596;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.1005.34/;19.3200.1005.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
DOMINO LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE E 34 840 / 1196X296;Recessed luminaires;19.3200.2001.34;1196 x 296 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;26;3445;133;4000;4000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;1196;296;2;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.2001.34/;19.3200.2001.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1
DOMINO LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE E 34 840 / 596X296;Recessed luminaires;19.3200.3002.34;596 x 296 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;26;3445;133;4000;4000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;596;296;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.3002.34/;19.3200.3002.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
DOMINO LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE E 34 840 / 596X596;Recessed luminaires;19.3200.1001.34;596 x 596 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;26;3445;133;4000;4000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;596;596;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.1001.34/;19.3200.1001.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
DOMINO LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE EDD 34 830 / 1196X296;Recessed luminaires;19.3200.2007.34;1196 x 296 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;26;3269;126;3000;3000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;1196;296;2;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.2007.34/;19.3200.2007.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1
DOMINO LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE EDD 34 830 / 596X296;Recessed luminaires;19.3200.3008.34;596 x 296 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;26;3269;126;3000;3000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;596;296;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.3008.34/;19.3200.3008.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
DOMINO LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE EDD 34 830 / 596X596;Recessed luminaires;19.3200.1007.34;596 x 596 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;26;3269;126;3000;3000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;596;596;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.1007.34/;19.3200.1007.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
DOMINO LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE EDD 34 840 / 1196X296;Recessed luminaires;19.3200.2003.34;1196 x 296 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;26;3445;133;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;1196;296;2;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.2003.34/;19.3200.2003.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1
DOMINO LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE EDD 34 840 / 596X296;Recessed luminaires;19.3200.3004.34;596 x 296 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;26;3445;133;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;596;296;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.3004.34/;19.3200.3004.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
DOMINO LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE EDD 34 840 / 596X596;Recessed luminaires;19.3200.1003.34;596 x 596 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;26;3445;133;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;596;596;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.1003.34/;19.3200.1003.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
DOMINO LOW UGR LED 6300 RASTER DAISY-BLACK-WIDE E 34 830 / 596X596;Recessed luminaires;19.3200.1006.34;596 x 596 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;40;4904;123;3000;3000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;596;596;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.1006.34/;19.3200.1006.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;3
DOMINO LOW UGR LED 6300 RASTER DAISY-BLACK-WIDE E 34 840 / 596X596;Recessed luminaires;19.3200.1002.34;596 x 596 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;40;5168;129;4000;4000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;596;596;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.1002.34/;19.3200.1002.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;3
DOMINO LOW UGR LED 6300 RASTER DAISY-BLACK-WIDE EDD 34 830 / 596X596;Recessed luminaires;19.3200.1008.34;596 x 596 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;40;4904;123;3000;3000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;596;596;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.1008.34/;19.3200.1008.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;3
DOMINO LOW UGR LED 6300 RASTER DAISY-BLACK-WIDE EDD 34 840 / 596X596;Recessed luminaires;19.3200.1004.34;596 x 596 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;40;5168;129;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;596;596;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.1004.34/;19.3200.1004.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;3
DOMINO LOW UGR LED 8400 RASTER DAISY-BLACK-WIDE E 34 830 / 1196X296;Recessed luminaires;19.3200.2006.34;1196 x 296 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;53;6539;123;3000;3000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;1196;296;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.2006.34/;19.3200.2006.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
DOMINO LOW UGR LED 8400 RASTER DAISY-BLACK-WIDE E 34 840 / 1196X296;Recessed luminaires;19.3200.2002.34;1196 x 296 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;53;6891;130;4000;4000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;1196;296;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.2002.34/;19.3200.2002.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
DOMINO LOW UGR LED 8400 RASTER DAISY-BLACK-WIDE EDD 34 830 / 1196X296;Recessed luminaires;19.3200.2008.34;1196 x 296 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;53;6539;123;3000;3000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;1196;296;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.2008.34/;19.3200.2008.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
DOMINO LOW UGR LED 8400 RASTER DAISY-BLACK-WIDE EDD 34 840 / 1196X296;Recessed luminaires;19.3200.2004.34;1196 x 296 x 23;mounted in module ceilings, plasterboard ceilings, directly on the ceiling or using the suspensions;53;6891;130;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;1196;296;23;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.2004.34/;19.3200.2004.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
DOMINO LOW UGR LED 1200 RASTER DAISY-BLACK-WIDE E 34 830 / 250x250 RECESSED;Recessed luminaires;19.3200.4006.34;250 x 250 x 43;mounted in plasterboard ceilings;8;973;122;3000;3000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;250;250;43;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.4006.34/;19.3200.4006.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
DOMINO LOW UGR LED 1200 RASTER DAISY-BLACK-WIDE E 34 840 / 250x250 RECESSED;Recessed luminaires;19.3200.4002.34;250 x 250 x 43;mounted in plasterboard ceilings;8;987;123;4000;4000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;250;250;43;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.4002.34/;19.3200.4002.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
DOMINO LOW UGR LED 1200 RASTER DAISY-BLACK-WIDE EDD 34 830 / 250x250 RECESSED;Recessed luminaires;19.3200.4008.34;250 x 250 x 43;mounted in plasterboard ceilings;8;973;122;3000;3000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;250;250;43;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.4008.34/;19.3200.4008.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
DOMINO LOW UGR LED 1200 RASTER DAISY-BLACK-WIDE EDD 34 840 / 250x250 RECESSED;Recessed luminaires;19.3200.4004.34;250 x 250 x 43;mounted in plasterboard ceilings;8;987;123;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;250;250;43;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.4004.34/;19.3200.4004.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;2
DOMINO LOW UGR LED 1800 RASTER DAISY-BLACK-WIDE E 34 830 / 250x250 RECESSED;Recessed luminaires;19.3200.4005.34;250 x 250 x 43;mounted in plasterboard ceilings;12;1457;121;3000;3000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;250;250;43;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.4005.34/;19.3200.4005.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;3
DOMINO LOW UGR LED 1800 RASTER DAISY-BLACK-WIDE E 34 840 / 250x250 RECESSED;Recessed luminaires;19.3200.4001.34;250 x 250 x 43;mounted in plasterboard ceilings;12;1482;124;4000;4000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;250;250;43;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.4001.34/;19.3200.4001.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;3
DOMINO LOW UGR LED 1800 RASTER DAISY-BLACK-WIDE EDD 34 830 / 250x250 RECESSED;Recessed luminaires;19.3200.4007.34;250 x 250 x 43;mounted in plasterboard ceilings;12;1457;121;3000;3000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;250;250;43;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.4007.34/;19.3200.4007.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;3
DOMINO LOW UGR LED 1800 RASTER DAISY-BLACK-WIDE EDD 34 840 / 250x250 RECESSED;Recessed luminaires;19.3200.4003.34;250 x 250 x 43;mounted in plasterboard ceilings;12;1482;124;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;250;250;43;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.4003.34/;19.3200.4003.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;3
DOMINO LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE E 34 830 / 1196X75;Recessed luminaires;19.3200.7002.34;1196 x 75 x 50;mounted in module ceilings, plasterboard ceilings;26;3269;126;3000;3000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;1196;75;50;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.7002.34/;19.3200.7002.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1
DOMINO LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE E 34 840 / 1196X75;Recessed luminaires;19.3200.7001.34;1196 x 75 x 50;mounted in module ceilings, plasterboard ceilings;26;3445;133;4000;4000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;1196;75;50;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.7001.34/;19.3200.7001.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1
DOMINO LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE EDD 34 830 / 1196X75;Recessed luminaires;19.3200.7004.34;1196 x 75 x 50;mounted in module ceilings, plasterboard ceilings;26;3269;126;3000;3000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;1196;75;50;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.7004.34/;19.3200.7004.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;"1
"
DOMINO LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE EDD 34 840 / 1196X75;Recessed luminaires;19.3200.7003.34;1196 x 75 x 50;mounted in module ceilings, plasterboard ceilings;26;3445;133;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;1196;75;50;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.7003.34/;19.3200.7003.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1
DOMINO LOW UGR LED 600 RASTER DAISY-BLACK-WIDE E 34 830 / 150X150 RECESSED;Recessed luminaires;19.3200.5001.34;150 x 150 x 43;mounted in plasterboard ceilings;4;484;121;3000;3000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;150;150;43;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.5001.34/;19.3200.5001.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
DOMINO LOW UGR LED 600 RASTER DAISY-BLACK-WIDE E 34 840 / 150X150 RECESSED;Recessed luminaires;19.3200.5002.34;150 x 150 x 43;mounted in plasterboard ceilings;4;494;123;4000;4000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;150;150;43;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.5002.34/;19.3200.5002.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
DOMINO LOW UGR LED 600 RASTER DAISY-BLACK-WIDE EDD 34 830 / 150X150 RECESSED;Recessed luminaires;19.3200.5003.34;150 x 150 x 43;mounted in plasterboard ceilings;4;484;121;3000;3000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;150;150;43;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.5003.34/;19.3200.5003.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
DOMINO LOW UGR LED 600 RASTER DAISY-BLACK-WIDE EDD 34 840 / 150X150 RECESSED;Recessed luminaires;19.3200.5004.34;150 x 150 x 43;mounted in plasterboard ceilings;4;494;123;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;150;150;43;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.5004.34/;19.3200.5004.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
DOMINO LOW UGR LED 1200 RASTER DAISY-BLACK-WIDE E 34 830 / 150X150 RECESSED;Recessed luminaires;19.3200.5005.34;150 x 150 x 43;mounted in plasterboard ceilings;8;973;122;3000;3000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;150;150;43;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.5005.34/;19.3200.5005.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
DOMINO LOW UGR LED 1200 RASTER DAISY-BLACK-WIDE E 34 840 / 150X150 RECESSED;Recessed luminaires;19.3200.5006.34;150 x 150 x 43;mounted in plasterboard ceilings;8;987;123;4000;4000;0.8298;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;150;150;43;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.5006.34/;19.3200.5006.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
DOMINO LOW UGR LED 1200 RASTER DAISY-BLACK-WIDE EDD 34 830 / 150X150 RECESSED;Recessed luminaires;19.3200.5007.34;150 x 150 x 43;mounted in plasterboard ceilings;8;973;122;3000;3000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;150;150;43;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.5007.34/;19.3200.5007.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
DOMINO LOW UGR LED 1200 RASTER DAISY-BLACK-WIDE EDD 34 840 / 150X150 RECESSED;Recessed luminaires;19.3200.5008.34;150 x 150 x 43;mounted in plasterboard ceilings;8;987;123;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP20;IK04;II;0;0.95;150;150;43;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/;https://luxiona.pl/oferta/oprawy-do-wbudowania/domino-low-ugr-led/19.3200.5008.34/;19.3200.5008.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0
