;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
EUROPANEL LED 3800 MICRO-PRM E 34 IP20 840 / 1200X300 S-1,5M;Surface mounted luminaires;19.3082.0001.34;1196 x 296 x 11;surface mounted on slings;21;2575;123;4000;4000;0.705;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;63000 (1) / 53000 (2);L70/B50 (1) / L80/B10 (2);>80;3;(C0-C180) / (C90-C270) - 91,8° / 94,4°;IP20;IK04;II;RG0;0,95;1196;296;11;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/19.3082.0001.34/;19.3082.0001.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
EUROPANEL LED 3800 MICRO-PRM E 34 IP20 840 / S-1,5M;Surface mounted luminaires;19.3082.0002.34;596 x 596 x 11;surface mounted on slings;21;2765;132;4000;4000;0.757;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;63000 (1) / 53000 (2);L70/B50 (1) / L80/B10 (2);>80;3;(C0-C180) / (C90-C270) - 93° / 82,6°;IP20;IK04;II;RG0;0,95;596;596;11;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/19.3082.0002.34/;19.3082.0002.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
EUROPANEL LED 3800 MICRO-PRM EDD 34 IP20 840 / S-1,5M;Surface mounted luminaires;19.3082.0003.34;596 x 596 x 11;surface mounted on slings;21;2765;132;4000;4000;0.757;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;63000 (1) / 53000 (2);L70/B50 (1) / L80/B10 (2);>80;3;(C0-C180) / (C90-C270) - 93° / 82,6°;IP20;IK04;II;RG0;0,95;596;596;11;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/19.3082.0003.34/;19.3082.0003.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
EUROPANEL LED 3800 MICRO-PRM E-LF 34 IP20 840 / S-1,5M;Surface mounted luminaires;19.3082.0004.34;596 x 596 x 11;surface mounted on slings;21;2765;132;4000;4000;0.757;low output flicker driver (E-LF);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;63000 (1) / 53000 (2);L70/B50 (1) / L80/B10 (2);>80;3;(C0-C180) / (C90-C270) - 93° / 82,6°;IP20;IK04;II;RG0;0,95;596;596;11;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/19.3082.0004.34/;19.3082.0004.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
EUROPANEL LED 3800 PLX E 34 IP20 840 / 1200X300 S-1,5M;Surface mounted luminaires;19.3082.0005.34;1196 x 296 x 11;surface mounted on slings;21;2466;117;4000;4000;0.675;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;63000 (1) / 53000 (2);L70/B50 (1) / L80/B10 (2);>80;3;(C0-C180) / (C90-C270) - 117° / 110,8°;IP20;IK04;II;RG0;0,95;1196;296;11;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/19.3082.0005.34/;19.3082.0005.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
EUROPANEL LED 3800 PLX E 34 IP20 840 / S-1,5M;Surface mounted luminaires;19.3082.0006.34;596 x 596 x 11;surface mounted on slings;21;2645;126;4000;4000;0.724;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;63000 (1) / 53000 (2);L70/B50 (1) / L80/B10 (2);>80;3;(C0-C180) / (C90-C270) - 115,4° / 107,6°;IP20;IK04;II;RG0;0,95;596;596;11;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/19.3082.0006.34/;19.3082.0006.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
EUROPANEL LED 3800 PLX EDD 34 IP20 840 / S-1,5M;Surface mounted luminaires;19.3082.0007.34;596 x 596 x 11;surface mounted on slings;21;2645;126;4000;4000;0.724;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;63000 (1) / 53000 (2);L70/B50 (1) / L80/B10 (2);>80;3;(C0-C180) / (C90-C270) - 115,4° / 107,6°;IP20;IK04;II;RG0;0,95;596;596;11;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/19.3082.0007.34/;19.3082.0007.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
EUROPANEL LED 4800 MICRO-PRM E 34 IP20 840 / S-1,5M;Surface mounted luminaires;19.3082.0008.34;596 x 596 x 11;surface mounted on slings;29.3;3857;132;4000;4000;0.757;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;63000 (1) / 53000 (2);L70/B50 (1) / L80/B10 (2);>80;3;(C0-C180) / (C90-C270) - 93° / 82,6°;IP20;IK04;II;RG0;0,95;596;596;11;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/19.3082.0008.34/;19.3082.0008.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
EUROPANEL LED 4800 MICRO-PRM EDD 34 IP20 840 / S-1,5M;Surface mounted luminaires;19.3082.0009.34;596 x 596 x 11;surface mounted on slings;29.3;3857;132;4000;4000;0.757;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;63000 (1) / 53000 (2);L70/B50 (1) / L80/B10 (2);>80;3;(C0-C180) / (C90-C270) - 93° / 82,6°;IP20;IK04;II;RG0;0,95;596;596;11;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/19.3082.0009.34/;19.3082.0009.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
EUROPANEL LED 4800 PLX E 34 IP20 840 / S-1,5M;Surface mounted luminaires;19.3082.0010.34;596 x 596 x 11;surface mounted on slings;29.3;3689;126;4000;4000;0.724;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;63000 (1) / 53000 (2);L70/B50 (1) / L80/B10 (2);>80;3;(C0-C180) / (C90-C270) - 115,4° / 107,6°;IP20;IK04;II;RG0;0,95;596;596;11;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/19.3082.0010.34/;19.3082.0010.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
EUROPANEL LED 4800 PLX EDD 34 IP20 840 / S-1,5M;Surface mounted luminaires;19.3082.0011.34;596 x 596 x 11;surface mounted on slings;29.3;3689;126;4000;4000;0.724;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;63000 (1) / 53000 (2);L70/B50 (1) / L80/B10 (2);>80;3;(C0-C180) / (C90-C270) - 115,4° / 107,6°;IP20;IK04;II;RG0;0,95;596;596;11;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/19.3082.0011.34/;19.3082.0011.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
EUROPANEL LED 5800 MICRO-PRM E 34 IP20 840 / 1200X300 S-1,5M;Surface mounted luminaires;19.3082.0012.34;1196 x 296 x 11;surface mounted on slings;46;4345;94;4000;4000;0.705;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;63000 (1) / 53000 (2);L70/B50 (1) / L80/B10 (2);>80;3;(C0-C180) / (C90-C270) - 91,8° / 94,4°;IP20;IK04;II;RG0;0,95;1196;296;11;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/19.3082.0012.34/;19.3082.0012.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
EUROPANEL LED 5800 MICRO-PRM E 34 IP20 840 / S-1,5M;Surface mounted luminaires;19.3082.0013.34;596 x 596 x 11;surface mounted on slings;45.6;4666;102;4000;4000;0.757;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;63000 (1) / 53000 (2);L70/B50 (1) / L80/B10 (2);>80;3;(C0-C180) / (C90-C270) - 93° / 82,6°;IP20;IK04;II;RG0;0,95;596;596;11;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/19.3082.0013.34/;19.3082.0013.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
EUROPANEL LED 5800 MICRO-PRM EDD 34 IP20 840 / 1200X300 S-1,5M;Surface mounted luminaires;19.3082.0014.34;1196 x 296 x 11;surface mounted on slings;46;4345;94;4000;4000;0.705;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;63000 (1) / 53000 (2);L70/B50 (1) / L80/B10 (2);>80;3;(C0-C180) / (C90-C270) - 91,8° / 94,4°;IP20;IK04;II;RG0;0,95;1196;296;11;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/19.3082.0014.34/;19.3082.0014.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
EUROPANEL LED 5800 MICRO-PRM EDD 34 IP20 840 / S-1,5M;Surface mounted luminaires;19.3082.0015.34;596 x 596 x 11;surface mounted on slings;45.6;4666;102;4000;4000;0.757;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;63000 (1) / 53000 (2);L70/B50 (1) / L80/B10 (2);>80;3;(C0-C180) / (C90-C270) - 93° / 82,6°;IP20;IK04;II;RG0;0,95;596;596;11;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/19.3082.0015.34/;19.3082.0015.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
EUROPANEL LED 5800 MICRO-PRM E-LF 34 IP20 840 / 1200X300 S-1,5M;Surface mounted luminaires;19.3082.0016.34;1196 x 296 x 11;surface mounted on slings;46;4345;94;4000;4000;0.705;low output flicker driver (E-LF);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;63000 (1) / 53000 (2);L70/B50 (1) / L80/B10 (2);>80;3;(C0-C180) / (C90-C270) - 91,8° / 94,4°;IP20;IK04;II;RG0;0,95;1196;296;11;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/19.3082.0016.34/;19.3082.0016.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
EUROPANEL LED 5800 PLX E 34 IP20 840 / S-1,5M;Surface mounted luminaires;19.3082.0017.34;596 x 596 x 11;surface mounted on slings;45.6;4462;98;4000;4000;0.724;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;63000 (1) / 53000 (2);L70/B50 (1) / L80/B10 (2);>80;3;(C0-C180) / (C90-C270) - 115,4° / 107,6°;IP20;IK04;II;RG0;0,95;596;596;11;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/19.3082.0017.34/;19.3082.0017.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
EUROPANEL LED 5800 PLX E 34 IP20 840 / 1200X300 S-1,5M;Surface mounted luminaires;19.3082.0018.34;1196 x 296 x 11;surface mounted on slings;46;4160;90;4000;4000;0.675;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;63000 (1) / 53000 (2);L70/B50 (1) / L80/B10 (2);>80;3;(C0-C180) / (C90-C270) - 117° / 110,8°;IP20;IK04;II;RG0;0,95;1196;296;11;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/19.3082.0018.34/;19.3082.0018.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
EUROPANEL LED 5800 PLX EDD 34 IP20 840 / S-1,5M;Surface mounted luminaires;19.3082.0019.34;596 x 596 x 11;surface mounted on slings;45.6;4462;98;4000;4000;0.724;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;63000 (1) / 53000 (2);L70/B50 (1) / L80/B10 (2);>80;3;(C0-C180) / (C90-C270) - 115,4° / 107,6°;IP20;IK04;II;RG0;0,95;596;596;11;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/;https://luxiona.pl/en/oferta/oprawy-nastropowe/europanel-led-s-15m/19.3082.0019.34/;19.3082.0019.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
