;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
KUBIK 2D LED 1800 SYM E IP65 25 840 / L-300;Outdoor luminaires;19.3147.0001.25;200 x 120 x 300;for the ground;12.5;1543;123;4000;4000;0.6805;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 7016 (anthracite, metallic, fine structure);LUXIONA_none;LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);>80;2;Rozsył asymetryczny;IP65;IK03;I;0;0.95;200;120;300;https://luxiona.pl/oferta/oprawy-zewnetrzne/kubik-2d-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/kubik-2d-led/19.3147.0001.25/;19.3147.0001.25_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
KUBIK 2D LED 1800 SYM E IP65 25 840 / L-600;Outdoor luminaires;19.3147.0002.25;200 x 120 x 600;for the ground;12.5;1543;123;4000;4000;0.6805;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 7016 (anthracite, metallic, fine structure);LUXIONA_none;LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);>80;2;Rozsył asymetryczny;IP65;IK03;I;0;0.95;200;120;600;https://luxiona.pl/oferta/oprawy-zewnetrzne/kubik-2d-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/kubik-2d-led/19.3147.0002.25/;19.3147.0002.25_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
KUBIK 2D LED 1800 SYM E IP65 25 840 / L-900;Outdoor luminaires;19.3147.0003.25;200 x 120 x 900;for the ground;12.5;1543;123;4000;4000;0.6805;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 7016 (anthracite, metallic, fine structure);LUXIONA_none;LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);>80;2;Rozsył asymetryczny;IP65;IK03;I;0;0.95;200;120;900;https://luxiona.pl/oferta/oprawy-zewnetrzne/kubik-2d-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/kubik-2d-led/19.3147.0003.25/;19.3147.0003.25_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
