;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
LOTOS ELEGANCE ROUND LUXIONA_PC LED COMPACT V2 1200 E IP54 830;Compact;19.3209.0019.34;?220 x 54;surface mounted on ceiling or on wall;12.5;1360;109;3000;3000;0.6659;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_white;LUXIONA_PC (opalescent polycarbonate);LED;0;30000;L70/B10;>80;0;(C0-C180) / (C90-C270) - 113,8° / 118,8°;IP54;IK08;II;0;0;54;220;https://luxiona.pl/oferta/compact/lotos-elegance-round-LUXIONA_PC-led-compact-v2/;https://luxiona.pl/oferta/compact/lotos-elegance-round-LUXIONA_PC-led-compact-v2/19.3209.0019.34/;19.3209.0019.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LOTOS ELEGANCE ROUND LUXIONA_PC LED COMPACT V2 1200 E IP54 840;Compact;19.3209.0020.34;?220 x 55;surface mounted on ceiling or on wall;12.5;1463;117;4000;4000;0.6659;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_white;LUXIONA_PC (opalescent polycarbonate);LED;0;30000;L70/B10;>80;0;(C0-C180) / (C90-C270) - 113,8° / 118,8°;IP54;IK08;II;0;0;54;220;https://luxiona.pl/oferta/compact/lotos-elegance-round-LUXIONA_PC-led-compact-v2/;https://luxiona.pl/oferta/compact/lotos-elegance-round-LUXIONA_PC-led-compact-v2/19.3209.0020.34/;19.3209.0020.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LOTOS ELEGANCE ROUND LUXIONA_PC LED COMPACT V2 1200 E CMW IP54 830;Compact;19.3209.0021.34;?220 x 56;surface mounted on ceiling or on wall;12.5;1360;109;3000;3000;0.6659;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_white;LUXIONA_PC (opalescent polycarbonate);LED;0;30000;L70/B10;>80;0;(C0-C180) / (C90-C270) - 113,8° / 118,8°;IP54;IK08;II;0;0;54;220;https://luxiona.pl/oferta/compact/lotos-elegance-round-LUXIONA_PC-led-compact-v2/;https://luxiona.pl/oferta/compact/lotos-elegance-round-LUXIONA_PC-led-compact-v2/19.3209.0021.34/;19.3209.0021.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LOTOS ELEGANCE ROUND LUXIONA_PC LED COMPACT V2 1200 E CMW IP54 840;Compact;19.3209.0022.34;?220 x 57;surface mounted on ceiling or on wall;12.5;1463;117;4000;4000;0.6659;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_white;LUXIONA_PC (opalescent polycarbonate);LED;0;30000;L70/B10;>80;0;(C0-C180) / (C90-C270) - 113,8° / 118,8°;IP54;IK08;II;0;0;54;220;https://luxiona.pl/oferta/compact/lotos-elegance-round-LUXIONA_PC-led-compact-v2/;https://luxiona.pl/oferta/compact/lotos-elegance-round-LUXIONA_PC-led-compact-v2/19.3209.0022.34/;19.3209.0022.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LOTOS ELEGANCE ROUND LUXIONA_PC LED COMPACT V2 1800 E IP54 840;Compact;19.3209.0002.34;?280 x 54;surface mounted on ceiling or on wall;17.3;1942;112;4000;4000;0.6659;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_white;LUXIONA_PC (opalescent polycarbonate);LED;0;30000;L70/B10;>80;0;(C0-C180) / (C90-C270) - 113,8° / 118,8°;IP54;IK08;II;0;0;54;280;https://luxiona.pl/oferta/compact/lotos-elegance-round-LUXIONA_PC-led-compact-v2/;https://luxiona.pl/oferta/compact/lotos-elegance-round-LUXIONA_PC-led-compact-v2/19.3209.0002.34/;19.3209.0002.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LOTOS ELEGANCE ROUND LUXIONA_PC LED COMPACT V2 1800 E CMW IP54 840;Compact;19.3209.0010.34;?280 x 55;surface mounted on ceiling or on wall;17.3;1942;112;4000;4000;0.6659;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_white;LUXIONA_PC (opalescent polycarbonate);LED;0;30000;L70/B10;>80;0;(C0-C180) / (C90-C270) - 113,8° / 118,8°;IP54;IK08;II;0;0;54;280;https://luxiona.pl/oferta/compact/lotos-elegance-round-LUXIONA_PC-led-compact-v2/;https://luxiona.pl/oferta/compact/lotos-elegance-round-LUXIONA_PC-led-compact-v2/19.3209.0010.34/;19.3209.0010.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
