;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
LUXCAN R 1800 13° E 04 840 3F;Projectors;19.3067.0001.04;?108 x 210;mounted on a three-phase track;12.8;1654;129;4000;4000;0.8039;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0001.04/;19.3067.0001.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 1800 13° E 21 840 3F;Projectors;19.3067.0001.21;?108 x 210;mounted on a three-phase track;12.8;1654;129;4000;4000;0.8039;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0001.21/;19.3067.0001.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 1800 13° E 63 840 3F;Projectors;19.3067.0001.63;?108 x 210;mounted on a three-phase track;12.8;1654;129;4000;4000;0.8039;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;50000;L80/B10;82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0001.63/;19.3067.0001.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 1800 13° EDD 04 840 3F;Projectors;19.3067.0002.04;?108 x 210;mounted on a three-phase track;12.8;1654;129;4000;4000;0.8039;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0002.04/;19.3067.0002.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 1800 13° EDD 21 840 3F;Projectors;19.3067.0002.21;?108 x 210;mounted on a three-phase track;12.8;1654;129;4000;4000;0.8039;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0002.21/;19.3067.0002.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 1800 13° EDD 63 840 3F;Projectors;19.3067.0002.63;?108 x 210;mounted on a three-phase track;12.8;1654;129;4000;4000;0.8039;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0002.63/;19.3067.0002.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 1800 36° E 04 840 3F;Projectors;19.3067.0003.04;?108 x 210;mounted on a three-phase track;12.8;1611;126;4000;4000;0.7828;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0003.04/;19.3067.0003.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 1800 36° E 21 840 3F;Projectors;19.3067.0003.21;?108 x 210;mounted on a three-phase track;12.8;1611;126;4000;4000;0.7828;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0003.21/;19.3067.0003.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 1800 36° E 63 840 3F;Projectors;19.3067.0003.63;?108 x 210;mounted on a three-phase track;12.8;1611;126;4000;4000;0.7828;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0003.63/;19.3067.0003.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 1800 36° EDD 04 840 3F;Projectors;19.3067.0004.04;?108 x 210;mounted on a three-phase track;12.8;1611;126;4000;4000;0.7828;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0004.04/;19.3067.0004.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 1800 36° EDD 21 840 3F;Projectors;19.3067.0004.21;?108 x 210;mounted on a three-phase track;12.8;1611;126;4000;4000;0.7828;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0004.21/;19.3067.0004.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 1800 36° EDD 63 840 3F;Projectors;19.3067.0004.63;?108 x 210;mounted on a three-phase track;12.8;1611;126;4000;4000;0.7828;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0004.63/;19.3067.0004.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 1800 60° E 04 840 3F;Projectors;19.3067.0005.04;?108 x 210;mounted on a three-phase track;12.8;1648;129;4000;4000;0.8008;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0005.04/;19.3067.0005.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 1800 60° E 21 840 3F;Projectors;19.3067.0005.21;?108 x 210;mounted on a three-phase track;12.8;1648;129;4000;4000;0.8008;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0005.21/;19.3067.0005.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 1800 60° E 63 840 3F;Projectors;19.3067.0005.63;?108 x 210;mounted on a three-phase track;12.8;1648;129;4000;4000;0.8008;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0005.63/;19.3067.0005.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 1800 60° EDD 04 840 3F;Projectors;19.3067.0006.04;?108 x 210;mounted on a three-phase track;12.8;1648;129;4000;4000;0.8008;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0006.04/;19.3067.0006.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 1800 60° EDD 21 840 3F;Projectors;19.3067.0006.21;?108 x 210;mounted on a three-phase track;12.8;1648;129;4000;4000;0.8008;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0006.21/;19.3067.0006.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 1800 60° EDD 63 840 3F;Projectors;19.3067.0006.63;?108 x 210;mounted on a three-phase track;12.8;1648;129;4000;4000;0.8008;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0006.63/;19.3067.0006.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 2500 13° E 04 840 3F;Projectors;19.3067.0007.04;?108 x 210;mounted on a three-phase track;18.8;2178;116;4000;4000;0.8039;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0007.04/;19.3067.0007.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 2500 13° E 21 840 3F;Projectors;19.3067.0007.21;?108 x 210;mounted on a three-phase track;18.8;2178;116;4000;4000;0.8039;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0007.21/;19.3067.0007.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 2500 13° E 63 840 3F;Projectors;19.3067.0007.63;?108 x 210;mounted on a three-phase track;18.8;2178;116;4000;4000;0.8039;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0007.63/;19.3067.0007.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 2500 13° EDD 04 840 3F;Projectors;19.3067.0008.04;?108 x 210;mounted on a three-phase track;18.8;2178;116;4000;4000;0.8039;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0008.04/;19.3067.0008.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 2500 13° EDD 21 840 3F;Projectors;19.3067.0008.21;?108 x 210;mounted on a three-phase track;18.8;2178;116;4000;4000;0.8039;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0008.21/;19.3067.0008.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 2500 13° EDD 63 840 3F;Projectors;19.3067.0008.63;?108 x 210;mounted on a three-phase track;18.8;2178;116;4000;4000;0.8039;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0008.63/;19.3067.0008.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 2500 36° E 04 840 3F;Projectors;19.3067.0009.04;?108 x 210;mounted on a three-phase track;18.8;2121;113;4000;4000;0.7828;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0009.04/;19.3067.0009.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 2500 36° E 21 840 3F;Projectors;19.3067.0009.21;?108 x 210;mounted on a three-phase track;18.8;2121;113;4000;4000;0.7828;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0009.21/;19.3067.0009.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 2500 36° E 63 840 3F;Projectors;19.3067.0009.63;?108 x 210;mounted on a three-phase track;18.8;2121;113;4000;4000;0.7828;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0009.63/;19.3067.0009.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 2500 36° EDD 04 840 3F;Projectors;19.3067.0010.04;?108 x 210;mounted on a three-phase track;18.8;2121;113;4000;4000;0.7828;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0010.04/;19.3067.0010.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 2500 36° EDD 21 840 3F;Projectors;19.3067.0010.21;?108 x 210;mounted on a three-phase track;18.8;2121;113;4000;4000;0.7828;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0010.21/;19.3067.0010.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 2500 36° EDD 63 840 3F;Projectors;19.3067.0010.63;?108 x 210;mounted on a three-phase track;18.8;2121;113;4000;4000;0.7828;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0010.63/;19.3067.0010.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 2500 60° E 04 840 3F;Projectors;19.3067.0011.04;?108 x 210;mounted on a three-phase track;18.8;2169;115;4000;4000;0.8008;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0011.04/;19.3067.0011.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 2500 60° E 21 840 3F;Projectors;19.3067.0011.21;?108 x 210;mounted on a three-phase track;18.8;2169;115;4000;4000;0.8008;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0011.21/;19.3067.0011.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 2500 60° E 63 840 3F;Projectors;19.3067.0011.63;?108 x 210;mounted on a three-phase track;18.8;2169;115;4000;4000;0.8008;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0011.63/;19.3067.0011.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 2500 60° EDD 04 840 3F;Projectors;19.3067.0012.04;?108 x 210;mounted on a three-phase track;18.8;2169;115;4000;4000;0.8008;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0012.04/;19.3067.0012.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 2500 60° EDD 21 840 3F;Projectors;19.3067.0012.21;?108 x 210;mounted on a three-phase track;18.8;2169;115;4000;4000;0.8008;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0012.21/;19.3067.0012.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 2500 60° EDD 63 840 3F;Projectors;19.3067.0012.63;?108 x 210;mounted on a three-phase track;18.8;2169;115;4000;4000;0.8008;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0012.63/;19.3067.0012.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 3700 13° E 04 840 3F;Projectors;19.3067.0013.04;?108 x 210;mounted on a three-phase track;26.4;3305;125;4000;4000;0.8039;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0013.04/;19.3067.0013.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 3700 13° E 21 840 3F;Projectors;19.3067.0013.21;?108 x 210;mounted on a three-phase track;26.4;3305;125;4000;4000;0.8039;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0013.21/;19.3067.0013.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 3700 13° E 63 840 3F;Projectors;19.3067.0013.63;?108 x 210;mounted on a three-phase track;26.4;3305;125;4000;4000;0.8039;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0013.63/;19.3067.0013.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 3700 13° EDD 04 840 3F;Projectors;19.3067.0014.04;?108 x 210;mounted on a three-phase track;26.4;3305;125;4000;4000;0.8039;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0014.04/;19.3067.0014.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 3700 13° EDD 21 840 3F;Projectors;19.3067.0014.21;?108 x 210;mounted on a three-phase track;26.4;3305;125;4000;4000;0.8039;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0014.21/;19.3067.0014.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 3700 13° EDD 63 840 3F;Projectors;19.3067.0014.63;?108 x 210;mounted on a three-phase track;26.4;3305;125;4000;4000;0.8039;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0014.63/;19.3067.0014.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 3700 36° E 04 840 3F;Projectors;19.3067.0015.04;?108 x 210;mounted on a three-phase track;26.4;3218;122;4000;4000;0.7828;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0015.04/;19.3067.0015.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 3700 36° E 21 840 3F;Projectors;19.3067.0015.21;?108 x 210;mounted on a three-phase track;26.4;3218;122;4000;4000;0.7828;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0015.21/;19.3067.0015.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 3700 36° E 63 840 3F;Projectors;19.3067.0015.63;?108 x 210;mounted on a three-phase track;26.4;3218;122;4000;4000;0.7828;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0015.63/;19.3067.0015.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 3700 36° EDD 04 840 3F;Projectors;19.3067.0016.04;?108 x 210;mounted on a three-phase track;26.4;3218;122;4000;4000;0.7828;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0016.04/;19.3067.0016.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 3700 36° EDD 21 840 3F;Projectors;19.3067.0016.21;?108 x 210;mounted on a three-phase track;26.4;3218;122;4000;4000;0.7828;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0016.21/;19.3067.0016.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 3700 36° EDD 63 840 3F;Projectors;19.3067.0016.63;?108 x 210;mounted on a three-phase track;26.4;3218;122;4000;4000;0.7828;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0016.63/;19.3067.0016.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 3700 60° E 04 840 3F;Projectors;19.3067.0017.04;?108 x 210;mounted on a three-phase track;26.4;3292;125;4000;4000;0.8008;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0017.04/;19.3067.0017.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 3700 60° E 21 840 3F;Projectors;19.3067.0017.21;?108 x 210;mounted on a three-phase track;26.4;3292;125;4000;4000;0.8008;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0017.21/;19.3067.0017.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 3700 60° E 63 840 3F;Projectors;19.3067.0017.63;?108 x 210;mounted on a three-phase track;26.4;3292;125;4000;4000;0.8008;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0017.63/;19.3067.0017.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 3700 60° EDD 04 840 3F;Projectors;19.3067.0018.04;?108 x 210;mounted on a three-phase track;26.4;3292;125;4000;4000;0.8008;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0018.04/;19.3067.0018.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 3700 60° EDD 21 840 3F;Projectors;19.3067.0018.21;?108 x 210;mounted on a three-phase track;26.4;3292;125;4000;4000;0.8008;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0018.21/;19.3067.0018.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 3700 60° EDD 63 840 3F;Projectors;19.3067.0018.63;?108 x 210;mounted on a three-phase track;26.4;3292;125;4000;4000;0.8008;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;86000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0018.63/;19.3067.0018.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 4800 13° E 04 840 3F;Projectors;19.3067.0019.04;?108 x 210;mounted on a three-phase track;33.1;4241;128;4000;4000;0.8039;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0019.04/;19.3067.0019.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 4800 13° E 21 840 3F;Projectors;19.3067.0019.21;?108 x 210;mounted on a three-phase track;33.1;4241;128;4000;4000;0.8039;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0019.21/;19.3067.0019.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 4800 13° E 63 840 3F;Projectors;19.3067.0019.63;?108 x 210;mounted on a three-phase track;33.1;4241;128;4000;4000;0.8039;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0019.63/;19.3067.0019.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 4800 13° EDD 04 840 3F;Projectors;19.3067.0020.04;?108 x 210;mounted on a three-phase track;33.1;4241;128;4000;4000;0.8039;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0020.04/;19.3067.0020.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 4800 13° EDD 21 840 3F;Projectors;19.3067.0020.21;?108 x 210;mounted on a three-phase track;33.1;4241;128;4000;4000;0.8039;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0020.21/;19.3067.0020.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 4800 13° EDD 63 840 3F;Projectors;19.3067.0020.63;?108 x 210;mounted on a three-phase track;33.1;4241;128;4000;4000;0.8039;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 11,6° / 13,4°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0020.63/;19.3067.0020.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 4800 36° E 04 840 3F;Projectors;19.3067.0021.04;?108 x 210;mounted on a three-phase track;33.1;4130;125;4000;4000;0.7828;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0021.04/;19.3067.0021.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 4800 36° E 21 840 3F;Projectors;19.3067.0021.21;?108 x 210;mounted on a three-phase track;33.1;4130;125;4000;4000;0.7828;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0021.21/;19.3067.0021.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 4800 36° E 63 840 3F;Projectors;19.3067.0021.63;?108 x 210;mounted on a three-phase track;33.1;4130;125;4000;4000;0.7828;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0021.63/;19.3067.0021.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 4800 36° EDD 04 840 3F;Projectors;19.3067.0022.04;?108 x 210;mounted on a three-phase track;33.1;4130;125;4000;4000;0.7828;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0022.04/;19.3067.0022.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 4800 36° EDD 21 840 3F;Projectors;19.3067.0022.21;?108 x 210;mounted on a three-phase track;33.1;4130;125;4000;4000;0.7828;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0022.21/;19.3067.0022.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 4800 36° EDD 63 840 3F;Projectors;19.3067.0022.63;?108 x 210;mounted on a three-phase track;33.1;4130;125;4000;4000;0.7828;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 36° / 33,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0022.63/;19.3067.0022.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 4800 60° E 04 840 3F;Projectors;19.3067.0023.04;?108 x 210;mounted on a three-phase track;33.1;4225;128;4000;4000;0.8008;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0023.04/;19.3067.0023.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 4800 60° E 21 840 3F;Projectors;19.3067.0023.21;?108 x 210;mounted on a three-phase track;33.1;4225;128;4000;4000;0.8008;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0023.21/;19.3067.0023.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 4800 60° E 63 840 3F;Projectors;19.3067.0023.63;?108 x 210;mounted on a three-phase track;33.1;4225;128;4000;4000;0.8008;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0023.63/;19.3067.0023.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 4800 60° EDD 04 840 3F;Projectors;19.3067.0024.04;?108 x 210;mounted on a three-phase track;33.1;4225;128;4000;4000;0.8008;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0024.04/;19.3067.0024.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 4800 60° EDD 21 840 3F;Projectors;19.3067.0024.21;?108 x 210;mounted on a three-phase track;33.1;4225;128;4000;4000;0.8008;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0024.21/;19.3067.0024.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LUXCAN R 4800 60° EDD 63 840 3F;Projectors;19.3067.0024.63;?108 x 210;mounted on a three-phase track;33.1;4225;128;4000;4000;0.8008;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9003 (white);LED;-0.571428571;77000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);82;3;(C0-C180) / (C90-C270) - 56,2° / 53,2°;IP20;IK04;I;0;0,95;0;0;210;108;https://luxiona.pl/oferta/projektory/luxcan-r/;https://luxiona.pl/oferta/projektory/luxcan-r/19.3067.0024.63/;19.3067.0024.63.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
