;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
METEOR LED COMPACT 4000 OPAL E 830 / L-1200;Surface mounted luminaires;19.3244.0001.34;1255 x 207 x 71;surface mounted on ceiling;27;3172;117;3000;3000;0.8015;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;50000;L70/B50;>80;3;(C0-C180) / (C90-C270) - 121,6° / 110,4°;IP20;IK04;I;0;0.95;1255;207;71;https://luxiona.pl/oferta/compact/meteor-led-compact/;https://luxiona.pl/oferta/compact/meteor-led-compact/19.3244.0001.34/;19.3244.0001.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
METEOR LED COMPACT 4000 OPAL E 840 / L-1200;Surface mounted luminaires;19.3244.0002.34;1255 x 207 x 71;surface mounted on ceiling;27;3516;130;4000;4000;0.8015;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;50000;L70/B50;>80;3;(C0-C180) / (C90-C270) - 121,6° / 110,4°;IP20;IK04;I;0;0.95;1255;207;71;https://luxiona.pl/oferta/compact/meteor-led-compact/;https://luxiona.pl/oferta/compact/meteor-led-compact/19.3244.0002.34/;19.3244.0002.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
METEOR LED COMPACT 6000 OPAL E 830 / L-1200;Surface mounted luminaires;19.3244.0003.34;1255 x 207 x 71;surface mounted on ceiling;39;4278;110;3000;3000;0.8015;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;50000;L70/B50;>80;3;(C0-C180) / (C90-C270) - 121,6° / 110,4°;IP20;IK04;I;0;0.95;1255;207;71;https://luxiona.pl/oferta/compact/meteor-led-compact/;https://luxiona.pl/oferta/compact/meteor-led-compact/19.3244.0003.34/;19.3244.0003.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
METEOR LED COMPACT 6000 OPAL E 840 / L-1200;Surface mounted luminaires;19.3244.0004.34;1255 x 207 x 71;surface mounted on ceiling;39;4787;123;4000;4000;0.8015;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;50000;L70/B50;>80;3;(C0-C180) / (C90-C270) - 121,6° / 110,4°;IP20;IK04;I;0;0.95;1255;207;71;https://luxiona.pl/oferta/compact/meteor-led-compact/;https://luxiona.pl/oferta/compact/meteor-led-compact/19.3244.0004.34/;19.3244.0004.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
METEOR LED COMPACT 8000 OPAL E 830 / L-1200;Surface mounted luminaires;19.3244.0006.34;1255 x 207 x 71;surface mounted on ceiling;55;6473;118;3000;3000;0.8179;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;50000;L70/B50;>80;3;(C0-C180) / (C90-C270) - 119,4° / 109,2°;IP20;IK04;I;0;0.95;1255;207;71;https://luxiona.pl/oferta/compact/meteor-led-compact/;https://luxiona.pl/oferta/compact/meteor-led-compact/19.3244.0006.34/;19.3244.0006.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
METEOR LED COMPACT 8000 OPAL E 840 / L-1200;Surface mounted luminaires;19.3244.0007.34;1255 x 207 x 71;surface mounted on ceiling;55;7176;130;4000;4000;0.8179;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9010 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;50000;L70/B50;>80;3;(C0-C180) / (C90-C270) - 119,4° / 109,2°;IP20;IK04;I;0;0.95;1255;207;71;https://luxiona.pl/oferta/compact/meteor-led-compact/;https://luxiona.pl/oferta/compact/meteor-led-compact/19.3244.0007.34/;19.3244.0007.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
