;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
NEPTUN LED V2 1300 PC-FROZEN E 21 IP66 830 / L-600;Industrial luminaires;19.3208.0009.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;7.3;1103;151;3000;3000;0.9162;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0009.21/;19.3208.0009.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 1300 PC-FROZEN E 21 IP66 830 / L-600 ZASIALNIE PRZELOTOWE 16A;Industrial luminaires;19.3208.0021.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;7.0;1103;158;3000;3000;0.9162;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0021.21/;19.3208.0021.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 1300 PC-FROZEN E 21 IP66 840 / L-600;Industrial luminaires;19.3208.0010.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;7.3;1230;168;4000;4000;0.9162;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0010.21/;19.3208.0010.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 1300 PC-FROZEN E 21 IP66 840 / L-600 ZASILANIE PRZELOTOWE 16A;Industrial luminaires;19.3208.0022.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;7.0;1230;176;4000;4000;0.9162;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0022.21/;19.3208.0022.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 1300 PC-FROZEN EDD 21 IP66 830 / L-600;Industrial luminaires;19.3208.0011.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;7.3;1103;151;3000;3000;0.9162;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0011.21/;19.3208.0011.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 1300 PC-FROZEN EDD 21 IP66 830 / L-600 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3208.0023.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;7.0;1103;158;3000;3000;0.9162;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0023.21/;19.3208.0023.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 1300 PC-FROZEN EDD 21 IP66 840 / L-600;Industrial luminaires;19.3208.0012.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;7.3;1230;168;4000;4000;0.9162;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0012.21/;19.3208.0012.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 1300 PC-FROZEN EDD 21 IP66 840 / L-600 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3208.0024.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;7.0;1230;176;4000;4000;0.9162;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0024.21/;19.3208.0024.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 2200 PC-FROZEN E 21 IP66 830 / L-600;Industrial luminaires;19.3208.0001.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;12.3;1932;157;3000;3000;0.9162;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0001.21/;19.3208.0001.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 2200 PC-FROZEN E 21 IP66 830 / L-600 ZASIALNIE PRZELOTOWE 16A;Industrial luminaires;19.3208.0013.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;12.0;1932;161;3000;3000;0.9162;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0013.21/;19.3208.0013.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 2200 PC-FROZEN E 21 IP66 840 / L-600;Industrial luminaires;19.3208.0002.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;12.3;2153;175;4000;4000;0.9162;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0002.21/;19.3208.0002.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 2200 PC-FROZEN E 21 IP66 840 / L-600 ZASILANIE PRZELOTOWE 16A;Industrial luminaires;19.3208.0014.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;12.0;2153;179;4000;4000;0.9162;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0014.21/;19.3208.0014.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 2200 PC-FROZEN EDD 21 IP66 830 / L-600;Industrial luminaires;19.3208.0003.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;12.3;1932;157;3000;3000;0.9162;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0003.21/;19.3208.0003.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 2200 PC-FROZEN EDD 21 IP66 830 / L-600 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3208.0015.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;12.0;1932;161;3000;3000;0.9162;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0015.21/;19.3208.0015.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 2200 PC-FROZEN EDD 21 IP66 840 / L-600;Industrial luminaires;19.3208.0004.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;12.3;2153;175;4000;4000;0.9162;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0004.21/;19.3208.0004.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 2200 PC-FROZEN EDD 21 IP66 840 / L-600 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3208.0016.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;12.0;2153;179;4000;4000;0.9162;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0016.21/;19.3208.0016.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 4400 PC-FROZEN E 21 IP66 830 / L-600;Industrial luminaires;19.3208.0005.21;620 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;24.2;3756;155;3000;3000;0.8902;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123° / 107,2°;IP66;IK10;I;0;0,95;620;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0005.21/;19.3208.0005.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 4400 PC-FROZEN E 21 IP66 830 / L-600 ZASILANIE PRZELOTOWE 16A;Industrial luminaires;19.3208.0017.21;620 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;24.0;3756;156;3000;3000;0.8902;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123° / 107,2°;IP66;IK10;I;0;0,95;620;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0017.21/;19.3208.0017.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 4400 PC-FROZEN E 21 IP66 840 / L-600;Industrial luminaires;19.3208.0006.21;620 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;24.2;4184;173;4000;4000;0.8902;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123° / 107,2°;IP66;IK10;I;0;0,95;620;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0006.21/;19.3208.0006.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 4400 PC-FROZEN E 21 IP66 840 / L-600 ZASIALNIE PRZELOTOWE 16A;Industrial luminaires;19.3208.0018.21;620 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;24.0;4184;174;4000;4000;0.8902;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123° / 107,2°;IP66;IK10;I;0;0,95;620;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0018.21/;19.3208.0018.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 4400 PC-FROZEN EDD 21 IP66 830 / L-600;Industrial luminaires;19.3208.0007.21;620 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;24.2;3756;155;3000;3000;0.8902;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123° / 107,2°;IP66;IK10;I;0;0,95;620;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0007.21/;19.3208.0007.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 4400 PC-FROZEN EDD 21 IP66 830 / L-600 ZASIALNIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3208.0019.21;620 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;24.0;3756;156;3000;3000;0.8902;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123° / 107,2°;IP66;IK10;I;0;0,95;620;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0019.21/;19.3208.0019.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 4400 PC-FROZEN EDD 21 IP66 840 / L-600;Industrial luminaires;19.3208.0008.21;620 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;24.2;4184;173;4000;4000;0.8902;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123° / 107,2°;IP66;IK10;I;0;0,95;620;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0008.21/;19.3208.0008.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 4400 PC-FROZEN EDD 21 IP66 840 / L-600 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3208.0020.21;620 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;24.0;4184;174;4000;4000;0.8902;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 123° / 107,2°;IP66;IK10;I;0;0,95;620;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3208.0020.21/;19.3208.0020.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 4400 PC-FROZEN E 21 IP66 830 / L-1200;Industrial luminaires;19.3206.0005.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;28.5;4511;158;3000;3000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0005.21/;19.3206.0005.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 4400 PC-FROZEN E 21 IP66 830 / L-1200 ZASILANIE PRZELOTOWE 16A;Industrial luminaires;19.3206.0025.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;29.0;4511;156;3000;3000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0025.21/;19.3206.0025.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 4400 PC-FROZEN E 21 IP66 840 / L-1200;Industrial luminaires;19.3206.0006.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;28.5;4741;166;4000;4000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0006.21/;19.3206.0006.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 4400 PC-FROZEN E 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 16A;Industrial luminaires;19.3206.0026.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;29.0;4741;163;4000;4000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0026.21/;19.3206.0026.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 4400 PC-FROZEN EDD 21 IP66 830 / L-1200;Industrial luminaires;19.3206.0007.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;28.5;4511;158;3000;3000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0007.21/;19.3206.0007.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 4400 PC-FROZEN EDD 21 IP66 830 / L-1200 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3206.0027.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;29.0;4511;156;3000;3000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0027.21/;19.3206.0027.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 4400 PC-FROZEN EDD 21 IP66 840 / L-1200;Industrial luminaires;19.3206.0008.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;28.5;4741;166;4000;4000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0008.21/;19.3206.0008.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 4400 PC-FROZEN EDD 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3206.0028.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;29.0;4741;163;4000;4000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0028.21/;19.3206.0028.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 4400 PC-FROZEN E 21 IP66 840 / L-1200, HT50;Industrial luminaires;19.3206.0047.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;28.5;4741;166;4000;4000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-40 ÷ 50;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0047.21/;19.3206.0047.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 4400 PC-FROZEN E 21 IP66 840 / L-1200,ZASILANIE PRZELOTOWE 16A , HT50;Industrial luminaires;19.3206.0051.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;28.5;4741;166;4000;4000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-40 ÷ 50;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0051.21/;19.3206.0051.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5200 PC-FROZEN E 21 IP66 830 / L-1200;Industrial luminaires;19.3206.0009.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;35.1;5562;158;3000;3000;0.9169;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0009.21/;19.3206.0009.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5200 PC-FROZEN E 21 IP66 830 / L-1200 ZASILANIE PRZELOTOWE 16A;Industrial luminaires;19.3206.0029.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;35.0;5562;159;3000;3000;0.9169;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0029.21/;19.3206.0029.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5200 PC-FROZEN E 21 IP66 840 / L-1200;Industrial luminaires;19.3206.0010.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;35.1;5845;167;4000;4000;0.9169;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0010.21/;19.3206.0010.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5200 PC-FROZEN E 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 16A;Industrial luminaires;19.3206.0030.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;35.0;5845;167;4000;4000;0.9169;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0030.21/;19.3206.0030.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5200 PC-FROZEN EDD 21 IP66 830 / L-1200;Industrial luminaires;19.3206.0011.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;35.1;5562;158;3000;3000;0.9169;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0011.21/;19.3206.0011.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5200 PC-FROZEN EDD 21 IP66 830 / L-1200 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3206.0031.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;35.0;5562;159;3000;3000;0.9169;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0031.21/;19.3206.0031.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5200 PC-FROZEN EDD 21 IP66 840 / L-1200;Industrial luminaires;19.3206.0012.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;35.1;5845;167;4000;4000;0.9169;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0012.21/;19.3206.0012.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5200 PC-FROZEN EDD 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3206.0032.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;35.0;5845;167;4000;4000;0.9169;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0032.21/;19.3206.0032.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5200 PC-FROZEN E 21 IP66 840 / L-1200, HT50;Industrial luminaires;19.3206.0048.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;35.1;5845;167;4000;4000;0.9169;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-40 ÷ 50;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0048.21/;19.3206.0048.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5200 PC-FROZEN E 21 IP66 840 / L-1200, ZASILANIE PRZELOTOWE 16A , HT50;Industrial luminaires;19.3206.0050.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;35.1;5845;167;4000;4000;0.9169;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-40 ÷ 50;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0050.21/;19.3206.0050.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5500 PC-FROZEN E 21 IP66 830 / L-1500;Industrial luminaires;19.3204.0005.21;1520 x72 x 60;directly mounted to ceiling construction or surface mounted on slings;34.7;5712;165;3000;3000;0.9418;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 116,4° / 102,2°;IP66;IK10;I;0;0,95;1520;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0005.21/;19.3204.0005.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5500 PC-FROZEN E 21 IP66 830 / L-1500 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3204.0021.21;1520 x72 x 60;directly mounted to ceiling construction or surface mounted on slings;35.0;5712;163;3000;3000;0.9418;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 116,4° / 102,2°;IP66;IK10;I;0;0,95;1520;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0021.21/;19.3204.0021.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5500 PC-FROZEN E 21 IP66 840 / L-1500;Industrial luminaires;19.3204.0006.21;1520 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;34.7;6005;173;4000;4000;0.9418;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 116,4° / 102,2°;IP66;IK10;I;0;0,95;1520;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0006.21/;19.3204.0006.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5500 PC-FROZEN E 21 IP66 840 / L-1500 ZASILANIE PRZELOTOWE 16A;Industrial luminaires;19.3204.0022.21;1520 x72 x 60;directly mounted to ceiling construction or surface mounted on slings;35.0;6005;172;4000;4000;0.9418;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 116,4° / 102,2°;IP66;IK10;I;0;0,95;1520;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0022.21/;19.3204.0022.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5500 PC-FROZEN EDD 21 IP66 830 / L-1500;Industrial luminaires;19.3204.0007.21;1520 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;34.7;5712;165;3000;3000;0.9418;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 116,4° / 102,2°;IP66;IK10;I;0;0,95;1520;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0007.21/;19.3204.0007.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5500 PC-FROZEN EDD 21 IP66 830 / L-1500 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3204.0023.21;1520 x72 x 60;directly mounted to ceiling construction or surface mounted on slings;35.0;5712;163;3000;3000;0.9418;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 116,4° / 102,2°;IP66;IK10;I;0;0,95;1520;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0023.21/;19.3204.0023.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5500 PC-FROZEN EDD 21 IP66 840 / L-1500;Industrial luminaires;19.3204.0008.21;1520 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;34.7;6005;173;4000;4000;0.9418;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 116,4° / 102,2°;IP66;IK10;I;0;0,95;1520;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0008.21/;19.3204.0008.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5500 PC-FROZEN EDD 21 IP66 840 / L-1500 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3204.0024.21;1520 x72 x 60;directly mounted to ceiling construction or surface mounted on slings;35.0;6005;172;4000;4000;0.9418;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 116,4° / 102,2°;IP66;IK10;I;0;0,95;1520;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0024.21/;19.3204.0024.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5500 PC-FROZEN E 21 IP66 840 / L-1500, HT50;Industrial luminaires;19.3204.0033.21;1520 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;34.7;6005;173;4000;4000;0.9418;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-40 ÷ 50;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 116,4° / 102,2°;IP66;IK10;I;0;0,95;1520;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0033.21/;19.3204.0033.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 5500 PC-FROZEN E 21 IP66 840 / L-1500,ZASILANIE PRZELOTOWE 16A , HT50;Industrial luminaires;19.3204.0034.21;1520 x72 x 60;directly mounted to ceiling construction or surface mounted on slings;34.7;6005;173;4000;4000;0.9418;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-40 ÷ 50;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 116,4° / 102,2°;IP66;IK10;I;0;0,95;1520;72;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0034.21/;19.3204.0034.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 7500 PC-FROZEN E 21 IP66 830 / L-1500;Industrial luminaires;19.3204.0009.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;42.2;7125;169;3000;3000;0.9398;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0009.21/;19.3204.0009.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 7500 PC-FROZEN E 21 IP66 830 / L-1500 ZASILANIE PRZELOTOWE 16A;Industrial luminaires;19.3204.0025.21;1520 x92 x 60;directly mounted to ceiling construction or surface mounted on slings;42.0;7125;170;3000;3000;0.9398;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0025.21/;19.3204.0025.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 7500 PC-FROZEN E 21 IP66 840 / L-1500;Industrial luminaires;19.3204.0010.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;42.2;7491;178;4000;4000;0.9398;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0010.21/;19.3204.0010.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 7500 PC-FROZEN E 21 IP66 840 / L-1500 ZASILANIE PRZELOTOWE 16A;Industrial luminaires;19.3204.0026.21;1520 x92 x 60;directly mounted to ceiling construction or surface mounted on slings;42.0;7491;178;4000;4000;0.9398;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0026.21/;19.3204.0026.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 7500 PC-FROZEN EDD 21 IP66 830 / L-1500;Industrial luminaires;19.3204.0011.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;42.2;7125;169;3000;3000;0.9398;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0011.21/;19.3204.0011.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 7500 PC-FROZEN EDD 21 IP66 830 / L-1500 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3204.0027.21;1520 x92 x 60;directly mounted to ceiling construction or surface mounted on slings;42.0;7125;170;3000;3000;0.9398;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0027.21/;19.3204.0027.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 7500 PC-FROZEN EDD 21 IP66 840 / L-1500;Industrial luminaires;19.3204.0012.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;42.2;7491;178;4000;4000;0.9398;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0012.21/;19.3204.0012.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 7500 PC-FROZEN EDD 21 IP66 840 / L-1500 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3204.0028.21;1520 x92 x 60;directly mounted to ceiling construction or surface mounted on slings;42.0;7491;178;4000;4000;0.9398;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0028.21/;19.3204.0028.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 7500 PC-FROZEN E 21 IP66 840 / L-1500, HT50;Industrial luminaires;19.3204.0035.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;42.2;7491;178;4000;4000;0.9398;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-40 ÷ 50;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0035.21/;19.3204.0035.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 7500 PC-FROZEN E 21 IP66 840 / L-1500,ZASILANIE PRZELOTOWE 16A , HT50;Industrial luminaires;19.3204.0036.21;1520 x92 x 60;directly mounted to ceiling construction or surface mounted on slings;42.2;7491;178;4000;4000;0.9398;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-40 ÷ 50;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0036.21/;19.3204.0036.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 8800 PC-FROZEN E 21 IP66 830 / L-1200;Industrial luminaires;19.3206.0013.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;46.9;7895;168;3000;3000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0013.21/;19.3206.0013.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 8800 PC-FROZEN E 21 IP66 830 / L-1200 ZASILANIE PRZELOTOWE 16A;Industrial luminaires;19.3206.0033.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;47.0;7895;168;3000;3000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0033.21/;19.3206.0033.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 8800 PC-FROZEN E 21 IP66 840 / L-1200;Industrial luminaires;19.3206.0014.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;46.9;8298;177;4000;4000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0014.21/;19.3206.0014.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 8800 PC-FROZEN E 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 16A;Industrial luminaires;19.3206.0034.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;47.0;8298;177;4000;4000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0034.21/;19.3206.0034.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 8800 PC-FROZEN EDD 21 IP66 830 / L-1200;Industrial luminaires;19.3206.0015.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;46.9;7895;168;3000;3000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0015.21/;19.3206.0015.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 8800 PC-FROZEN EDD 21 IP66 830 / L-1200 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3206.0035.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;47.0;7895;168;3000;3000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0035.21/;19.3206.0035.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 8800 PC-FROZEN EDD 21 IP66 840 / L-1200;Industrial luminaires;19.3206.0016.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;46.9;8298;177;4000;4000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0016.21/;19.3206.0016.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 8800 PC-FROZEN EDD 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3206.0036.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;47.0;8298;177;4000;4000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0036.21/;19.3206.0036.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 8800 PC-FROZEN E 21 IP66 840 / L-1200, HT50;Industrial luminaires;19.3206.0046.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;46.9;8298;177;4000;4000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-40 ÷ 50;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0046.21/;19.3206.0046.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 8800 PC-FROZEN E 21 IP66 840 / L-1200,ZASILANIE PRZELOTOWE 16A , HT50;Industrial luminaires;19.3206.0049.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;46.9;8298;177;4000;4000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-40 ÷ 50;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0049.21/;19.3206.0049.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 10000 PC-FROZEN E 21 IP66 830 / L-1200;Industrial luminaires;19.3206.0017.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;56.8;9022;159;3000;3000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0017.21/;19.3206.0017.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 10000 PC-FROZEN E 21 IP66 830 / L-1200 ZASILANIE PRZELOTOWE 16A;Industrial luminaires;19.3206.0037.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;57.0;9022;158;3000;3000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0037.21/;19.3206.0037.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 10000 PC-FROZEN E 21 IP66 840 / L-1200;Industrial luminaires;19.3206.0018.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;56.8;9483;167;4000;4000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0018.21/;19.3206.0018.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 10000 PC-FROZEN E 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 16A;Industrial luminaires;19.3206.0038.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;57.0;9483;166;4000;4000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0038.21/;19.3206.0038.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 10000 PC-FROZEN EDD 21 IP66 830 / L-1200;Industrial luminaires;19.3206.0019.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;56.8;9022;159;3000;3000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0019.21/;19.3206.0019.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 10000 PC-FROZEN EDD 21 IP66 830 / L-1200 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3206.0039.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;57.0;9022;158;3000;3000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0039.21/;19.3206.0039.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 10000 PC-FROZEN EDD 21 IP66 840 / L-1200;Industrial luminaires;19.3206.0020.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;56.8;9483;167;4000;4000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0020.21/;19.3206.0020.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 10000 PC-FROZEN EDD 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3206.0040.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;57.0;9483;166;4000;4000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0040.21/;19.3206.0040.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 11000 PC-FROZEN E 21 IP66 830 / L-1500;Industrial luminaires;19.3204.0013.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;57.7;9974;173;3000;3000;0.9398;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0013.21/;19.3204.0013.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 11000 PC-FROZEN E 21 IP66 830 / L-1500 ZASILANIE PRZELOTOWE 16A;Industrial luminaires;19.3204.0029.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;58.0;9974;172;3000;3000;0.9398;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0029.21/;19.3204.0029.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 11000 PC-FROZEN E 21 IP66 840 / L-1500;Industrial luminaires;19.3204.0014.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;57.7;10485;182;4000;4000;0.9398;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0014.21/;19.3204.0014.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 11000 PC-FROZEN E 21 IP66 840 / L-1500 ZASILANIE PRZELOTOWE 16A;Industrial luminaires;19.3204.0030.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;58.0;10485;181;4000;4000;0.9398;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0030.21/;19.3204.0030.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 11000 PC-FROZEN EDD 21 IP66 830 / L-1500;Industrial luminaires;19.3204.0015.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;57.7;9974;173;3000;3000;0.9398;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0015.21/;19.3204.0015.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 11000 PC-FROZEN EDD 21 IP66 830 / L-1500 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3204.0031.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;58.0;9974;172;3000;3000;0.9398;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0031.21/;19.3204.0031.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 11000 PC-FROZEN EDD 21 IP66 840 / L-1500;Industrial luminaires;19.3204.0016.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;57.7;10485;182;4000;4000;0.9398;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0016.21/;19.3204.0016.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 11000 PC-FROZEN EDD 21 IP66 840 / L-1500 ZASILANIE PRZELOTOWE 16A 5X;Industrial luminaires;19.3204.0032.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;58.0;10485;181;4000;4000;0.9398;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3204.0032.21/;19.3204.0032.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 16000 PC-FROZEN E 21 IP66 840 / L-1200;Industrial luminaires;19.3206.0041.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;97.4;14890;153;4000;4000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0041.21/;19.3206.0041.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED V2 16000 PC-FROZEN E 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 16A;Industrial luminaires;19.3206.0043.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;97.4;14890;153;4000;4000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/;https://luxiona.pl/oferta/oprawy-przemyslowe/neptun-led-v2/19.3206.0043.21/;19.3206.0043.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
