;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
ONLINE SURFACE 1X MAX23W TC-DSE E27 PLX 34 IP44;Surface mounted luminaires;19.3089.0002.34;300 x 92 x 87;surface mounted on ceiling;11;461;42;4000;0;0.4374;none;230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);RETROFIT E27 (brak w komplecie);0;w zależności od użytego źródła światła;w zależności od użytego źródła światła;w zależności od użytego źródła światła;w zależności od użytego źródła światła;(C0-C180) / (C90-C270) - 113,2° / 114,4°;IP44;IK04;I;0;0;300;92;87;https://luxiona.pl/en/oferta/oprawy-nastropowe/online-e27/;https://luxiona.pl/en/oferta/oprawy-nastropowe/online-e27/19.3089.0002.34/;19.3089.0002.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
