;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
PATOS-LINE LED 1300 PLX E 830 LINE-S / L-562 mm;Architectural luminaires;19.3031.0106.34;562 x 77 x 81;mounted in plasterboard ceilings;9;899;100;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,9;562;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0106.34/;19.3031.0106.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1300 PLX E 840 LINE-S / L-562 mm;Architectural luminaires;19.3031.0103.34;562 x 77 x 81;mounted in plasterboard ceilings;9;947;105;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,9;562;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0103.34/;19.3031.0103.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2200 PLX E 830 LINE-S / L-562 mm;Architectural luminaires;19.3031.0114.34;562 x 77 x 81;mounted in plasterboard ceilings;12.6;1469;117;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,9;562;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0114.34/;19.3031.0114.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2200 PLX E 840 LINE-S / L-562MM;Architectural luminaires;19.3031.0117.34;562 x 77 x 81;mounted in plasterboard ceilings;12.6;1522;121;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,9;562;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0117.34/;19.3031.0117.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2600 PLX E 830 LINE-S / L-1122MM;Architectural luminaires;19.3031.0306.34;1122 x 77 x 81;mounted in plasterboard ceilings;14.4;1683;117;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1122;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0306.34/;19.3031.0306.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2600 PLX E 840 LINE-S / L-1122 mm;Architectural luminaires;19.3031.0303.34;1122 x 77 x 81;mounted in plasterboard ceilings;14.4;1744;121;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1122;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0303.34/;19.3031.0303.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3250 PLX E 830 LINE-S / L-1402MM;Architectural luminaires;19.3031.0406.34;1402 x 77 x 81;mounted in plasterboard ceilings;18.3;2105;115;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1402;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0406.34/;19.3031.0406.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3250 PLX E 840 LINE-S / L-1402 mm;Architectural luminaires;19.3031.0403.34;1402 x 77 x 81;mounted in plasterboard ceilings;18.3;2182;119;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1402;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0403.34/;19.3031.0403.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3900 PLX E 830 LINE-S / L-1682MM;Architectural luminaires;19.3031.0506.34;1682 x 77 x 81;mounted in plasterboard ceilings;21.7;2525;116;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1682;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0506.34/;19.3031.0506.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3900 PLX E 840 LINE-S / L-1682 mm;Architectural luminaires;19.3031.0503.34;1682 x 77 x 81;mounted in plasterboard ceilings;21.7;2617;121;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1682;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0503.34/;19.3031.0503.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 4400 PLX E 830 LINE-S / L-1122 mm;Architectural luminaires;19.3031.0324.34;1122 x 77 x 81;mounted in plasterboard ceilings;24.7;2937;119;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1122;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0324.34/;19.3031.0324.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 4400 PLX E 840 LINE-S / L-1122 mm;Architectural luminaires;19.3031.0327.34;1122 x 77 x 81;mounted in plasterboard ceilings;24.7;3043;123;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1122;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0327.34/;19.3031.0327.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 5500 PLX E 830 LINE-S / L-1402 mm;Architectural luminaires;19.3031.0426.34;1122 x 77 x 81;mounted in plasterboard ceilings;30.5;3684;121;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1122;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0426.34/;19.3031.0426.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 5500 PLX E 840 LINE-S / L-1402MM;Architectural luminaires;19.3031.0429.34;1122 x 77 x 81;mounted in plasterboard ceilings;30.5;3818;125;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1122;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0429.34/;19.3031.0429.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 6600 PLX E 830 LINE-S / L-1682 mm;Architectural luminaires;19.3031.0515.34;1682 x 77 x 81;mounted in plasterboard ceilings;35.3;4405;125;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1682;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0515.34/;19.3031.0515.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
