;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
ROLLER LED 1000 FLOOD E IP65 04 830;Outdoor luminaires;19.3172.0001.04;145 x 260;surface mounted on ceiling or on wall;9.8;983;100;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0001.04/;19.3172.0001.04_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1000 FLOOD E IP65 04 840;Outdoor luminaires;19.3172.0002.04;145 x 260;surface mounted on ceiling or on wall;9.8;1010;103;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0002.04/;19.3172.0002.04_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1000 FLOOD E IP65 21 830;Outdoor luminaires;19.3172.0001.21;145 x 260;surface mounted on ceiling or on wall;9.8;983;100;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0001.21/;19.3172.0001.21_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1000 FLOOD E IP65 21 840;Outdoor luminaires;19.3172.0002.21;145 x 260;surface mounted on ceiling or on wall;9.8;1010;103;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0002.21/;19.3172.0002.21_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1000 FLOOD E IP65 22 830;Outdoor luminaires;19.3172.0001.22;145 x 260;surface mounted on ceiling or on wall;9.8;983;100;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9007 (dark gray);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0001.22/;19.3172.0001.22_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1000 FLOOD E IP65 22 840;Outdoor luminaires;19.3172.0002.22;145 x 260;surface mounted on ceiling or on wall;9.8;1010;103;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9007 (dark gray);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0002.22/;19.3172.0002.22_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1000 FLOOD E IP65 25 830;Outdoor luminaires;19.3172.0001.25;145 x 260;surface mounted on ceiling or on wall;9.8;983;100;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 7016 (anthracite, metallic, fine structure);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0001.25/;19.3172.0001.25_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1000 FLOOD E IP65 25 840;Outdoor luminaires;19.3172.0002.25;145 x 260;surface mounted on ceiling or on wall;9.8;1010;103;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 7016 (anthracite, metallic, fine structure);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0002.25/;19.3172.0002.25_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1000 FLOOD E IP65 34 830;Outdoor luminaires;19.3172.0001.34;145 x 260;surface mounted on ceiling or on wall;9.8;983;100;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0001.34/;19.3172.0001.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1000 FLOOD E IP65 34 840;Outdoor luminaires;19.3172.0002.34;145 x 260;surface mounted on ceiling or on wall;9.8;1010;103;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0002.34/;19.3172.0002.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1000 FLOOD E PIR IP65 04 830;Outdoor luminaires;19.3172.0003.04;145 x 260;surface mounted on ceiling or on wall;9.8;983;100;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0003.04/;19.3172.0003.04_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1000 FLOOD E PIR IP65 04 840;Outdoor luminaires;19.3172.0004.04;145 x 260;surface mounted on ceiling or on wall;9.8;1010;103;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0004.04/;19.3172.0004.04_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1000 FLOOD E PIR IP65 21 830;Outdoor luminaires;19.3172.0003.21;145 x 260;surface mounted on ceiling or on wall;9.8;983;100;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0003.21/;19.3172.0003.21_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1000 FLOOD E PIR IP65 21 840;Outdoor luminaires;19.3172.0004.21;145 x 260;surface mounted on ceiling or on wall;9.8;1010;103;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0004.21/;19.3172.0004.21_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1000 FLOOD E PIR IP65 22 830;Outdoor luminaires;19.3172.0003.22;145 x 260;surface mounted on ceiling or on wall;9.8;983;100;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9007 (dark gray);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0003.22/;19.3172.0003.22_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1000 FLOOD E PIR IP65 22 840;Outdoor luminaires;19.3172.0004.22;145 x 260;surface mounted on ceiling or on wall;9.8;1010;103;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9007 (dark gray);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0004.22/;19.3172.0004.22_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1000 FLOOD E PIR IP65 25 830;Outdoor luminaires;19.3172.0003.25;145 x 260;surface mounted on ceiling or on wall;9.8;983;100;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 7016 (anthracite, metallic, fine structure);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0003.25/;19.3172.0003.25_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1000 FLOOD E PIR IP65 25 840;Outdoor luminaires;19.3172.0004.25;145 x 260;surface mounted on ceiling or on wall;9.8;1010;103;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 7016 (anthracite, metallic, fine structure);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0004.25/;19.3172.0004.25_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1000 FLOOD E PIR IP65 34 830;Outdoor luminaires;19.3172.0003.34;145 x 260;surface mounted on ceiling or on wall;9.8;983;100;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0003.34/;19.3172.0003.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1000 FLOOD E PIR IP65 34 840;Outdoor luminaires;19.3172.0004.34;145 x 260;surface mounted on ceiling or on wall;9.8;1010;103;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;88000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;3;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0004.34/;19.3172.0004.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E IP65 04 830;Outdoor luminaires;19.3172.0005.04;145 x 260;surface mounted on ceiling or on wall;12.8;1521;119;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0005.04/;19.3172.0005.04_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E IP65 04 840;Outdoor luminaires;19.3172.0006.04;145 x 260;surface mounted on ceiling or on wall;12.8;1565;122;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0006.04/;19.3172.0006.04_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E IP65 21 830;Outdoor luminaires;19.3172.0005.21;145 x 260;surface mounted on ceiling or on wall;12.8;1521;119;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0005.21/;19.3172.0005.21_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E IP65 21 840;Outdoor luminaires;19.3172.0006.21;145 x 260;surface mounted on ceiling or on wall;12.8;1565;122;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0006.21/;19.3172.0006.21_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E IP65 22 830;Outdoor luminaires;19.3172.0005.22;145 x 260;surface mounted on ceiling or on wall;12.8;1521;119;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9007 (dark gray);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0005.22/;19.3172.0005.22_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E IP65 22 840;Outdoor luminaires;19.3172.0006.22;145 x 260;surface mounted on ceiling or on wall;12.8;1565;122;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9007 (dark gray);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0006.22/;19.3172.0006.22_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E IP65 25 830;Outdoor luminaires;19.3172.0005.25;145 x 260;surface mounted on ceiling or on wall;12.8;1521;119;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 7016 (anthracite, metallic, fine structure);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0005.25/;19.3172.0005.25_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E IP65 25 840;Outdoor luminaires;19.3172.0006.25;145 x 260;surface mounted on ceiling or on wall;12.8;1565;122;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 7016 (anthracite, metallic, fine structure);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0006.25/;19.3172.0006.25_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E IP65 34 830;Outdoor luminaires;19.3172.0005.34;145 x 260;surface mounted on ceiling or on wall;12.8;1521;119;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0005.34/;19.3172.0005.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E IP65 34 840;Outdoor luminaires;19.3172.0006.34;145 x 260;surface mounted on ceiling or on wall;12.8;1565;122;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0006.34/;19.3172.0006.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E PIR IP65 04 830;Outdoor luminaires;19.3172.0007.04;145 x 260;surface mounted on ceiling or on wall;12.8;1521;119;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0007.04/;19.3172.0007.04_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E PIR IP65 04 840;Outdoor luminaires;19.3172.0008.04;145 x 260;surface mounted on ceiling or on wall;12.8;1565;122;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0008.04/;19.3172.0008.04_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E PIR IP65 21 830;Outdoor luminaires;19.3172.0007.21;145 x 260;surface mounted on ceiling or on wall;12.8;1521;119;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0007.21/;19.3172.0007.21_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E PIR IP65 21 840;Outdoor luminaires;19.3172.0008.21;145 x 260;surface mounted on ceiling or on wall;12.8;1565;122;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0008.21/;19.3172.0008.21_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E PIR IP65 22 830;Outdoor luminaires;19.3172.0007.22;145 x 260;surface mounted on ceiling or on wall;12.8;1521;119;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9007 (dark gray);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0007.22/;19.3172.0007.22_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E PIR IP65 22 840;Outdoor luminaires;19.3172.0008.22;145 x 260;surface mounted on ceiling or on wall;12.8;1565;122;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9007 (dark gray);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0008.22/;19.3172.0008.22_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E PIR IP65 25 830;Outdoor luminaires;19.3172.0007.25;145 x 260;surface mounted on ceiling or on wall;12.8;1521;119;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 7016 (anthracite, metallic, fine structure);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0007.25/;19.3172.0007.25_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E PIR IP65 25 840;Outdoor luminaires;19.3172.0008.25;145 x 260;surface mounted on ceiling or on wall;12.8;1565;122;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 7016 (anthracite, metallic, fine structure);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0008.25/;19.3172.0008.25_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E PIR IP65 34 830;Outdoor luminaires;19.3172.0007.34;145 x 260;surface mounted on ceiling or on wall;12.8;1521;119;3000;3000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0007.34/;19.3172.0007.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ROLLER LED 1800 FLOOD E PIR IP65 34 840;Outdoor luminaires;19.3172.0008.34;145 x 260;surface mounted on ceiling or on wall;12.8;1565;122;4000;4000;0.7606;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PC (opalescent polycarbonate);LED;-25 ÷ 30;83000 (1) / 100000 (2) / 100000 (3);L90/B10 (1) / L80/B10 (2) / L70/B10 (3);85;2;(C0-C180) / (C90-C270) - 95° / 92,8°;IP65;IK02;I;0;0.9;260;145;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/roller-led/19.3172.0008.34/;19.3172.0008.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
