;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
TEAR LED 2000 NARROW E 04 3F 830;Projectors;19.3068.0005.04;?130 x 312;mounted on a three-phase track;23;1934;84;3000;3000;0.8281;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_transparent glass;LED;5 ÷ 30;68000;L90/B10;>80;2;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0005.04/;19.3068.0005.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 2000 NARROW E 34 3F 830;Projectors;19.3068.0005.34;?130 x 312;mounted on a three-phase track;23;1934;84;3000;3000;0.8281;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent glass;LED;5 ÷ 30;68000;L90/B10;>80;2;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0005.34/;19.3068.0005.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 2000 NARROW E 34 3F 840;Projectors;19.3068.0006.34;?130 x 312;mounted on a three-phase track;23;2012;87;4000;4000;0.8281;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent glass;LED;5 ÷ 30;68000;L90/B10;>80;2;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0006.34/;19.3068.0006.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 2000 NARROW EDD 04 3F 830;Projectors;19.3068.0007.04;?130 x 312;mounted on a three-phase track;23;1934;84;3000;3000;0.8281;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_transparent glass;LED;5 ÷ 30;68000;L90/B10;>80;2;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0007.04/;19.3068.0007.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 2000 NARROW EDD 04 3F 840;Projectors;19.3068.0008.04;?130 x 312;mounted on a three-phase track;23;2012;87;4000;4000;0.8281;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_transparent glass;LED;5 ÷ 30;68000;L90/B10;>80;2;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0008.04/;19.3068.0008.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 2000 NARROW EDD 34 3F 830;Projectors;19.3068.0007.34;?130 x 312;mounted on a three-phase track;23;1934;84;3000;3000;0.8281;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent glass;LED;5 ÷ 30;68000;L90/B10;>80;2;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0007.34/;19.3068.0007.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 2000 NARROW EDD 34 3F 840;Projectors;19.3068.0008.34;?130 x 312;mounted on a three-phase track;23;2012;87;4000;4000;0.8281;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent glass;LED;5 ÷ 30;68000;L90/B10;>80;2;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0008.34/;19.3068.0008.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 3000 NARROW E 04 3F 830;Projectors;19.3068.0013.04;?130 x 312;mounted on a three-phase track;28;3031;108;3000;3000;0.8281;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_transparent glass;LED;5 ÷ 30;84000;L90/B10;>80;2;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0013.04/;19.3068.0013.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 3000 NARROW E 04 3F 840;Projectors;19.3068.0014.04;?130 x 312;mounted on a three-phase track;28;3209;115;4000;4000;0.8281;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_transparent glass;LED;5 ÷ 30;76000;L90/B10;>80;2;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0014.04/;19.3068.0014.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 3000 NARROW E 34 3F 830;Projectors;19.3068.0013.34;?130 x 312;mounted on a three-phase track;28;3031;108;3000;3000;0.8281;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent glass;LED;5 ÷ 30;84000;L90/B10;>80;2;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0013.34/;19.3068.0013.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 3000 NARROW E 34 3F 840;Projectors;19.3068.0014.34;?130 x 312;mounted on a three-phase track;28;3209;115;4000;4000;0.8281;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent glass;LED;5 ÷ 30;76000;L90/B10;>80;2;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0014.34/;19.3068.0014.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 3000 NARROW EDD 04 3F 830;Projectors;19.3068.0015.04;?130 x 312;mounted on a three-phase track;28;3031;108;3000;3000;0.8281;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_transparent glass;LED;5 ÷ 30;84000;L90/B10;>80;2;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0015.04/;19.3068.0015.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 3000 NARROW EDD 04 3F 840;Projectors;19.3068.0016.04;?130 x 312;mounted on a three-phase track;28;3209;115;4000;4000;0.8281;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_transparent glass;LED;5 ÷ 30;76000;L90/B10;>80;2;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0016.04/;19.3068.0016.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 3000 NARROW EDD 34 3F 830;Projectors;19.3068.0015.34;?130 x 312;mounted on a three-phase track;28;3031;108;3000;3000;0.8281;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent glass;LED;5 ÷ 30;84000;L90/B10;>80;2;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0015.34/;19.3068.0015.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 3000 NARROW EDD 34 3F 840;Projectors;19.3068.0016.34;?130 x 312;mounted on a three-phase track;28;3209;115;4000;4000;0.8281;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent glass;LED;5 ÷ 30;76000;L90/B10;>80;2;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0016.34/;19.3068.0016.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 5000 NARROW E 04 3F 830;Projectors;19.3068.0021.04;?130 x 312;mounted on a three-phase track;42;4579;109;3000;3000;0.8281;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_transparent glass;LED;5 ÷ 30;83000;L90/B10;>80;2;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0021.04/;19.3068.0021.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 5000 NARROW E 04 3F 840;Projectors;19.3068.0022.04;?130 x 312;mounted on a three-phase track;41;4899;119;4000;4000;0.8281;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_transparent glass;LED;5 ÷ 30;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0022.04/;19.3068.0022.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 5000 NARROW E 34 3F 830;Projectors;19.3068.0021.34;?130 x 312;mounted on a three-phase track;42;4579;109;3000;3000;0.8281;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent glass;LED;5 ÷ 30;83000;L90/B10;>80;2;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0021.34/;19.3068.0021.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 5000 NARROW E 34 3F 840;Projectors;19.3068.0022.34;?130 x 312;mounted on a three-phase track;41;4899;119;4000;4000;0.8281;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent glass;LED;5 ÷ 30;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0022.34/;19.3068.0022.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 5000 NARROW EDD 04 3F 830;Projectors;19.3068.0023.04;?130 x 312;mounted on a three-phase track;42;4579;109;3000;3000;0.8281;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_transparent glass;LED;5 ÷ 30;83000;L90/B10;>80;2;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0023.04/;19.3068.0023.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 5000 NARROW EDD 04 3F 840;Projectors;19.3068.0024.04;?130 x 312;mounted on a three-phase track;41;4899;119;4000;4000;0.8281;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_transparent glass;LED;5 ÷ 30;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0024.04/;19.3068.0024.04.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 5000 NARROW EDD 34 3F 830;Projectors;19.3068.0023.34;?130 x 312;mounted on a three-phase track;42;4579;109;3000;3000;0.8281;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent glass;LED;5 ÷ 30;83000;L90/B10;>80;2;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0023.34/;19.3068.0023.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
TEAR LED 5000 NARROW EDD 34 3F 840;Projectors;19.3068.0024.34;?130 x 312;mounted on a three-phase track;42;4579;109;4000;4000;0.8281;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_transparent glass;LED;5 ÷ 30;83000;L90/B10;>80;3;(C0-C180) / (C90-C270) - 32,6° / 32,6°;IP20;IK04;I;RG1;0.95;312;130;https://luxiona.pl/oferta/projektory/tear-led-3f/;https://luxiona.pl/oferta/projektory/tear-led-3f/19.3068.0024.34/;19.3068.0024.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
