;Assembly Code##OTHER##;Assembly##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Dimensions##OTHER##;Voltage (range)##OTHER##;Driver##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Power of luminaire##ELECTRICAL_WATTAGE##WATTS;Luminaire luminous flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Luminaire's light efficiency##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;Color of the light##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Efficiency##OTHER##;Power factor##OTHER##;Manufacturer##OTHER##;URL##OTHER##;Catalogue##OTHER## ;Photometric Web File##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN
X-LINE SLIGHT L-DOWN LED 1300 MICRO-PRM E 04 830 / L-572MM S-1,5M;19.4085.5111.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.6;1144;133;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5111.04-en-x-line-slight-l-down-led-1300-micro-prm-e-04-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-MICRO-PRM-E-04-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 1300 MICRO-PRM E 04 840 / L-572MM S-1,5M;19.4085.5121.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.6;1229.7;143;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5121.04-en-x-line-slight-l-down-led-1300-micro-prm-e-04-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-MICRO-PRM-E-04-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 1300 MICRO-PRM E 21 830 / L-572MM S-1,5M;19.4085.5111.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.6;1144;133;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5111.21-en-x-line-slight-l-down-led-1300-micro-prm-e-21-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-MICRO-PRM-E-21-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 1300 MICRO-PRM E 21 840 / L-572MM S-1,5M;19.4085.5121.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.6;1229.7;143;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5121.21-en-x-line-slight-l-down-led-1300-micro-prm-e-21-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-MICRO-PRM-E-21-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 1300 MICRO-PRM E 24 830 / L-572MM S-1,5M;19.4085.5111.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.6;1144;133;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5111.24-en-x-line-slight-l-down-led-1300-micro-prm-e-24-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-MICRO-PRM-E-24-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 1300 MICRO-PRM E 24 840 / L-572MM S-1,5M;19.4085.5121.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.6;1229.7;143;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5121.24-en-x-line-slight-l-down-led-1300-micro-prm-e-24-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-MICRO-PRM-E-24-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 1300 MICRO-PRM E 34 830 / L-572MM S-1,5M;19.4085.5111.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.6;1144;133;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5111.34-en-x-line-slight-l-down-led-1300-micro-prm-e-34-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-MICRO-PRM-E-34-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 1300 MICRO-PRM E 34 840 / L-572MM S-1,5M;19.4085.5121.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.6;1229.7;143;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5121.34-en-x-line-slight-l-down-led-1300-micro-prm-e-34-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-MICRO-PRM-E-34-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 1300 MICRO-PRM EDD 04 830 / L-572MM S-1,5M;19.4085.5113.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.6;1144;133;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5113.04-en-x-line-slight-l-down-led-1300-micro-prm-edd-04-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-MICRO-PRM-EDD-04-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 1300 MICRO-PRM EDD 04 840 / L-572MM S-1,5M;19.4085.5123.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.6;1229.7;143;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5123.04-en-x-line-slight-l-down-led-1300-micro-prm-edd-04-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-MICRO-PRM-EDD-04-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 1300 MICRO-PRM EDD 21 830 / L-572MM S-1,5M;19.4085.5113.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.6;1144;133;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5113.21-en-x-line-slight-l-down-led-1300-micro-prm-edd-21-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-MICRO-PRM-EDD-21-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 1300 MICRO-PRM EDD 21 840 / L-572MM S-1,5M;19.4085.5123.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.6;1229.7;143;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5123.21-en-x-line-slight-l-down-led-1300-micro-prm-edd-21-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-MICRO-PRM-EDD-21-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 1300 MICRO-PRM EDD 24 830 / L-572MM S-1,5M;19.4085.5113.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.6;1144;133;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5113.24-en-x-line-slight-l-down-led-1300-micro-prm-edd-24-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-MICRO-PRM-EDD-24-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 1300 MICRO-PRM EDD 24 840 / L-572MM S-1,5M;19.4085.5123.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.6;1229.7;143;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5123.24-en-x-line-slight-l-down-led-1300-micro-prm-edd-24-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-MICRO-PRM-EDD-24-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 1300 MICRO-PRM EDD 34 830 / L-572MM S-1,5M;19.4085.5113.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.6;1144;133;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5113.34-en-x-line-slight-l-down-led-1300-micro-prm-edd-34-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-MICRO-PRM-EDD-34-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 1300 MICRO-PRM EDD 34 840 / L-572MM S-1,5M;19.4085.5123.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.6;1229.7;143;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5123.34-en-x-line-slight-l-down-led-1300-micro-prm-edd-34-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-MICRO-PRM-EDD-34-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 1300 PLX E 04 830 / L-572MM S-1,5M;19.4085.1111.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.6;1052.8;122.4;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1111.04-en-x-line-slight-l-down-led-1300-plx-e-04-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-PLX-E-04-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 1300 PLX E 04 840 / L-572MM S-1,5M;19.4085.1121.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.6;1131.7;131.6;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1121.04-en-x-line-slight-l-down-led-1300-plx-e-04-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-PLX-E-04-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 1300 PLX E 21 830 / L-572MM S-1,5M;19.4085.1111.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.6;1052.8;122.4;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1111.21-en-x-line-slight-l-down-led-1300-plx-e-21-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-PLX-E-21-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 1300 PLX E 21 840 / L-572MM S-1,5M;19.4085.1121.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.6;1131.7;131.6;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1121.21-en-x-line-slight-l-down-led-1300-plx-e-21-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-PLX-E-21-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 1300 PLX E 24 830 / L-572MM S-1,5M;19.4085.1111.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.6;1052.8;122.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1111.24-en-x-line-slight-l-down-led-1300-plx-e-24-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-PLX-E-24-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 1300 PLX E 24 840 / L-572MM S-1,5M;19.4085.1121.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.6;1131.7;131.6;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1121.24-en-x-line-slight-l-down-led-1300-plx-e-24-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-PLX-E-24-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 1300 PLX E 34 830 / L-572MM S-1,5M;19.4085.1111.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.6;1052.8;122.4;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1111.34-en-x-line-slight-l-down-led-1300-plx-e-34-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-PLX-E-34-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 1300 PLX E 34 840 / L-572MM S-1,5M;19.4085.1121.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.6;1131.7;131.6;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1121.34-en-x-line-slight-l-down-led-1300-plx-e-34-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-PLX-E-34-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 1300 PLX EDD 04 830 / L-572MM S-1,5M;19.4085.1113.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.6;1052.8;122.4;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1113.04-en-x-line-slight-l-down-led-1300-plx-edd-04-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-PLX-EDD-04-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 1300 PLX EDD 04 840 / L-572MM S-1,5M;19.4085.1123.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.6;1131.7;131.6;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1123.04-en-x-line-slight-l-down-led-1300-plx-edd-04-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-PLX-EDD-04-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 1300 PLX EDD 21 830 / L-572MM S-1,5M;19.4085.1113.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.6;1052.8;122.4;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1113.21-en-x-line-slight-l-down-led-1300-plx-edd-21-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-PLX-EDD-21-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 1300 PLX EDD 21 840 / L-572MM S-1,5M;19.4085.1123.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.6;1131.7;131.6;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1123.21-en-x-line-slight-l-down-led-1300-plx-edd-21-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-PLX-EDD-21-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 1300 PLX EDD 24 830 / L-572MM S-1,5M;19.4085.1113.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.6;1052.8;122.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1113.24-en-x-line-slight-l-down-led-1300-plx-edd-24-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-PLX-EDD-24-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 1300 PLX EDD 24 840 / L-572MM S-1,5M;19.4085.1123.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.6;1131.7;131.6;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1123.24-en-x-line-slight-l-down-led-1300-plx-edd-24-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-PLX-EDD-24-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 1300 PLX EDD 34 830 / L-572MM S-1,5M;19.4085.1113.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.6;1052.8;122.4;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1113.34-en-x-line-slight-l-down-led-1300-plx-edd-34-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-PLX-EDD-34-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 1300 PLX EDD 34 840 / L-572MM S-1,5M;19.4085.1123.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.6;1131.7;131.6;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1123.34-en-x-line-slight-l-down-led-1300-plx-edd-34-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-1300-PLX-EDD-34-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2200 MICRO-PRM E 04 830 / L-572MM S-1,5M;19.4085.5211.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.4;1815.9;135.5;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5211.04-en-x-line-slight-l-down-led-2200-micro-prm-e-04-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-MICRO-PRM-E-04-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2200 MICRO-PRM E 04 840 / L-572MM S-1,5M;19.4085.5221.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.4;1952;145.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5221.04-en-x-line-slight-l-down-led-2200-micro-prm-e-04-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-MICRO-PRM-E-04-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2200 MICRO-PRM E 21 830 / L-572MM S-1,5M;19.4085.5211.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.4;1815.9;135.5;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5211.21-en-x-line-slight-l-down-led-2200-micro-prm-e-21-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-MICRO-PRM-E-21-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2200 MICRO-PRM E 21 840 / L-572MM S-1,5M;19.4085.5221.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.4;1952;145.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5221.21-en-x-line-slight-l-down-led-2200-micro-prm-e-21-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-MICRO-PRM-E-21-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2200 MICRO-PRM E 24 830 / L-572MM S-1,5M;19.4085.5211.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.4;1815.9;135.5;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5211.24-en-x-line-slight-l-down-led-2200-micro-prm-e-24-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-MICRO-PRM-E-24-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2200 MICRO-PRM E 24 840 / L-572MM S-1,5M;19.4085.5221.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.4;1952;145.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5221.24-en-x-line-slight-l-down-led-2200-micro-prm-e-24-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-MICRO-PRM-E-24-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2200 MICRO-PRM E 34 830 / L-572MM S-1,5M;19.4085.5211.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.4;1815.9;135.5;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5211.34-en-x-line-slight-l-down-led-2200-micro-prm-e-34-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-MICRO-PRM-E-34-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2200 MICRO-PRM E 34 840 / L-572MM S-1,5M;19.4085.5221.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.4;1952;145.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5221.34-en-x-line-slight-l-down-led-2200-micro-prm-e-34-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-MICRO-PRM-E-34-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2200 MICRO-PRM EDD 04 830 / L-572MM S-1,5M;19.4085.5213.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.4;1815.9;135.5;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5213.04-en-x-line-slight-l-down-led-2200-micro-prm-edd-04-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-MICRO-PRM-EDD-04-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2200 MICRO-PRM EDD 04 840 / L-572MM S-1,5M;19.4085.5223.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.4;1952;145.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5223.04-en-x-line-slight-l-down-led-2200-micro-prm-edd-04-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-MICRO-PRM-EDD-04-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2200 MICRO-PRM EDD 21 830 / L-572MM S-1,5M;19.4085.5213.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.4;1815.9;135.5;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5213.21-en-x-line-slight-l-down-led-2200-micro-prm-edd-21-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-MICRO-PRM-EDD-21-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2200 MICRO-PRM EDD 21 840 / L-572MM S-1,5M;19.4085.5223.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.4;1952;145.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5223.21-en-x-line-slight-l-down-led-2200-micro-prm-edd-21-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-MICRO-PRM-EDD-21-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2200 MICRO-PRM EDD 24 830 / L-572MM S-1,5M;19.4085.5213.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.4;1815.9;135.5;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5213.24-en-x-line-slight-l-down-led-2200-micro-prm-edd-24-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-MICRO-PRM-EDD-24-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2200 MICRO-PRM EDD 24 840 / L-572MM S-1,5M;19.4085.5223.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.4;1952;145.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5223.24-en-x-line-slight-l-down-led-2200-micro-prm-edd-24-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-MICRO-PRM-EDD-24-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2200 MICRO-PRM EDD 34 830 / L-572MM S-1,5M;19.4085.5213.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.4;1815.9;135.5;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5213.34-en-x-line-slight-l-down-led-2200-micro-prm-edd-34-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-MICRO-PRM-EDD-34-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2200 MICRO-PRM EDD 34 840 / L-572MM S-1,5M;19.4085.5223.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.4;1952;145.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.5223.34-en-x-line-slight-l-down-led-2200-micro-prm-edd-34-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-MICRO-PRM-EDD-34-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2200 PLX E 04 830 / L-572MM S-1,5M;19.4085.1211.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.4;1671.1;124.7;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1211.04-en-x-line-slight-l-down-led-2200-plx-e-04-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-PLX-E-04-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2200 PLX E 04 840 / L-572MM S-1,5M;19.4085.1221.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.4;1796.3;134.1;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1221.04-en-x-line-slight-l-down-led-2200-plx-e-04-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-PLX-E-04-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2200 PLX E 21 830 / L-572MM S-1,5M;19.4085.1211.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.4;1671.1;124.7;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1211.21-en-x-line-slight-l-down-led-2200-plx-e-21-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-PLX-E-21-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2200 PLX E 21 840 / L-572MM S-1,5M;19.4085.1221.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.4;1796.3;134.1;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1221.21-en-x-line-slight-l-down-led-2200-plx-e-21-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-PLX-E-21-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2200 PLX E 24 830 / L-572MM S-1,5M;19.4085.1211.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.4;1671.1;124.7;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1211.24-en-x-line-slight-l-down-led-2200-plx-e-24-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-PLX-E-24-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2200 PLX E 24 840 / L-572MM S-1,5M;19.4085.1221.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.4;1796.3;134.1;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1221.24-en-x-line-slight-l-down-led-2200-plx-e-24-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-PLX-E-24-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2200 PLX E 34 830 / L-572MM S-1,5M;19.4085.1211.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.4;1671.1;124.7;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1211.34-en-x-line-slight-l-down-led-2200-plx-e-34-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-PLX-E-34-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2200 PLX E 34 840 / L-572MM S-1,5M;19.4085.1221.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.4;1796.3;134.1;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1221.34-en-x-line-slight-l-down-led-2200-plx-e-34-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-PLX-E-34-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2200 PLX EDD 04 830 / L-572MM S-1,5M;19.4085.1213.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.4;1671.1;124.7;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1213.04-en-x-line-slight-l-down-led-2200-plx-edd-04-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-PLX-EDD-04-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2200 PLX EDD 04 840 / L-572MM S-1,5M;19.4085.1223.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.4;1796.3;134.1;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1223.04-en-x-line-slight-l-down-led-2200-plx-edd-04-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-PLX-EDD-04-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2200 PLX EDD 21 830 / L-572MM S-1,5M;19.4085.1213.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.4;1671.1;124.7;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1213.21-en-x-line-slight-l-down-led-2200-plx-edd-21-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-PLX-EDD-21-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2200 PLX EDD 21 840 / L-572MM S-1,5M;19.4085.1223.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.4;1796.3;134.1;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1223.21-en-x-line-slight-l-down-led-2200-plx-edd-21-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-PLX-EDD-21-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2200 PLX EDD 24 830 / L-572MM S-1,5M;19.4085.1213.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.4;1671.1;124.7;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1213.24-en-x-line-slight-l-down-led-2200-plx-edd-24-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-PLX-EDD-24-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2200 PLX EDD 24 840 / L-572MM S-1,5M;19.4085.1223.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.4;1796.3;134.1;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1223.24-en-x-line-slight-l-down-led-2200-plx-edd-24-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-PLX-EDD-24-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2200 PLX EDD 34 830 / L-572MM S-1,5M;19.4085.1213.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.4;1671.1;124.7;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1213.34-en-x-line-slight-l-down-led-2200-plx-edd-34-830-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-PLX-EDD-34-830-L-572MM-S-15M.ies;572;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2200 PLX EDD 34 840 / L-572MM S-1,5M;19.4085.1223.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);572 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.4;1796.3;134.1;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.1223.34-en-x-line-slight-l-down-led-2200-plx-edd-34-840-l-572mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2200-PLX-EDD-34-840-L-572MM-S-15M.ies;572;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2600 MICRO-PRM E 04 830 / L-1134MM S-1,5M;19.4085.6311.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;15.7;2288.5;145.8;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6311.04-en-x-line-slight-l-down-led-2600-micro-prm-e-04-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-MICRO-PRM-E-04-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2600 MICRO-PRM E 04 840 / L-1134MM S-1,5M;19.4085.6321.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;15.7;2459.7;156.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6321.04-en-x-line-slight-l-down-led-2600-micro-prm-e-04-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-MICRO-PRM-E-04-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2600 MICRO-PRM E 21 830 / L-1134MM S-1,5M;19.4085.6311.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;15.7;2288.5;145.8;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6311.21-en-x-line-slight-l-down-led-2600-micro-prm-e-21-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-MICRO-PRM-E-21-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2600 MICRO-PRM E 21 840 / L-1134MM S-1,5M;19.4085.6321.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;15.7;2459.7;156.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6321.21-en-x-line-slight-l-down-led-2600-micro-prm-e-21-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-MICRO-PRM-E-21-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2600 MICRO-PRM E 24 830 / L-1134MM S-1,5M;19.4085.6311.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;15.7;2288.5;145.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6311.24-en-x-line-slight-l-down-led-2600-micro-prm-e-24-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-MICRO-PRM-E-24-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2600 MICRO-PRM E 24 840 / L-1134MM S-1,5M;19.4085.6321.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;15.7;2459.7;156.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6321.24-en-x-line-slight-l-down-led-2600-micro-prm-e-24-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-MICRO-PRM-E-24-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2600 MICRO-PRM E 34 830 / L-1134MM S-1,5M;19.4085.6311.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;15.7;2288.5;145.8;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6311.34-en-x-line-slight-l-down-led-2600-micro-prm-e-34-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-MICRO-PRM-E-34-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2600 MICRO-PRM E 34 840 / L-1134MM S-1,5M;19.4085.6321.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;15.7;2459.7;156.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6321.34-en-x-line-slight-l-down-led-2600-micro-prm-e-34-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-MICRO-PRM-E-34-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2600 MICRO-PRM EDD 04 830 / L-1134MM S-1,5M;19.4085.6313.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;15.7;2288.5;145.8;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6313.04-en-x-line-slight-l-down-led-2600-micro-prm-edd-04-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-MICRO-PRM-EDD-04-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2600 MICRO-PRM EDD 04 840 / L-1134MM S-1,5M;19.4085.6323.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;15.7;2459.7;156.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6323.04-en-x-line-slight-l-down-led-2600-micro-prm-edd-04-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-MICRO-PRM-EDD-04-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2600 MICRO-PRM EDD 21 830 / L-1134MM S-1,5M;19.4085.6313.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;15.7;2288.5;145.8;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6313.21-en-x-line-slight-l-down-led-2600-micro-prm-edd-21-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-MICRO-PRM-EDD-21-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2600 MICRO-PRM EDD 21 840 / L-1134MM S-1,5M;19.4085.6323.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;15.7;2459.7;156.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6323.21-en-x-line-slight-l-down-led-2600-micro-prm-edd-21-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-MICRO-PRM-EDD-21-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2600 MICRO-PRM EDD 24 830 / L-1134MM S-1,5M;19.4085.6313.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;15.7;2288.5;145.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6313.24-en-x-line-slight-l-down-led-2600-micro-prm-edd-24-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-MICRO-PRM-EDD-24-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2600 MICRO-PRM EDD 24 840 / L-1134MM S-1,5M;19.4085.6323.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;15.7;2459.7;156.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6323.24-en-x-line-slight-l-down-led-2600-micro-prm-edd-24-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-MICRO-PRM-EDD-24-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2600 MICRO-PRM EDD 34 830 / L-1134MM S-1,5M;19.4085.6313.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;15.7;2288.5;145.8;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6313.34-en-x-line-slight-l-down-led-2600-micro-prm-edd-34-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-MICRO-PRM-EDD-34-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2600 MICRO-PRM EDD 34 840 / L-1134MM S-1,5M;19.4085.6323.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;15.7;2459.7;156.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6323.34-en-x-line-slight-l-down-led-2600-micro-prm-edd-34-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-MICRO-PRM-EDD-34-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2600 PLX E 04 830 / L-1134MM S-1,5M;19.4085.2311.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;15.7;2106;134.1;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2311.04-en-x-line-slight-l-down-led-2600-plx-e-04-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-PLX-E-04-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2600 PLX E 04 840 / L-1134MM S-1,5M;19.4085.2321.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;15.7;2263.5;144.2;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2321.04-en-x-line-slight-l-down-led-2600-plx-e-04-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-PLX-E-04-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2600 PLX E 21 830 / L-1134MM S-1,5M;19.4085.2311.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;15.7;2106;134.1;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2311.21-en-x-line-slight-l-down-led-2600-plx-e-21-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-PLX-E-21-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2600 PLX E 21 840 / L-1134MM S-1,5M;19.4085.2321.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;15.7;2263.5;144.2;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2321.21-en-x-line-slight-l-down-led-2600-plx-e-21-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-PLX-E-21-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2600 PLX E 24 830 / L-1134MM S-1,5M;19.4085.2311.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;15.7;2106;134.1;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2311.24-en-x-line-slight-l-down-led-2600-plx-e-24-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-PLX-E-24-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2600 PLX E 24 840 / L-1134MM S-1,5M;19.4085.2321.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;15.7;2263.5;144.2;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2321.24-en-x-line-slight-l-down-led-2600-plx-e-24-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-PLX-E-24-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2600 PLX E 34 830 / L-1134MM S-1,5M;19.4085.2311.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;15.7;2106;134.1;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2311.34-en-x-line-slight-l-down-led-2600-plx-e-34-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-PLX-E-34-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2600 PLX E 34 840 / L-1134MM S-1,5M;19.4085.2321.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;15.7;2263.5;144.2;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2321.34-en-x-line-slight-l-down-led-2600-plx-e-34-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-PLX-E-34-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2600 PLX EDD 04 830 / L-1134MM S-1,5M;19.4085.2313.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;15.7;2106;134.1;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2313.04-en-x-line-slight-l-down-led-2600-plx-edd-04-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-PLX-EDD-04-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2600 PLX EDD 04 840 / L-1134MM S-1,5M;19.4085.2323.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;15.7;2263.5;144.2;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2323.04-en-x-line-slight-l-down-led-2600-plx-edd-04-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-PLX-EDD-04-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2600 PLX EDD 21 830 / L-1134MM S-1,5M;19.4085.2313.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;15.7;2106;134.1;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2313.21-en-x-line-slight-l-down-led-2600-plx-edd-21-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-PLX-EDD-21-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2600 PLX EDD 21 840 / L-1134MM S-1,5M;19.4085.2323.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;15.7;2263.5;144.2;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2323.21-en-x-line-slight-l-down-led-2600-plx-edd-21-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-PLX-EDD-21-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2600 PLX EDD 24 830 / L-1134MM S-1,5M;19.4085.2313.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;15.7;2106;134.1;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2313.24-en-x-line-slight-l-down-led-2600-plx-edd-24-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-PLX-EDD-24-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2600 PLX EDD 24 840 / L-1134MM S-1,5M;19.4085.2323.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;15.7;2263.5;144.2;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2323.24-en-x-line-slight-l-down-led-2600-plx-edd-24-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-PLX-EDD-24-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 2600 PLX EDD 34 830 / L-1134MM S-1,5M;19.4085.2313.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;15.7;2106;134.1;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2313.34-en-x-line-slight-l-down-led-2600-plx-edd-34-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-PLX-EDD-34-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 2600 PLX EDD 34 840 / L-1134MM S-1,5M;19.4085.2323.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;15.7;2263.5;144.2;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2323.34-en-x-line-slight-l-down-led-2600-plx-edd-34-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-2600-PLX-EDD-34-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 3900 MICRO-PRM E 04 830 / L-1693MM S-1,5M;19.4085.7511.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;23.5;3432.8;146.1;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7511.04-en-x-line-slight-l-down-led-3900-micro-prm-e-04-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-MICRO-PRM-E-04-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 3900 MICRO-PRM E 04 840 / L-1693MM S-1,5M;19.4085.7521.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;23.5;3689.5;157;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7521.04-en-x-line-slight-l-down-led-3900-micro-prm-e-04-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-MICRO-PRM-E-04-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 3900 MICRO-PRM E 21 830 / L-1693MM S-1,5M;19.4085.7511.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;23.5;3432.8;146.1;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7511.21-en-x-line-slight-l-down-led-3900-micro-prm-e-21-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-MICRO-PRM-E-21-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 3900 MICRO-PRM E 21 840 / L-1693MM S-1,5M;19.4085.7521.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;23.5;3689.5;157;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7521.21-en-x-line-slight-l-down-led-3900-micro-prm-e-21-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-MICRO-PRM-E-21-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 3900 MICRO-PRM E 24 830 / L-1693MM S-1,5M;19.4085.7511.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;23.5;3432.8;146.1;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7511.24-en-x-line-slight-l-down-led-3900-micro-prm-e-24-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-MICRO-PRM-E-24-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 3900 MICRO-PRM E 24 840 / L-1693MM S-1,5M;19.4085.7521.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;23.5;3689.5;157;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7521.24-en-x-line-slight-l-down-led-3900-micro-prm-e-24-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-MICRO-PRM-E-24-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 3900 MICRO-PRM E 34 830 / L-1693MM S-1,5M;19.4085.7511.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;23.5;3432.8;146.1;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7511.34-en-x-line-slight-l-down-led-3900-micro-prm-e-34-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-MICRO-PRM-E-34-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 3900 MICRO-PRM E 34 840 / L-1693MM S-1,5M;19.4085.7521.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;23.5;3689.5;157;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7521.34-en-x-line-slight-l-down-led-3900-micro-prm-e-34-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-MICRO-PRM-E-34-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 3900 MICRO-PRM EDD 04 830 / L-1693MM S-1,5M;19.4085.7513.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;23.5;3432.8;146.1;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7513.04-en-x-line-slight-l-down-led-3900-micro-prm-edd-04-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-MICRO-PRM-EDD-04-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 3900 MICRO-PRM EDD 04 840 / L-1693MM S-1,5M;19.4085.7523.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;23.5;3689.5;157;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7523.04-en-x-line-slight-l-down-led-3900-micro-prm-edd-04-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-MICRO-PRM-EDD-04-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 3900 MICRO-PRM EDD 21 830 / L-1693MM S-1,5M;19.4085.7513.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;23.5;3432.8;146.1;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7513.21-en-x-line-slight-l-down-led-3900-micro-prm-edd-21-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-MICRO-PRM-EDD-21-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 3900 MICRO-PRM EDD 21 840 / L-1693MM S-1,5M;19.4085.7523.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;23.5;3689.5;157;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7523.21-en-x-line-slight-l-down-led-3900-micro-prm-edd-21-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-MICRO-PRM-EDD-21-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 3900 MICRO-PRM EDD 24 830 / L-1693MM S-1,5M;19.4085.7513.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;23.5;3432.8;146.1;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7513.24-en-x-line-slight-l-down-led-3900-micro-prm-edd-24-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-MICRO-PRM-EDD-24-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 3900 MICRO-PRM EDD 24 840 / L-1693MM S-1,5M;19.4085.7523.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;23.5;3689.5;157;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7523.24-en-x-line-slight-l-down-led-3900-micro-prm-edd-24-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-MICRO-PRM-EDD-24-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 3900 MICRO-PRM EDD 34 830 / L-1693MM S-1,5M;19.4085.7513.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;23.5;3432.8;146.1;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7513.34-en-x-line-slight-l-down-led-3900-micro-prm-edd-34-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-MICRO-PRM-EDD-34-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 3900 MICRO-PRM EDD 34 840 / L-1693MM S-1,5M;19.4085.7523.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;23.5;3689.5;157;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7523.34-en-x-line-slight-l-down-led-3900-micro-prm-edd-34-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-MICRO-PRM-EDD-34-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 3900 PLX E 04 830 / L-1693MM S-1,5M;19.4085.3511.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;23.5;3159;134.4;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3511.04-en-x-line-slight-l-down-led-3900-plx-e-04-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-PLX-E-04-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 3900 PLX E 04 840 / L-1693MM S-1,5M;19.4085.3521.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;23.5;3395.3;144.5;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3521.04-en-x-line-slight-l-down-led-3900-plx-e-04-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-PLX-E-04-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 3900 PLX E 21 830 / L-1693MM S-1,5M;19.4085.3511.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;23.5;3159;134.4;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3511.21-en-x-line-slight-l-down-led-3900-plx-e-21-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-PLX-E-21-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 3900 PLX E 21 840 / L-1693MM S-1,5M;19.4085.3521.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;23.5;3395.3;144.5;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3521.21-en-x-line-slight-l-down-led-3900-plx-e-21-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-PLX-E-21-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 3900 PLX E 24 830 / L-1693MM S-1,5M;19.4085.3511.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;23.5;3159;134.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3511.24-en-x-line-slight-l-down-led-3900-plx-e-24-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-PLX-E-24-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 3900 PLX E 24 840 / L-1693MM S-1,5M;19.4085.3521.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;23.5;3395.3;144.5;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3521.24-en-x-line-slight-l-down-led-3900-plx-e-24-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-PLX-E-24-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 3900 PLX E 34 830 / L-1693MM S-1,5M;19.4085.3511.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;23.5;3159;134.4;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3511.34-en-x-line-slight-l-down-led-3900-plx-e-34-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-PLX-E-34-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 3900 PLX E 34 840 / L-1693MM S-1,5M;19.4085.3521.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;23.5;3395.3;144.5;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3521.34-en-x-line-slight-l-down-led-3900-plx-e-34-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-PLX-E-34-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 3900 PLX EDD 04 830 / L-1693MM S-1,5M;19.4085.3513.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;23.5;3159;134.4;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3513.04-en-x-line-slight-l-down-led-3900-plx-edd-04-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-PLX-EDD-04-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 3900 PLX EDD 04 840 / L-1693MM S-1,5M;19.4085.3523.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;23.5;3395.3;144.5;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3523.04-en-x-line-slight-l-down-led-3900-plx-edd-04-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-PLX-EDD-04-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 3900 PLX EDD 21 830 / L-1693MM S-1,5M;19.4085.3513.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;23.5;3159;134.4;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3513.21-en-x-line-slight-l-down-led-3900-plx-edd-21-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-PLX-EDD-21-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 3900 PLX EDD 21 840 / L-1693MM S-1,5M;19.4085.3523.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;23.5;3395.3;144.5;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3523.21-en-x-line-slight-l-down-led-3900-plx-edd-21-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-PLX-EDD-21-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 3900 PLX EDD 24 830 / L-1693MM S-1,5M;19.4085.3513.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;23.5;3159;134.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3513.24-en-x-line-slight-l-down-led-3900-plx-edd-24-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-PLX-EDD-24-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 3900 PLX EDD 24 840 / L-1693MM S-1,5M;19.4085.3523.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;23.5;3395.3;144.5;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3523.24-en-x-line-slight-l-down-led-3900-plx-edd-24-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-PLX-EDD-24-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 3900 PLX EDD 34 830 / L-1693MM S-1,5M;19.4085.3513.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;23.5;3159;134.4;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3513.34-en-x-line-slight-l-down-led-3900-plx-edd-34-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-PLX-EDD-34-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 3900 PLX EDD 34 840 / L-1693MM S-1,5M;19.4085.3523.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;23.5;3395.3;144.5;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3523.34-en-x-line-slight-l-down-led-3900-plx-edd-34-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-3900-PLX-EDD-34-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 4400 MICRO-PRM E 04 830 / L-1134MM S-1,5M;19.4085.6611.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.9;3631.6;140.2;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6611.04-en-x-line-slight-l-down-led-4400-micro-prm-e-04-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-MICRO-PRM-E-04-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 4400 MICRO-PRM E 04 840 / L-1134MM S-1,5M;19.4085.6621.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.9;3903.9;150.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6621.04-en-x-line-slight-l-down-led-4400-micro-prm-e-04-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-MICRO-PRM-E-04-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 4400 MICRO-PRM E 21 830 / L-1134MM S-1,5M;19.4085.6611.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.9;3631.6;140.2;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6611.21-en-x-line-slight-l-down-led-4400-micro-prm-e-21-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-MICRO-PRM-E-21-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 4400 MICRO-PRM E 21 840 / L-1134MM S-1,5M;19.4085.6621.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.9;3903.9;150.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6621.21-en-x-line-slight-l-down-led-4400-micro-prm-e-21-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-MICRO-PRM-E-21-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 4400 MICRO-PRM E 24 830 / L-1134MM S-1,5M;19.4085.6611.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.9;3631.6;140.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6611.24-en-x-line-slight-l-down-led-4400-micro-prm-e-24-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-MICRO-PRM-E-24-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 4400 MICRO-PRM E 24 840 / L-1134MM S-1,5M;19.4085.6621.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.9;3903.9;150.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6621.24-en-x-line-slight-l-down-led-4400-micro-prm-e-24-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-MICRO-PRM-E-24-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 4400 MICRO-PRM E 34 830 / L-1134MM S-1,5M;19.4085.6611.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.9;3631.6;140.2;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6611.34-en-x-line-slight-l-down-led-4400-micro-prm-e-34-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-MICRO-PRM-E-34-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 4400 MICRO-PRM E 34 840 / L-1134MM S-1,5M;19.4085.6621.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.9;3903.9;150.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6621.34-en-x-line-slight-l-down-led-4400-micro-prm-e-34-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-MICRO-PRM-E-34-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 4400 MICRO-PRM EDD 04 830 / L-1134MM S-1,5M;19.4085.6613.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.9;3631.6;140.2;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6613.04-en-x-line-slight-l-down-led-4400-micro-prm-edd-04-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-MICRO-PRM-EDD-04-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 4400 MICRO-PRM EDD 04 840 / L-1134MM S-1,5M;19.4085.6623.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.9;3903.9;150.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6623.04-en-x-line-slight-l-down-led-4400-micro-prm-edd-04-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-MICRO-PRM-EDD-04-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 4400 MICRO-PRM EDD 21 830 / L-1134MM S-1,5M;19.4085.6613.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.9;3631.6;140.2;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6613.21-en-x-line-slight-l-down-led-4400-micro-prm-edd-21-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-MICRO-PRM-EDD-21-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 4400 MICRO-PRM EDD 21 840 / L-1134MM S-1,5M;19.4085.6623.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.9;3903.9;150.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6623.21-en-x-line-slight-l-down-led-4400-micro-prm-edd-21-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-MICRO-PRM-EDD-21-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 4400 MICRO-PRM EDD 24 830 / L-1134MM S-1,5M;19.4085.6613.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.9;3631.6;140.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6613.24-en-x-line-slight-l-down-led-4400-micro-prm-edd-24-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-MICRO-PRM-EDD-24-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 4400 MICRO-PRM EDD 24 840 / L-1134MM S-1,5M;19.4085.6623.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.9;3903.9;150.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6623.24-en-x-line-slight-l-down-led-4400-micro-prm-edd-24-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-MICRO-PRM-EDD-24-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 4400 MICRO-PRM EDD 34 830 / L-1134MM S-1,5M;19.4085.6613.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.9;3631.6;140.2;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6613.34-en-x-line-slight-l-down-led-4400-micro-prm-edd-34-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-MICRO-PRM-EDD-34-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 4400 MICRO-PRM EDD 34 840 / L-1134MM S-1,5M;19.4085.6623.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.9;3903.9;150.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.6623.34-en-x-line-slight-l-down-led-4400-micro-prm-edd-34-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-MICRO-PRM-EDD-34-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 4400 PLX E 04 830 / L-1134MM S-1,5M;19.4085.2611.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.9;3342;129;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2611.04-en-x-line-slight-l-down-led-4400-plx-e-04-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-PLX-E-04-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 4400 PLX E 04 840 / L-1134MM S-1,5M;19.4085.2621.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.9;3592.5;138.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2621.04-en-x-line-slight-l-down-led-4400-plx-e-04-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-PLX-E-04-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 4400 PLX E 21 830 / L-1134MM S-1,5M;19.4085.2611.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.9;3342;129;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2611.21-en-x-line-slight-l-down-led-4400-plx-e-21-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-PLX-E-21-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 4400 PLX E 21 840 / L-1134MM S-1,5M;19.4085.2621.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.9;3592.5;138.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2621.21-en-x-line-slight-l-down-led-4400-plx-e-21-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-PLX-E-21-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 4400 PLX E 24 830 / L-1134MM S-1,5M;19.4085.2611.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.9;3342;129;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2611.24-en-x-line-slight-l-down-led-4400-plx-e-24-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-PLX-E-24-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 4400 PLX E 24 840 / L-1134MM S-1,5M;19.4085.2621.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.9;3592.5;138.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2621.24-en-x-line-slight-l-down-led-4400-plx-e-24-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-PLX-E-24-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 4400 PLX E 34 830 / L-1134MM S-1,5M;19.4085.2611.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.9;3342;129;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2611.34-en-x-line-slight-l-down-led-4400-plx-e-34-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-PLX-E-34-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 4400 PLX E 34 840 / L-1134MM S-1,5M;19.4085.2621.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.9;3592.5;138.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2621.34-en-x-line-slight-l-down-led-4400-plx-e-34-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-PLX-E-34-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 4400 PLX EDD 04 830 / L-1134MM S-1,5M;19.4085.2613.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.9;3342;129;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2613.04-en-x-line-slight-l-down-led-4400-plx-edd-04-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-PLX-EDD-04-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 4400 PLX EDD 04 840 / L-1134MM S-1,5M;19.4085.2623.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.9;3592.5;138.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2623.04-en-x-line-slight-l-down-led-4400-plx-edd-04-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-PLX-EDD-04-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 4400 PLX EDD 21 830 / L-1134MM S-1,5M;19.4085.2613.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.9;3342;129;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2613.21-en-x-line-slight-l-down-led-4400-plx-edd-21-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-PLX-EDD-21-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 4400 PLX EDD 21 840 / L-1134MM S-1,5M;19.4085.2623.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.9;3592.5;138.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2623.21-en-x-line-slight-l-down-led-4400-plx-edd-21-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-PLX-EDD-21-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 4400 PLX EDD 24 830 / L-1134MM S-1,5M;19.4085.2613.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.9;3342;129;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2613.24-en-x-line-slight-l-down-led-4400-plx-edd-24-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-PLX-EDD-24-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 4400 PLX EDD 24 840 / L-1134MM S-1,5M;19.4085.2623.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.9;3592.5;138.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2623.24-en-x-line-slight-l-down-led-4400-plx-edd-24-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-PLX-EDD-24-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 4400 PLX EDD 34 830 / L-1134MM S-1,5M;19.4085.2613.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.9;3342;129;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2613.34-en-x-line-slight-l-down-led-4400-plx-edd-34-830-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-PLX-EDD-34-830-L-1134MM-S-15M.ies;1134;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 4400 PLX EDD 34 840 / L-1134MM S-1,5M;19.4085.2623.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);1134 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.9;3592.5;138.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.2623.34-en-x-line-slight-l-down-led-4400-plx-edd-34-840-l-1134mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-4400-PLX-EDD-34-840-L-1134MM-S-15M.ies;1134;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 5200 MICRO-PRM E 04 830 / L-2256MM S-1,5M;19.4085.8711.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.4;4577;145.8;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8711.04-en-x-line-slight-l-down-led-5200-micro-prm-e-04-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-MICRO-PRM-E-04-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 5200 MICRO-PRM E 04 840 / L-2256MM S-1,5M;19.4085.8721.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.4;4919.3;156.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8721.04-en-x-line-slight-l-down-led-5200-micro-prm-e-04-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-MICRO-PRM-E-04-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 5200 MICRO-PRM E 21 830 / L-2256MM S-1,5M;19.4085.8711.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.4;4577;145.8;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8711.21-en-x-line-slight-l-down-led-5200-micro-prm-e-21-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-MICRO-PRM-E-21-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 5200 MICRO-PRM E 21 840 / L-2256MM S-1,5M;19.4085.8721.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.4;4919.3;156.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8721.21-en-x-line-slight-l-down-led-5200-micro-prm-e-21-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-MICRO-PRM-E-21-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 5200 MICRO-PRM E 24 830 / L-2256MM S-1,5M;19.4085.8711.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.4;4577;145.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8711.24-en-x-line-slight-l-down-led-5200-micro-prm-e-24-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-MICRO-PRM-E-24-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 5200 MICRO-PRM E 24 840 / L-2256MM S-1,5M;19.4085.8721.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.4;4919.3;156.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8721.24-en-x-line-slight-l-down-led-5200-micro-prm-e-24-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-MICRO-PRM-E-24-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 5200 MICRO-PRM E 34 830 / L-2256MM S-1,5M;19.4085.8711.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.4;4577;145.8;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8711.34-en-x-line-slight-l-down-led-5200-micro-prm-e-34-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-MICRO-PRM-E-34-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 5200 MICRO-PRM E 34 840 / L-2256MM S-1,5M;19.4085.8721.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.4;4919.3;156.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8721.34-en-x-line-slight-l-down-led-5200-micro-prm-e-34-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-MICRO-PRM-E-34-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 5200 MICRO-PRM EDD 04 830 / L-2256MM S-1,5M;19.4085.8713.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.4;4577;145.8;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8713.04-en-x-line-slight-l-down-led-5200-micro-prm-edd-04-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-MICRO-PRM-EDD-04-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 5200 MICRO-PRM EDD 04 840 / L-2256MM S-1,5M;19.4085.8723.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.4;4919.3;156.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8723.04-en-x-line-slight-l-down-led-5200-micro-prm-edd-04-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-MICRO-PRM-EDD-04-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 5200 MICRO-PRM EDD 21 830 / L-2256MM S-1,5M;19.4085.8713.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.4;4577;145.8;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8713.21-en-x-line-slight-l-down-led-5200-micro-prm-edd-21-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-MICRO-PRM-EDD-21-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 5200 MICRO-PRM EDD 21 840 / L-2256MM S-1,5M;19.4085.8723.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.4;4919.3;156.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8723.21-en-x-line-slight-l-down-led-5200-micro-prm-edd-21-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-MICRO-PRM-EDD-21-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 5200 MICRO-PRM EDD 24 830 / L-2256MM S-1,5M;19.4085.8713.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.4;4577;145.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8713.24-en-x-line-slight-l-down-led-5200-micro-prm-edd-24-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-MICRO-PRM-EDD-24-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 5200 MICRO-PRM EDD 24 840 / L-2256MM S-1,5M;19.4085.8723.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.4;4919.3;156.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8723.24-en-x-line-slight-l-down-led-5200-micro-prm-edd-24-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-MICRO-PRM-EDD-24-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 5200 MICRO-PRM EDD 34 830 / L-2256MM S-1,5M;19.4085.8713.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.4;4577;145.8;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8713.34-en-x-line-slight-l-down-led-5200-micro-prm-edd-34-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-MICRO-PRM-EDD-34-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 5200 MICRO-PRM EDD 34 840 / L-2256MM S-1,5M;19.4085.8723.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.4;4919.3;156.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8723.34-en-x-line-slight-l-down-led-5200-micro-prm-edd-34-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-MICRO-PRM-EDD-34-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 5200 PLX E 04 830 / L-2256MM S-1,5M;19.4085.4711.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.4;4212;134.1;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4711.04-en-x-line-slight-l-down-led-5200-plx-e-04-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-PLX-E-04-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 5200 PLX E 04 840 / L-2256MM S-1,5M;19.4085.4721.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.4;4527;144.2;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4721.04-en-x-line-slight-l-down-led-5200-plx-e-04-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-PLX-E-04-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 5200 PLX E 21 830 / L-2256MM S-1,5M;19.4085.4711.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.4;4212;134.1;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4711.21-en-x-line-slight-l-down-led-5200-plx-e-21-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-PLX-E-21-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 5200 PLX E 21 840 / L-2256MM S-1,5M;19.4085.4721.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.4;4527;144.2;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4721.21-en-x-line-slight-l-down-led-5200-plx-e-21-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-PLX-E-21-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 5200 PLX E 24 830 / L-2256MM S-1,5M;19.4085.4711.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.4;4212;134.1;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4711.24-en-x-line-slight-l-down-led-5200-plx-e-24-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-PLX-E-24-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 5200 PLX E 24 840 / L-2256MM S-1,5M;19.4085.4721.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.4;4527;144.2;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4721.24-en-x-line-slight-l-down-led-5200-plx-e-24-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-PLX-E-24-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 5200 PLX E 34 830 / L-2256MM S-1,5M;19.4085.4711.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.4;4212;134.1;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4711.34-en-x-line-slight-l-down-led-5200-plx-e-34-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-PLX-E-34-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 5200 PLX E 34 840 / L-2256MM S-1,5M;19.4085.4721.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.4;4527;144.2;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4721.34-en-x-line-slight-l-down-led-5200-plx-e-34-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-PLX-E-34-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 5200 PLX EDD 04 830 / L-2256MM S-1,5M;19.4085.4713.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.4;4212;134.1;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4713.04-en-x-line-slight-l-down-led-5200-plx-edd-04-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-PLX-EDD-04-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 5200 PLX EDD 04 840 / L-2256MM S-1,5M;19.4085.4723.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.4;4527;144.2;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4723.04-en-x-line-slight-l-down-led-5200-plx-edd-04-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-PLX-EDD-04-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 5200 PLX EDD 21 830 / L-2256MM S-1,5M;19.4085.4713.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.4;4212;134.1;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4713.21-en-x-line-slight-l-down-led-5200-plx-edd-21-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-PLX-EDD-21-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 5200 PLX EDD 21 840 / L-2256MM S-1,5M;19.4085.4723.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.4;4527;144.2;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4723.21-en-x-line-slight-l-down-led-5200-plx-edd-21-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-PLX-EDD-21-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 5200 PLX EDD 24 830 / L-2256MM S-1,5M;19.4085.4713.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.4;4212;134.1;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4713.24-en-x-line-slight-l-down-led-5200-plx-edd-24-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-PLX-EDD-24-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 5200 PLX EDD 24 840 / L-2256MM S-1,5M;19.4085.4723.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.4;4527;144.2;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4723.24-en-x-line-slight-l-down-led-5200-plx-edd-24-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-PLX-EDD-24-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 5200 PLX EDD 34 830 / L-2256MM S-1,5M;19.4085.4713.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.4;4212;134.1;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4713.34-en-x-line-slight-l-down-led-5200-plx-edd-34-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-PLX-EDD-34-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 5200 PLX EDD 34 840 / L-2256MM S-1,5M;19.4085.4723.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.4;4527;144.2;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4723.34-en-x-line-slight-l-down-led-5200-plx-edd-34-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-5200-PLX-EDD-34-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 6600 MICRO-PRM E 04 830 / L-1693MM S-1,5M;19.4085.7811.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;38.9;5447.5;140;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7811.04-en-x-line-slight-l-down-led-6600-micro-prm-e-04-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-MICRO-PRM-E-04-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 6600 MICRO-PRM E 04 840 / L-1693MM S-1,5M;19.4085.7821.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;38.9;5855.8;150.5;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7821.04-en-x-line-slight-l-down-led-6600-micro-prm-e-04-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-MICRO-PRM-E-04-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 6600 MICRO-PRM E 21 830 / L-1693MM S-1,5M;19.4085.7811.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;38.9;5447.5;140;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7811.21-en-x-line-slight-l-down-led-6600-micro-prm-e-21-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-MICRO-PRM-E-21-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 6600 MICRO-PRM E 21 840 / L-1693MM S-1,5M;19.4085.7821.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;38.9;5855.8;150.5;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7821.21-en-x-line-slight-l-down-led-6600-micro-prm-e-21-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-MICRO-PRM-E-21-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 6600 MICRO-PRM E 24 830 / L-1693MM S-1,5M;19.4085.7811.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;38.9;5447.5;140;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7811.24-en-x-line-slight-l-down-led-6600-micro-prm-e-24-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-MICRO-PRM-E-24-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 6600 MICRO-PRM E 24 840 / L-1693MM S-1,5M;19.4085.7821.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;38.9;5855.8;150.5;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7821.24-en-x-line-slight-l-down-led-6600-micro-prm-e-24-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-MICRO-PRM-E-24-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 6600 MICRO-PRM E 34 830 / L-1693MM S-1,5M;19.4085.7811.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;38.9;5447.5;140;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7811.34-en-x-line-slight-l-down-led-6600-micro-prm-e-34-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-MICRO-PRM-E-34-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 6600 MICRO-PRM E 34 840 / L-1693MM S-1,5M;19.4085.7821.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;38.9;5855.8;150.5;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7821.34-en-x-line-slight-l-down-led-6600-micro-prm-e-34-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-MICRO-PRM-E-34-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 6600 MICRO-PRM EDD 04 830 / L-1693MM S-1,5M;19.4085.7813.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;38.9;5447.5;140;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7813.04-en-x-line-slight-l-down-led-6600-micro-prm-edd-04-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-MICRO-PRM-EDD-04-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 6600 MICRO-PRM EDD 04 840 / L-1693MM S-1,5M;19.4085.7823.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;38.9;5855.8;150.5;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7823.04-en-x-line-slight-l-down-led-6600-micro-prm-edd-04-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-MICRO-PRM-EDD-04-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 6600 MICRO-PRM EDD 21 830 / L-1693MM S-1,5M;19.4085.7813.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;38.9;5447.5;140;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7813.21-en-x-line-slight-l-down-led-6600-micro-prm-edd-21-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-MICRO-PRM-EDD-21-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 6600 MICRO-PRM EDD 21 840 / L-1693MM S-1,5M;19.4085.7823.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;38.9;5855.8;150.5;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7823.21-en-x-line-slight-l-down-led-6600-micro-prm-edd-21-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-MICRO-PRM-EDD-21-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 6600 MICRO-PRM EDD 24 830 / L-1693MM S-1,5M;19.4085.7813.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;38.9;5447.5;140;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7813.24-en-x-line-slight-l-down-led-6600-micro-prm-edd-24-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-MICRO-PRM-EDD-24-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 6600 MICRO-PRM EDD 24 840 / L-1693MM S-1,5M;19.4085.7823.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;38.9;5855.8;150.5;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7823.24-en-x-line-slight-l-down-led-6600-micro-prm-edd-24-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-MICRO-PRM-EDD-24-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 6600 MICRO-PRM EDD 34 830 / L-1693MM S-1,5M;19.4085.7813.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;38.9;5447.5;140;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7813.34-en-x-line-slight-l-down-led-6600-micro-prm-edd-34-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-MICRO-PRM-EDD-34-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 6600 MICRO-PRM EDD 34 840 / L-1693MM S-1,5M;19.4085.7823.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;38.9;5855.8;150.5;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.7823.34-en-x-line-slight-l-down-led-6600-micro-prm-edd-34-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-MICRO-PRM-EDD-34-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 6600 PLX E 04 830 / L-1693MM S-1,5M;19.4085.3811.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;38.9;5013;128.9;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3811.04-en-x-line-slight-l-down-led-6600-plx-e-04-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-PLX-E-04-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 6600 PLX E 04 840 / L-1693MM S-1,5M;19.4085.3821.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;38.9;5388.8;138.5;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3821.04-en-x-line-slight-l-down-led-6600-plx-e-04-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-PLX-E-04-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 6600 PLX E 21 830 / L-1693MM S-1,5M;19.4085.3811.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;38.9;5013;128.9;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3811.21-en-x-line-slight-l-down-led-6600-plx-e-21-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-PLX-E-21-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 6600 PLX E 21 840 / L-1693MM S-1,5M;19.4085.3821.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;38.9;5388.8;138.5;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3821.21-en-x-line-slight-l-down-led-6600-plx-e-21-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-PLX-E-21-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 6600 PLX E 24 830 / L-1693MM S-1,5M;19.4085.3811.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;38.9;5013;128.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3811.24-en-x-line-slight-l-down-led-6600-plx-e-24-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-PLX-E-24-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 6600 PLX E 24 840 / L-1693MM S-1,5M;19.4085.3821.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;38.9;5388.8;138.5;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3821.24-en-x-line-slight-l-down-led-6600-plx-e-24-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-PLX-E-24-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 6600 PLX E 34 830 / L-1693MM S-1,5M;19.4085.3811.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;38.9;5013;128.9;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3811.34-en-x-line-slight-l-down-led-6600-plx-e-34-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-PLX-E-34-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 6600 PLX E 34 840 / L-1693MM S-1,5M;19.4085.3821.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;38.9;5388.8;138.5;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3821.34-en-x-line-slight-l-down-led-6600-plx-e-34-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-PLX-E-34-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 6600 PLX EDD 04 830 / L-1693MM S-1,5M;19.4085.3813.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;38.9;5013;128.9;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3813.04-en-x-line-slight-l-down-led-6600-plx-edd-04-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-PLX-EDD-04-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 6600 PLX EDD 04 840 / L-1693MM S-1,5M;19.4085.3823.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;38.9;5388.8;138.5;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3823.04-en-x-line-slight-l-down-led-6600-plx-edd-04-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-PLX-EDD-04-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 6600 PLX EDD 21 830 / L-1693MM S-1,5M;19.4085.3813.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;38.9;5013;128.9;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3813.21-en-x-line-slight-l-down-led-6600-plx-edd-21-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-PLX-EDD-21-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 6600 PLX EDD 21 840 / L-1693MM S-1,5M;19.4085.3823.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;38.9;5388.8;138.5;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3823.21-en-x-line-slight-l-down-led-6600-plx-edd-21-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-PLX-EDD-21-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 6600 PLX EDD 24 830 / L-1693MM S-1,5M;19.4085.3813.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;38.9;5013;128.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3813.24-en-x-line-slight-l-down-led-6600-plx-edd-24-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-PLX-EDD-24-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 6600 PLX EDD 24 840 / L-1693MM S-1,5M;19.4085.3823.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;38.9;5388.8;138.5;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3823.24-en-x-line-slight-l-down-led-6600-plx-edd-24-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-PLX-EDD-24-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 6600 PLX EDD 34 830 / L-1693MM S-1,5M;19.4085.3813.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;38.9;5013;128.9;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3813.34-en-x-line-slight-l-down-led-6600-plx-edd-34-830-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-PLX-EDD-34-830-L-1693MM-S-15M.ies;1693;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 6600 PLX EDD 34 840 / L-1693MM S-1,5M;19.4085.3823.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);1693 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;38.9;5388.8;138.5;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.3823.34-en-x-line-slight-l-down-led-6600-plx-edd-34-840-l-1693mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-6600-PLX-EDD-34-840-L-1693MM-S-15M.ies;1693;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 8800 MICRO-PRM E 04 830 / L-2256MM S-1,5M;19.4085.8911.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;51.8;7263.3;140.2;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8911.04-en-x-line-slight-l-down-led-8800-micro-prm-e-04-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-MICRO-PRM-E-04-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 8800 MICRO-PRM E 04 840 / L-2256MM S-1,5M;19.4085.8921.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;51.8;7807.7;150.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8921.04-en-x-line-slight-l-down-led-8800-micro-prm-e-04-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-MICRO-PRM-E-04-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 8800 MICRO-PRM E 21 830 / L-2256MM S-1,5M;19.4085.8911.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;51.8;7263.3;140.2;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8911.21-en-x-line-slight-l-down-led-8800-micro-prm-e-21-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-MICRO-PRM-E-21-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 8800 MICRO-PRM E 21 840 / L-2256MM S-1,5M;19.4085.8921.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;51.8;7807.7;150.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8921.21-en-x-line-slight-l-down-led-8800-micro-prm-e-21-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-MICRO-PRM-E-21-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 8800 MICRO-PRM E 24 830 / L-2256MM S-1,5M;19.4085.8911.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;51.8;7263.3;140.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8911.24-en-x-line-slight-l-down-led-8800-micro-prm-e-24-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-MICRO-PRM-E-24-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 8800 MICRO-PRM E 24 840 / L-2256MM S-1,5M;19.4085.8921.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;51.8;7807.7;150.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8921.24-en-x-line-slight-l-down-led-8800-micro-prm-e-24-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-MICRO-PRM-E-24-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 8800 MICRO-PRM E 34 830 / L-2256MM S-1,5M;19.4085.8911.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;51.8;7263.3;140.2;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8911.34-en-x-line-slight-l-down-led-8800-micro-prm-e-34-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-MICRO-PRM-E-34-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 8800 MICRO-PRM E 34 840 / L-2256MM S-1,5M;19.4085.8921.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;51.8;7807.7;150.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8921.34-en-x-line-slight-l-down-led-8800-micro-prm-e-34-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-MICRO-PRM-E-34-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 8800 MICRO-PRM EDD 04 830 / L-2256MM S-1,5M;19.4085.8913.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;51.8;7263.3;140.2;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8913.04-en-x-line-slight-l-down-led-8800-micro-prm-edd-04-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-MICRO-PRM-EDD-04-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 8800 MICRO-PRM EDD 04 840 / L-2256MM S-1,5M;19.4085.8923.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;51.8;7807.7;150.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8923.04-en-x-line-slight-l-down-led-8800-micro-prm-edd-04-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-MICRO-PRM-EDD-04-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 8800 MICRO-PRM EDD 21 830 / L-2256MM S-1,5M;19.4085.8913.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;51.8;7263.3;140.2;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8913.21-en-x-line-slight-l-down-led-8800-micro-prm-edd-21-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-MICRO-PRM-EDD-21-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 8800 MICRO-PRM EDD 21 840 / L-2256MM S-1,5M;19.4085.8923.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;51.8;7807.7;150.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8923.21-en-x-line-slight-l-down-led-8800-micro-prm-edd-21-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-MICRO-PRM-EDD-21-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 8800 MICRO-PRM EDD 24 830 / L-2256MM S-1,5M;19.4085.8913.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;51.8;7263.3;140.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8913.24-en-x-line-slight-l-down-led-8800-micro-prm-edd-24-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-MICRO-PRM-EDD-24-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 8800 MICRO-PRM EDD 24 840 / L-2256MM S-1,5M;19.4085.8923.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;51.8;7807.7;150.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8923.24-en-x-line-slight-l-down-led-8800-micro-prm-edd-24-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-MICRO-PRM-EDD-24-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 8800 MICRO-PRM EDD 34 830 / L-2256MM S-1,5M;19.4085.8913.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;51.8;7263.3;140.2;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8913.34-en-x-line-slight-l-down-led-8800-micro-prm-edd-34-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-MICRO-PRM-EDD-34-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 8800 MICRO-PRM EDD 34 840 / L-2256MM S-1,5M;19.4085.8923.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;51.8;7807.7;150.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111°;IP40;IK04;I;RG0;0.815008;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.8923.34-en-x-line-slight-l-down-led-8800-micro-prm-edd-34-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-MICRO-PRM-EDD-34-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 8800 PLX E 04 830 / L-2256MM S-1,5M;19.4085.4911.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;51.8;6684;129;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4911.04-en-x-line-slight-l-down-led-8800-plx-e-04-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-PLX-E-04-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 8800 PLX E 04 840 / L-2256MM S-1,5M;19.4085.4921.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;51.8;7185;138.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4921.04-en-x-line-slight-l-down-led-8800-plx-e-04-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-PLX-E-04-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 8800 PLX E 21 830 / L-2256MM S-1,5M;19.4085.4911.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;51.8;6684;129;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4911.21-en-x-line-slight-l-down-led-8800-plx-e-21-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-PLX-E-21-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 8800 PLX E 21 840 / L-2256MM S-1,5M;19.4085.4921.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;51.8;7185;138.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4921.21-en-x-line-slight-l-down-led-8800-plx-e-21-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-PLX-E-21-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 8800 PLX E 24 830 / L-2256MM S-1,5M;19.4085.4911.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;51.8;6684;129;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4911.24-en-x-line-slight-l-down-led-8800-plx-e-24-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-PLX-E-24-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 8800 PLX E 24 840 / L-2256MM S-1,5M;19.4085.4921.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;51.8;7185;138.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4921.24-en-x-line-slight-l-down-led-8800-plx-e-24-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-PLX-E-24-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 8800 PLX E 34 830 / L-2256MM S-1,5M;19.4085.4911.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;51.8;6684;129;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4911.34-en-x-line-slight-l-down-led-8800-plx-e-34-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-PLX-E-34-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 8800 PLX E 34 840 / L-2256MM S-1,5M;19.4085.4921.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;51.8;7185;138.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4921.34-en-x-line-slight-l-down-led-8800-plx-e-34-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-PLX-E-34-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 8800 PLX EDD 04 830 / L-2256MM S-1,5M;19.4085.4913.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;51.8;6684;129;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4913.04-en-x-line-slight-l-down-led-8800-plx-edd-04-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-PLX-EDD-04-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 8800 PLX EDD 04 840 / L-2256MM S-1,5M;19.4085.4923.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;51.8;7185;138.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4923.04-en-x-line-slight-l-down-led-8800-plx-edd-04-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-PLX-EDD-04-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 8800 PLX EDD 21 830 / L-2256MM S-1,5M;19.4085.4913.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;51.8;6684;129;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4913.21-en-x-line-slight-l-down-led-8800-plx-edd-21-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-PLX-EDD-21-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 8800 PLX EDD 21 840 / L-2256MM S-1,5M;19.4085.4923.21;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;51.8;7185;138.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4923.21-en-x-line-slight-l-down-led-8800-plx-edd-21-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-PLX-EDD-21-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 8800 PLX EDD 24 830 / L-2256MM S-1,5M;19.4085.4913.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;51.8;6684;129;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4913.24-en-x-line-slight-l-down-led-8800-plx-edd-24-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-PLX-EDD-24-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 8800 PLX EDD 24 840 / L-2256MM S-1,5M;19.4085.4923.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;51.8;7185;138.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4923.24-en-x-line-slight-l-down-led-8800-plx-edd-24-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-PLX-EDD-24-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
X-LINE SLIGHT L-DOWN LED 8800 PLX EDD 34 830 / L-2256MM S-1,5M;19.4085.4913.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;51.8;6684;129;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4913.34-en-x-line-slight-l-down-led-8800-plx-edd-34-830-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-PLX-EDD-34-830-L-2256MM-S-15M.ies;2256;34;68;230;3000
X-LINE SLIGHT L-DOWN LED 8800 PLX EDD 34 840 / L-2256MM S-1,5M;19.4085.4923.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);2256 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;51.8;7185;138.7;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103°;IP40;IK04;I;RG0;0.755007;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4085.4923.34-en-x-line-slight-l-down-led-8800-plx-edd-34-840-l-2256mm-s-15m.pdf;X-LINE-SLIGHT-L-DOWN-LED-8800-PLX-EDD-34-840-L-2256MM-S-15M.ies;2256;34;68;230;4000
