;Assembly Code##OTHER##;Assembly##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Dimensions##OTHER##;Voltage (range)##OTHER##;Driver##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Power of luminaire##ELECTRICAL_WATTAGE##WATTS;Luminaire luminous flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Luminaire's light efficiency##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;Color of the light##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Efficiency##OTHER##;Power factor##OTHER##;Manufacturer##OTHER##;URL##OTHER##;Catalogue##OTHER## ;Photometric Web File##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN
X-LINE SLIGHT SPOTS L-DOWN LED 2600 MICRO-PRM E / 2x 600 15° E 04 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.211E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.211E.04-en-x-line-slight-spots-l-down-led-2600-micro-prm-e-2x-600-15-e-04-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-MICRO-PRM-E-2X-600-15-E-04-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 MICRO-PRM E / 2x 600 15° E 04 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.212E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.212E.04-en-x-line-slight-spots-l-down-led-2600-micro-prm-e-2x-600-15-e-04-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-MICRO-PRM-E-2X-600-15-E-04-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 MICRO-PRM E / 2x 600 15° E 24 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.211E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.211E.24-en-x-line-slight-spots-l-down-led-2600-micro-prm-e-2x-600-15-e-24-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-MICRO-PRM-E-2X-600-15-E-24-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 MICRO-PRM E / 2x 600 15° E 24 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.212E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.212E.24-en-x-line-slight-spots-l-down-led-2600-micro-prm-e-2x-600-15-e-24-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-MICRO-PRM-E-2X-600-15-E-24-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 MICRO-PRM E / 2x 600 15° E 34 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.211E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.211E.34-en-x-line-slight-spots-l-down-led-2600-micro-prm-e-2x-600-15-e-34-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-MICRO-PRM-E-2X-600-15-E-34-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 MICRO-PRM E / 2x 600 15° E 34 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.212E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.212E.34-en-x-line-slight-spots-l-down-led-2600-micro-prm-e-2x-600-15-e-34-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-MICRO-PRM-E-2X-600-15-E-34-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 MICRO-PRM EDD / 2x 600 15° EDD 04 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.211F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.211F.04-en-x-line-slight-spots-l-down-led-2600-micro-prm-edd-2x-600-15-edd-04-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-MICRO-PRM-EDD-2X-600-15-EDD-04-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 MICRO-PRM EDD / 2x 600 15° EDD 04 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.212F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.212F.04-en-x-line-slight-spots-l-down-led-2600-micro-prm-edd-2x-600-15-edd-04-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-MICRO-PRM-EDD-2X-600-15-EDD-04-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 MICRO-PRM EDD / 2x 600 15° EDD 24 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.211F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.211F.24-en-x-line-slight-spots-l-down-led-2600-micro-prm-edd-2x-600-15-edd-24-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-MICRO-PRM-EDD-2X-600-15-EDD-24-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 MICRO-PRM EDD / 2x 600 15° EDD 24 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.212F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.212F.24-en-x-line-slight-spots-l-down-led-2600-micro-prm-edd-2x-600-15-edd-24-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-MICRO-PRM-EDD-2X-600-15-EDD-24-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 MICRO-PRM EDD / 2x 600 15° EDD 34 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.211F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.211F.34-en-x-line-slight-spots-l-down-led-2600-micro-prm-edd-2x-600-15-edd-34-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-MICRO-PRM-EDD-2X-600-15-EDD-34-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 MICRO-PRM EDD / 2x 600 15° EDD 34 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.212F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.212F.34-en-x-line-slight-spots-l-down-led-2600-micro-prm-edd-2x-600-15-edd-34-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-MICRO-PRM-EDD-2X-600-15-EDD-34-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 PLX E / 2x 600 15° E 04 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.111E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.111E.04-en-x-line-slight-spots-l-down-led-2600-plx-e-2x-600-15-e-04-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-PLX-E-2X-600-15-E-04-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 PLX E / 2x 600 15° E 04 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.112E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.112E.04-en-x-line-slight-spots-l-down-led-2600-plx-e-2x-600-15-e-04-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-PLX-E-2X-600-15-E-04-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 PLX E / 2x 600 15° E 24 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.111E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.111E.24-en-x-line-slight-spots-l-down-led-2600-plx-e-2x-600-15-e-24-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-PLX-E-2X-600-15-E-24-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 PLX E / 2x 600 15° E 24 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.112E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.112E.24-en-x-line-slight-spots-l-down-led-2600-plx-e-2x-600-15-e-24-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-PLX-E-2X-600-15-E-24-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 PLX E / 2x 600 15° E 34 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.111E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.111E.34-en-x-line-slight-spots-l-down-led-2600-plx-e-2x-600-15-e-34-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-PLX-E-2X-600-15-E-34-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 PLX E / 2x 600 15° E 34 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.112E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.112E.34-en-x-line-slight-spots-l-down-led-2600-plx-e-2x-600-15-e-34-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-PLX-E-2X-600-15-E-34-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 PLX EDD / 2x 600 15° EDD 04 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.111F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.111F.04-en-x-line-slight-spots-l-down-led-2600-plx-e-2x-600-15-edd-04-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-PLX-EDD-2X-600-15-EDD-04-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 PLX EDD / 2x 600 15° EDD 04 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.112F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.112F.04-en-x-line-slight-spots-l-down-led-2600-plx-e-2x-600-15-edd-04-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-PLX-EDD-2X-600-15-EDD-04-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 PLX EDD / 2x 600 15° EDD 24 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.111F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.111F.24-en-x-line-slight-spots-l-down-led-2600-plx-e-2x-600-15-edd-24-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-PLX-EDD-2X-600-15-EDD-24-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 PLX EDD / 2x 600 15° EDD 24 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.112F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.112F.24-en-x-line-slight-spots-l-down-led-2600-plx-e-2x-600-15-edd-24-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-PLX-EDD-2X-600-15-EDD-24-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 PLX EDD / 2x 600 15° EDD 34 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.111F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.111F.34-en-x-line-slight-spots-l-down-led-2600-plx-e-2x-600-15-edd-34-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-PLX-EDD-2X-600-15-EDD-34-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 2600 PLX EDD / 2x 600 15° EDD 34 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.112F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.112F.34-en-x-line-slight-spots-l-down-led-2600-plx-e-2x-600-15-edd-34-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-2600-PLX-EDD-2X-600-15-EDD-34-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 MICRO-PRM E / 2x 600 15° E 04 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.431E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.431E.04-en-x-line-slight-spots-l-down-led-3900-micro-prm-e-2x-600-15-e-04-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-MICRO-PRM-E-2X-600-15-E-04-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 MICRO-PRM E / 2x 600 15° E 04 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.432E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.432E.04-en-x-line-slight-spots-l-down-led-3900-micro-prm-e-2x-600-15-e-04-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-MICRO-PRM-E-2X-600-15-E-04-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 MICRO-PRM E / 2x 600 15° E 24 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.431E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.431E.24-en-x-line-slight-spots-l-down-led-3900-micro-prm-e-2x-600-15-e-24-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-MICRO-PRM-E-2X-600-15-E-24-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 MICRO-PRM E / 2x 600 15° E 24 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.432E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.432E.24-en-x-line-slight-spots-l-down-led-3900-micro-prm-e-2x-600-15-e-24-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-MICRO-PRM-E-2X-600-15-E-24-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 MICRO-PRM E / 2x 600 15° E 34 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.431E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.431E.34-en-x-line-slight-spots-l-down-led-3900-micro-prm-e-2x-600-15-e-34-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-MICRO-PRM-E-2X-600-15-E-34-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 MICRO-PRM E / 2x 600 15° E 34 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.432E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.432E.34-en-x-line-slight-spots-l-down-led-3900-micro-prm-e-2x-600-15-e-34-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-MICRO-PRM-E-2X-600-15-E-34-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 MICRO-PRM EDD / 2x 600 15° EDD 04 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.431F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.431F.04-en-x-line-slight-spots-l-down-led-3900-micro-prm-edd-2x-600-15-edd-04-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-MICRO-PRM-EDD-2X-600-15-EDD-04-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 MICRO-PRM EDD / 2x 600 15° EDD 04 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.432F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.432F.04-en-x-line-slight-spots-l-down-led-3900-micro-prm-edd-2x-600-15-edd-04-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-MICRO-PRM-EDD-2X-600-15-EDD-04-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 MICRO-PRM EDD / 2x 600 15° EDD 24 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.431F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.431F.24-en-x-line-slight-spots-l-down-led-3900-micro-prm-edd-2x-600-15-edd-24-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-MICRO-PRM-EDD-2X-600-15-EDD-24-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 MICRO-PRM EDD / 2x 600 15° EDD 24 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.432F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.432F.24-en-x-line-slight-spots-l-down-led-3900-micro-prm-edd-2x-600-15-edd-24-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-MICRO-PRM-EDD-2X-600-15-EDD-24-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 MICRO-PRM EDD / 2x 600 15° EDD 34 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.431F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.431F.34-en-x-line-slight-spots-l-down-led-3900-micro-prm-edd-2x-600-15-edd-34-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-MICRO-PRM-EDD-2X-600-15-EDD-34-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 MICRO-PRM EDD / 2x 600 15° EDD 34 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.432F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.432F.34-en-x-line-slight-spots-l-down-led-3900-micro-prm-edd-2x-600-15-edd-34-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-MICRO-PRM-EDD-2X-600-15-EDD-34-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 PLX E / 2x 600 15° E 04 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.331E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.331E.04-en-x-line-slight-spots-l-down-led-3900-plx-e-2x-600-15-e-04-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-PLX-E-2X-600-15-E-04-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 PLX E / 2x 600 15° E 04 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.332E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.332E.04-en-x-line-slight-spots-l-down-led-3900-plx-e-2x-600-15-e-04-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-PLX-E-2X-600-15-E-04-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 PLX E / 2x 600 15° E 24 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.331E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.331E.24-en-x-line-slight-spots-l-down-led-3900-plx-e-2x-600-15-e-24-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-PLX-E-2X-600-15-E-24-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 PLX E / 2x 600 15° E 24 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.332E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.332E.24-en-x-line-slight-spots-l-down-led-3900-plx-e-2x-600-15-e-24-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-PLX-E-2X-600-15-E-24-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 PLX E / 2x 600 15° E 34 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.331E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.331E.34-en-x-line-slight-spots-l-down-led-3900-plx-e-2x-600-15-e-34-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-PLX-E-2X-600-15-E-34-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 PLX E / 2x 600 15° E 34 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.332E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.332E.34-en-x-line-slight-spots-l-down-led-3900-plx-e-2x-600-15-e-34-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-PLX-E-2X-600-15-E-34-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 PLX EDD / 2x 600 15° EDD 04 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.331F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.331F.04-en-x-line-slight-spots-l-down-led-3900-plx-edd-2x-600-15-e-04-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-PLX-EDD-2X-600-15-EDD-04-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 PLX EDD / 2x 600 15° EDD 04 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.332F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.332F.04-en-x-line-slight-spots-l-down-led-3900-plx-edd-2x-600-15-e-04-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-PLX-EDD-2X-600-15-EDD-04-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 PLX EDD / 2x 600 15° EDD 24 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.331F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.331F.24-en-x-line-slight-spots-l-down-led-3900-plx-edd-2x-600-15-e-24-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-PLX-EDD-2X-600-15-EDD-24-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 PLX EDD / 2x 600 15° EDD 24 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.332F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.332F.24-en-x-line-slight-spots-l-down-led-3900-plx-edd-2x-600-15-e-24-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-PLX-EDD-2X-600-15-EDD-24-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 PLX EDD / 2x 600 15° EDD 34 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.331F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.331F.34-en-x-line-slight-spots-l-down-led-3900-plx-edd-2x-600-15-e-34-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-PLX-EDD-2X-600-15-EDD-34-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 3900 PLX EDD / 2x 600 15° EDD 34 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.332F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.332F.34-en-x-line-slight-spots-l-down-led-3900-plx-edd-2x-600-15-e-34-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-3900-PLX-EDD-2X-600-15-EDD-34-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 MICRO-PRM E / 2x 600 15° E 04 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.221E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.221E.04-en-x-line-slight-spots-l-down-led-4400-micro-prm-e-2x-600-15-e-04-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-MICRO-PRM-E-2X-600-15-E-04-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 MICRO-PRM E / 2x 600 15° E 04 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.222E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.222E.04-en-x-line-slight-spots-l-down-led-4400-micro-prm-e-2x-600-15-e-04-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-MICRO-PRM-E-2X-600-15-E-04-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 MICRO-PRM E / 2x 600 15° E 24 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.221E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.221E.24-en-x-line-slight-spots-l-down-led-4400-micro-prm-e-2x-600-15-e-24-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-MICRO-PRM-E-2X-600-15-E-24-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 MICRO-PRM E / 2x 600 15° E 24 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.222E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.222E.24-en-x-line-slight-spots-l-down-led-4400-micro-prm-e-2x-600-15-e-24-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-MICRO-PRM-E-2X-600-15-E-24-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 MICRO-PRM E / 2x 600 15° E 34 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.221E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.221E.34-en-x-line-slight-spots-l-down-led-4400-micro-prm-e-2x-600-15-e-34-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-MICRO-PRM-E-2X-600-15-E-34-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 MICRO-PRM E / 2x 600 15° E 34 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.222E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.222E.34-en-x-line-slight-spots-l-down-led-4400-micro-prm-e-2x-600-15-e-34-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-MICRO-PRM-E-2X-600-15-E-34-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 MICRO-PRM EDD / 2x 600 15° EDD 04 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.221F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.221F.04-en-x-line-slight-spots-l-down-led-4400-micro-prm-edd-2x-600-15-edd-04-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-MICRO-PRM-EDD-2X-600-15-EDD-04-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 MICRO-PRM EDD / 2x 600 15° EDD 04 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.222F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.222F.04-en-x-line-slight-spots-l-down-led-4400-micro-prm-edd-2x-600-15-edd-04-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-MICRO-PRM-EDD-2X-600-15-EDD-04-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 MICRO-PRM EDD / 2x 600 15° EDD 24 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.221F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.221F.24-en-x-line-slight-spots-l-down-led-4400-micro-prm-edd-2x-600-15-edd-24-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-MICRO-PRM-EDD-2X-600-15-EDD-24-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 MICRO-PRM EDD / 2x 600 15° EDD 24 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.222F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.222F.24-en-x-line-slight-spots-l-down-led-4400-micro-prm-edd-2x-600-15-edd-24-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-MICRO-PRM-EDD-2X-600-15-EDD-24-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 MICRO-PRM EDD / 2x 600 15° EDD 34 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.221F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.221F.34-en-x-line-slight-spots-l-down-led-4400-micro-prm-edd-2x-600-15-edd-34-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-MICRO-PRM-EDD-2X-600-15-EDD-34-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 MICRO-PRM EDD / 2x 600 15° EDD 34 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.222F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.222F.34-en-x-line-slight-spots-l-down-led-4400-micro-prm-edd-2x-600-15-edd-34-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-MICRO-PRM-EDD-2X-600-15-EDD-34-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 PLX E / 2x 600 15° E 04 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.121E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.121E.04-en-x-line-slight-spots-l-down-led-4400-plx-e-2x-600-15-e-04-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-PLX-E-2X-600-15-E-04-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 PLX E / 2x 600 15° E 04 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.122E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.122E.04-en-x-line-slight-spots-l-down-led-4400-plx-e-2x-600-15-e-04-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-PLX-E-2X-600-15-E-04-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 PLX E / 2x 600 15° E 24 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.121E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.121E.24-en-x-line-slight-spots-l-down-led-4400-plx-e-2x-600-15-e-24-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-PLX-E-2X-600-15-E-24-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 PLX E / 2x 600 15° E 24 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.122E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.122E.24-en-x-line-slight-spots-l-down-led-4400-plx-e-2x-600-15-e-24-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-PLX-E-2X-600-15-E-24-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 PLX E / 2x 600 15° E 34 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.121E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.121E.34-en-x-line-slight-spots-l-down-led-4400-plx-e-2x-600-15-e-34-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-PLX-E-2X-600-15-E-34-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 PLX E / 2x 600 15° E 34 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.122E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.122E.34-en-x-line-slight-spots-l-down-led-4400-plx-e-2x-600-15-e-34-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-PLX-E-2X-600-15-E-34-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 PLX EDD / 2x 600 15° EDD 04 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.121F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.121F.04-en-x-line-slight-spots-l-down-led-4400-plx-e-2x-600-15-edd-04-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-PLX-EDD-2X-600-15-EDD-04-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 PLX EDD / 2x 600 15° EDD 04 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.122F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.122F.04-en-x-line-slight-spots-l-down-led-4400-plx-e-2x-600-15-edd-04-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-PLX-EDD-2X-600-15-EDD-04-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 PLX EDD / 2x 600 15° EDD 24 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.121F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.121F.24-en-x-line-slight-spots-l-down-led-4400-plx-e-2x-600-15-edd-24-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-PLX-EDD-2X-600-15-EDD-24-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 PLX EDD / 2x 600 15° EDD 24 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.122F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.122F.24-en-x-line-slight-spots-l-down-led-4400-plx-e-2x-600-15-edd-24-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-PLX-EDD-2X-600-15-EDD-24-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 PLX EDD / 2x 600 15° EDD 34 830 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.121F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.121F.34-en-x-line-slight-spots-l-down-led-4400-plx-e-2x-600-15-edd-34-830-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-PLX-EDD-2X-600-15-EDD-34-830-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 4400 PLX EDD / 2x 600 15° EDD 34 840 / L-1162MM S-1,5M TWO CIRCUIT;19.4398.122F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1162 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.122F.34-en-x-line-slight-spots-l-down-led-4400-plx-e-2x-600-15-edd-34-840-l-1162mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-4400-PLX-EDD-2X-600-15-EDD-34-840-L-1162MM-S-15M-TWO-CIRCUIT.zip;1162;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 MICRO-PRM E / 2x 600 15° E 04 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.651E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.651E.04-en-x-line-slight-spots-l-down-led-5200-micro-prm-e-2x-600-15-e-04-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-MICRO-PRM-E-2X-600-15-E-04-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 MICRO-PRM E / 2x 600 15° E 04 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.652E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.652E.04-en-x-line-slight-spots-l-down-led-5200-micro-prm-e-2x-600-15-e-04-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-MICRO-PRM-E-2X-600-15-E-04-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 MICRO-PRM E / 2x 600 15° E 24 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.651E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.651E.24-en-x-line-slight-spots-l-down-led-5200-micro-prm-e-2x-600-15-e-24-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-MICRO-PRM-E-2X-600-15-E-24-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 MICRO-PRM E / 2x 600 15° E 24 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.652E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.652E.24-en-x-line-slight-spots-l-down-led-5200-micro-prm-e-2x-600-15-e-24-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-MICRO-PRM-E-2X-600-15-E-24-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 MICRO-PRM E / 2x 600 15° E 34 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.651E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.651E.34-en-x-line-slight-spots-l-down-led-5200-micro-prm-e-2x-600-15-e-34-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-MICRO-PRM-E-2X-600-15-E-34-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 MICRO-PRM E / 2x 600 15° E 34 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.652E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.652E.34-en-x-line-slight-spots-l-down-led-5200-micro-prm-e-2x-600-15-e-34-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-MICRO-PRM-E-2X-600-15-E-34-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 MICRO-PRM EDD / 2x 600 15° EDD 04 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.651F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.651F.04-en-x-line-slight-spots-l-down-led-5200-micro-prm-edd-2x-600-15-edd-04-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-MICRO-PRM-EDD-2X-600-15-EDD-04-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 MICRO-PRM EDD / 2x 600 15° EDD 04 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.652F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.652F.04-en-x-line-slight-spots-l-down-led-5200-micro-prm-edd-2x-600-15-edd-04-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-MICRO-PRM-EDD-2X-600-15-EDD-04-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 MICRO-PRM EDD / 2x 600 15° EDD 24 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.651F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.651F.24-en-x-line-slight-spots-l-down-led-5200-micro-prm-edd-2x-600-15-edd-24-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-MICRO-PRM-EDD-2X-600-15-EDD-24-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 MICRO-PRM EDD / 2x 600 15° EDD 24 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.652F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.652F.24-en-x-line-slight-spots-l-down-led-5200-micro-prm-edd-2x-600-15-edd-24-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-MICRO-PRM-EDD-2X-600-15-EDD-24-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 MICRO-PRM EDD / 2x 600 15° EDD 34 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.651F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.651F.34-en-x-line-slight-spots-l-down-led-5200-micro-prm-edd-2x-600-15-edd-34-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-MICRO-PRM-EDD-2X-600-15-EDD-34-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 MICRO-PRM EDD / 2x 600 15° EDD 34 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.652F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.652F.34-en-x-line-slight-spots-l-down-led-5200-micro-prm-edd-2x-600-15-edd-34-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-MICRO-PRM-EDD-2X-600-15-EDD-34-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 PLX E / 2x 600 15° E 04 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.551E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.551E.04-en-x-line-slight-spots-l-down-led-5200-plx-e-2x-600-15-e-04-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-PLX-E-2X-600-15-E-04-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 PLX E / 2x 600 15° E 04 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.552E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.552E.04-en-x-line-slight-spots-l-down-led-5200-plx-e-2x-600-15-e-04-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-PLX-E-2X-600-15-E-04-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 PLX E / 2x 600 15° E 24 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.551E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.551E.24-en-x-line-slight-spots-l-down-led-5200-plx-e-2x-600-15-e-24-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-PLX-E-2X-600-15-E-24-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 PLX E / 2x 600 15° E 24 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.552E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.552E.24-en-x-line-slight-spots-l-down-led-5200-plx-e-2x-600-15-e-24-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-PLX-E-2X-600-15-E-24-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 PLX E / 2x 600 15° E 34 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.551E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.551E.34-en-x-line-slight-spots-l-down-led-5200-plx-e-2x-600-15-e-34-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-PLX-E-2X-600-15-E-34-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 PLX E / 2x 600 15° E 34 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.552E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.552E.34-en-x-line-slight-spots-l-down-led-5200-plx-e-2x-600-15-e-34-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-PLX-E-2X-600-15-E-34-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 PLX EDD / 2x 600 15° EDD 04 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.551F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.551F.04-en-x-line-slight-spots-l-down-led-5200-plx-edd-2x-600-15-edd-04-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-PLX-EDD-2X-600-15-EDD-04-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 PLX EDD / 2x 600 15° EDD 04 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.552F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.552F.04-en-x-line-slight-spots-l-down-led-5200-plx-edd-2x-600-15-edd-04-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-PLX-EDD-2X-600-15-EDD-04-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 PLX EDD / 2x 600 15° EDD 24 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.551F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.551F.24-en-x-line-slight-spots-l-down-led-5200-plx-edd-2x-600-15-edd-24-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-PLX-EDD-2X-600-15-EDD-24-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 PLX EDD / 2x 600 15° EDD 24 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.552F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.552F.24-en-x-line-slight-spots-l-down-led-5200-plx-edd-2x-600-15-edd-24-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-PLX-EDD-2X-600-15-EDD-24-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 PLX EDD / 2x 600 15° EDD 34 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.551F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.551F.34-en-x-line-slight-spots-l-down-led-5200-plx-edd-2x-600-15-edd-34-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-PLX-EDD-2X-600-15-EDD-34-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 5200 PLX EDD / 2x 600 15° EDD 34 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.552F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.552F.34-en-x-line-slight-spots-l-down-led-5200-plx-edd-2x-600-15-edd-34-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-5200-PLX-EDD-2X-600-15-EDD-34-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 MICRO-PRM E / 2x 600 15° E 04 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.441E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.441E.04-en-x-line-slight-spots-l-down-led-6600-micro-prm-e-2x-600-15-e-04-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-MICRO-PRM-E-2X-600-15-E-04-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 MICRO-PRM E / 2x 600 15° E 04 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.442E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.442E.04-en-x-line-slight-spots-l-down-led-6600-micro-prm-e-2x-600-15-e-04-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-MICRO-PRM-E-2X-600-15-E-04-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 MICRO-PRM E / 2x 600 15° E 24 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.441E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.441E.24-en-x-line-slight-spots-l-down-led-6600-micro-prm-e-2x-600-15-e-24-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-MICRO-PRM-E-2X-600-15-E-24-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 MICRO-PRM E / 2x 600 15° E 24 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.442E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.442E.24-en-x-line-slight-spots-l-down-led-6600-micro-prm-e-2x-600-15-e-24-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-MICRO-PRM-E-2X-600-15-E-24-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 MICRO-PRM E / 2x 600 15° E 34 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.441E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.441E.34-en-x-line-slight-spots-l-down-led-6600-micro-prm-e-2x-600-15-e-34-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-MICRO-PRM-E-2X-600-15-E-34-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 MICRO-PRM E / 2x 600 15° E 34 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.442E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.442E.34-en-x-line-slight-spots-l-down-led-6600-micro-prm-e-2x-600-15-e-34-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-MICRO-PRM-E-2X-600-15-E-34-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 MICRO-PRM EDD / 2x 600 15° EDD 04 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.441F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.441F.04-en-x-line-slight-spots-l-down-led-6600-micro-prm-edd-2x-600-15-edd-04-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-MICRO-PRM-EDD-2X-600-15-EDD-04-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 MICRO-PRM EDD / 2x 600 15° EDD 04 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.442F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.442F.04-en-x-line-slight-spots-l-down-led-6600-micro-prm-edd-2x-600-15-edd-04-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-MICRO-PRM-EDD-2X-600-15-EDD-04-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 MICRO-PRM EDD / 2x 600 15° EDD 24 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.441F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.441F.24-en-x-line-slight-spots-l-down-led-6600-micro-prm-edd-2x-600-15-edd-24-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-MICRO-PRM-EDD-2X-600-15-EDD-24-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 MICRO-PRM EDD / 2x 600 15° EDD 24 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.442F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.442F.24-en-x-line-slight-spots-l-down-led-6600-micro-prm-edd-2x-600-15-edd-24-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-MICRO-PRM-EDD-2X-600-15-EDD-24-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 MICRO-PRM EDD / 2x 600 15° EDD 34 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.441F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.441F.34-en-x-line-slight-spots-l-down-led-6600-micro-prm-edd-2x-600-15-edd-34-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-MICRO-PRM-EDD-2X-600-15-EDD-34-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 MICRO-PRM EDD / 2x 600 15° EDD 34 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.442F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.442F.34-en-x-line-slight-spots-l-down-led-6600-micro-prm-edd-2x-600-15-edd-34-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-MICRO-PRM-EDD-2X-600-15-EDD-34-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 PLX E / 2x 600 15° E 04 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.341E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.341E.04-en-x-line-slight-spots-l-down-led-6600-plx-e-2x-600-15-e-04-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-PLX-E-2X-600-15-E-04-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 PLX E / 2x 600 15° E 04 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.342E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.342E.04-en-x-line-slight-spots-l-down-led-6600-plx-e-2x-600-15-e-04-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-PLX-E-2X-600-15-E-04-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 PLX E / 2x 600 15° E 24 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.341E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.341E.24-en-x-line-slight-spots-l-down-led-6600-plx-e-2x-600-15-e-24-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-PLX-E-2X-600-15-E-24-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 PLX E / 2x 600 15° E 24 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.342E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.342E.24-en-x-line-slight-spots-l-down-led-6600-plx-e-2x-600-15-e-24-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-PLX-E-2X-600-15-E-24-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 PLX E / 2x 600 15° E 34 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.341E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.341E.34-en-x-line-slight-spots-l-down-led-6600-plx-e-2x-600-15-e-34-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-PLX-E-2X-600-15-E-34-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 PLX E / 2x 600 15° E 34 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.342E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.342E.34-en-x-line-slight-spots-l-down-led-6600-plx-e-2x-600-15-e-34-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-PLX-E-2X-600-15-E-34-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 PLX EDD / 2x 600 15° EDD 04 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.341F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.341F.04-en-x-line-slight-spots-l-down-led-6600-plx-edd-2x-600-15-e-04-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-PLX-EDD-2X-600-15-EDD-04-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 PLX EDD / 2x 600 15° EDD 04 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.342F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.342F.04-en-x-line-slight-spots-l-down-led-6600-plx-edd-2x-600-15-e-04-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-PLX-EDD-2X-600-15-EDD-04-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 PLX EDD / 2x 600 15° EDD 24 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.341F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.341F.24-en-x-line-slight-spots-l-down-led-6600-plx-edd-2x-600-15-e-24-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-PLX-EDD-2X-600-15-EDD-24-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 PLX EDD / 2x 600 15° EDD 24 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.342F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.342F.24-en-x-line-slight-spots-l-down-led-6600-plx-edd-2x-600-15-e-24-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-PLX-EDD-2X-600-15-EDD-24-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 PLX EDD / 2x 600 15° EDD 34 830 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.341F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.341F.34-en-x-line-slight-spots-l-down-led-6600-plx-edd-2x-600-15-e-34-830-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-PLX-EDD-2X-600-15-EDD-34-830-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 6600 PLX EDD / 2x 600 15° EDD 34 840 / L-1723MM S-1,5M TWO CIRCUIT;19.4398.342F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;1723 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.342F.34-en-x-line-slight-spots-l-down-led-6600-plx-edd-2x-600-15-e-34-840-l-1723mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-6600-PLX-EDD-2X-600-15-EDD-34-840-L-1723MM-S-15M-TWO-CIRCUIT.zip;1723;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 MICRO-PRM E / 2x 600 15° E 04 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.661E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.661E.04-en-x-line-slight-spots-l-down-led-8800-micro-prm-e-2x-600-15-e-04-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-MICRO-PRM-E-2X-600-15-E-04-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 MICRO-PRM E / 2x 600 15° E 04 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.662E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.662E.04-en-x-line-slight-spots-l-down-led-8800-micro-prm-e-2x-600-15-e-04-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-MICRO-PRM-E-2X-600-15-E-04-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 MICRO-PRM E / 2x 600 15° E 24 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.661E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.661E.24-en-x-line-slight-spots-l-down-led-8800-micro-prm-e-2x-600-15-e-24-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-MICRO-PRM-E-2X-600-15-E-24-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 MICRO-PRM E / 2x 600 15° E 24 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.662E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.662E.24-en-x-line-slight-spots-l-down-led-8800-micro-prm-e-2x-600-15-e-24-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-MICRO-PRM-E-2X-600-15-E-24-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 MICRO-PRM E / 2x 600 15° E 34 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.661E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.661E.34-en-x-line-slight-spots-l-down-led-8800-micro-prm-e-2x-600-15-e-34-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-MICRO-PRM-E-2X-600-15-E-34-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 MICRO-PRM E / 2x 600 15° E 34 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.662E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.662E.34-en-x-line-slight-spots-l-down-led-8800-micro-prm-e-2x-600-15-e-34-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-MICRO-PRM-E-2X-600-15-E-34-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 MICRO-PRM EDD / 2x 600 15° EDD 04 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.661F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.661F.04-en-x-line-slight-spots-l-down-led-8800-micro-prm-edd-2x-600-15-edd-04-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-MICRO-PRM-EDD-2X-600-15-EDD-04-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 MICRO-PRM EDD / 2x 600 15° EDD 04 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.662F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.662F.04-en-x-line-slight-spots-l-down-led-8800-micro-prm-edd-2x-600-15-edd-04-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-MICRO-PRM-EDD-2X-600-15-EDD-04-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 MICRO-PRM EDD / 2x 600 15° EDD 24 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.661F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.661F.24-en-x-line-slight-spots-l-down-led-8800-micro-prm-edd-2x-600-15-edd-24-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-MICRO-PRM-EDD-2X-600-15-EDD-24-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 MICRO-PRM EDD / 2x 600 15° EDD 24 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.662F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.662F.24-en-x-line-slight-spots-l-down-led-8800-micro-prm-edd-2x-600-15-edd-24-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-MICRO-PRM-EDD-2X-600-15-EDD-24-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 MICRO-PRM EDD / 2x 600 15° EDD 34 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.661F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.661F.34-en-x-line-slight-spots-l-down-led-8800-micro-prm-edd-2x-600-15-edd-34-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-MICRO-PRM-EDD-2X-600-15-EDD-34-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 MICRO-PRM EDD / 2x 600 15° EDD 34 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.662F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 86,2° / 111° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.815008;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.662F.34-en-x-line-slight-spots-l-down-led-8800-micro-prm-edd-2x-600-15-edd-34-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-MICRO-PRM-EDD-2X-600-15-EDD-34-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 PLX E / 2x 600 15° E 04 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.561E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.561E.04-en-x-line-slight-spots-l-down-led-8800-plx-e-2x-600-15-e-04-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-PLX-E-2X-600-15-E-04-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 PLX E / 2x 600 15° E 04 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.562E.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.562E.04-en-x-line-slight-spots-l-down-led-8800-plx-e-2x-600-15-e-04-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-PLX-E-2X-600-15-E-04-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 PLX E / 2x 600 15° E 24 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.561E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.561E.24-en-x-line-slight-spots-l-down-led-8800-plx-e-2x-600-15-e-24-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-PLX-E-2X-600-15-E-24-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 PLX E / 2x 600 15° E 24 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.562E.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.562E.24-en-x-line-slight-spots-l-down-led-8800-plx-e-2x-600-15-e-24-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-PLX-E-2X-600-15-E-24-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 PLX E / 2x 600 15° E 34 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.561E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.561E.34-en-x-line-slight-spots-l-down-led-8800-plx-e-2x-600-15-e-34-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-PLX-E-2X-600-15-E-34-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 PLX E / 2x 600 15° E 34 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.562E.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E) / standard on/off (E);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.562E.34-en-x-line-slight-spots-l-down-led-8800-plx-e-2x-600-15-e-34-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-PLX-E-2X-600-15-E-34-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 PLX EDD / 2x 600 15° EDD 04 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.561F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.561F.04-en-x-line-slight-spots-l-down-led-8800-plx-edd-2x-600-15-edd-04-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-PLX-EDD-2X-600-15-EDD-04-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 PLX EDD / 2x 600 15° EDD 04 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.562F.04;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.562F.04-en-x-line-slight-spots-l-down-led-8800-plx-edd-2x-600-15-edd-04-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-PLX-EDD-2X-600-15-EDD-04-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 PLX EDD / 2x 600 15° EDD 24 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.561F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.561F.24-en-x-line-slight-spots-l-down-led-8800-plx-edd-2x-600-15-edd-24-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-PLX-EDD-2X-600-15-EDD-24-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 PLX EDD / 2x 600 15° EDD 24 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.562F.24;surface mounted on slings;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.562F.24-en-x-line-slight-spots-l-down-led-8800-plx-edd-2x-600-15-edd-24-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-PLX-EDD-2X-600-15-EDD-24-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 PLX EDD / 2x 600 15° EDD 34 830 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.561F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;3000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.561F.34-en-x-line-slight-spots-l-down-led-8800-plx-edd-2x-600-15-edd-34-830-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-PLX-EDD-2X-600-15-EDD-34-830-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;3000
X-LINE SLIGHT SPOTS L-DOWN LED 8800 PLX EDD / 2x 600 15° EDD 34 840 / L-2284MM S-1,5M TWO CIRCUIT;19.4398.562F.34;surface mounted on slings;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal) / optical system based on PMMA lenses;2284 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD) / DIM DALI (EDD);LED;5 ÷ 35;0;0;0;80000;L80/B10;4000;>80;3;(C0-C180) / (C90-C270) - 99,6° / 103° // (C0-C180) / (C90-C270) - 17,8° / 19,8°;IP40;IK04;I;RG0;0.755007;0;LUXIONA;https://luxiona.com/products/x-line-slight-spots-l-down-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4398.562F.34-en-x-line-slight-spots-l-down-led-8800-plx-edd-2x-600-15-edd-34-840-l-2284mm-s-15m-two-circuit.pdf;X-LINE-SLIGHT-SPOTS-L-DOWN-LED-8800-PLX-EDD-2X-600-15-EDD-34-840-L-2284MM-S-15M-TWO-CIRCUIT.zip;2284;34;68;230;4000
