;Assembly Code##OTHER##;Assembly##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Dimensions##OTHER##;Voltage (range)##OTHER##;Driver##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Power of luminaire##ELECTRICAL_WATTAGE##WATTS;Luminaire luminous flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Luminaire's light efficiency##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;Color of the light##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Efficiency##OTHER##;Power factor##OTHER##;Manufacturer##OTHER##;URL##OTHER##;Catalogue##OTHER## ;Photometric Web File##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 04 830 / L-800MM;19.4309.1111.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1111.04-en-x-line-slight-surface-low-ugr-led-1200-louver-e-04-830-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-04-830-L-800MM.ies;800;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 04 840 / L-800MM;19.4309.1121.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1121.04-en-x-line-slight-surface-low-ugr-led-1200-louver-e-04-840-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-04-840-L-800MM.ies;800;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 21 830 / L-800MM;19.4309.1111.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1111.21-en-x-line-slight-surface-low-ugr-led-1200-louver-e-21-830-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-21-830-L-800MM.ies;800;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 21 840 / L-800MM;19.4309.1121.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1121.21-en-x-line-slight-surface-low-ugr-led-1200-louver-e-21-840-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-21-840-L-800MM.ies;800;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 24 830 / L-800MM;19.4309.1111.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1111.24-en-x-line-slight-surface-low-ugr-led-1200-louver-e-24-830-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-24-830-L-800MM.ies;800;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 24 840 / L-800MM;19.4309.1121.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1121.24-en-x-line-slight-surface-low-ugr-led-1200-louver-e-24-840-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-24-840-L-800MM.ies;800;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 34 830 / L-800MM;19.4309.1111.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1111.34-en-x-line-slight-surface-low-ugr-led-1200-louver-e-34-830-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-34-830-L-800MM.ies;800;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 34 840 / L-800MM;19.4309.1121.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1121.34-en-x-line-slight-surface-low-ugr-led-1200-louver-e-34-840-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-34-840-L-800MM.ies;800;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 04 830 / L-800MM;19.4309.1113.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1113.04-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-04-830-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-04-830-L-800MM.ies;800;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 04 840 / L-800MM;19.4309.1123.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1123.04-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-04-840-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-04-840-L-800MM.ies;800;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 21 830 / L-800MM;19.4309.1113.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1113.21-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-21-830-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-21-830-L-800MM.ies;800;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 21 840 / L-800MM;19.4309.1123.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1123.21-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-21-840-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-21-840-L-800MM.ies;800;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 24 830 / L-800MM;19.4309.1113.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1113.24-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-24-830-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-24-830-L-800MM.ies;800;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 24 840 / L-800MM;19.4309.1123.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1123.24-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-24-840-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-24-840-L-800MM.ies;800;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 34 830 / L-800MM;19.4309.1113.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1113.34-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-34-830-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-34-830-L-800MM.ies;800;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 34 840 / L-800MM;19.4309.1123.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1123.34-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-34-840-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-34-840-L-800MM.ies;800;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 04 830 / L-1200MM;19.4309.2311.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2311.04-en-x-line-slight-surface-low-ugr-led-1800-louver-e-04-830-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-04-830-L-1200MM.ies;1200;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 04 840 / L-1200MM;19.4309.2321.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2321.04-en-x-line-slight-surface-low-ugr-led-1800-louver-e-04-840-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-04-840-L-1200MM.ies;1200;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 21 830 / L-1200MM;19.4309.2311.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2311.21-en-x-line-slight-surface-low-ugr-led-1800-louver-e-21-830-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-21-830-L-1200MM.ies;1200;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 21 840 / L-1200MM;19.4309.2321.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2321.21-en-x-line-slight-surface-low-ugr-led-1800-louver-e-21-840-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-21-840-L-1200MM.ies;1200;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 24 830 / L-1200MM;19.4309.2311.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2311.24-en-x-line-slight-surface-low-ugr-led-1800-louver-e-24-830-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-24-830-L-1200MM.ies;1200;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 24 840 / L-1200MM;19.4309.2321.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2321.24-en-x-line-slight-surface-low-ugr-led-1800-louver-e-24-840-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-24-840-L-1200MM.ies;1200;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 34 830 / L-1200MM;19.4309.2311.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2311.34-en-x-line-slight-surface-low-ugr-led-1800-louver-e-34-830-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-34-830-L-1200MM.ies;1200;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 34 840 / L-1200MM;19.4309.2321.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2321.34-en-x-line-slight-surface-low-ugr-led-1800-louver-e-34-840-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-34-840-L-1200MM.ies;1200;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 04 830 / L-1200MM;19.4309.2313.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2313.04-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-04-830-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-04-830-L-1200MM.ies;1200;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 04 840 / L-1200MM;19.4309.2323.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2323.04-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-04-840-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-04-840-L-1200MM.ies;1200;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 21 830 / L-1200MM;19.4309.2313.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2313.21-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-21-830-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-21-830-L-1200MM.ies;1200;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 21 840 / L-1200MM;19.4309.2323.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2323.21-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-21-840-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-21-840-L-1200MM.ies;1200;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 24 830 / L-1200MM;19.4309.2313.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2313.24-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-24-830-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-24-830-L-1200MM.ies;1200;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 24 840 / L-1200MM;19.4309.2323.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2323.24-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-24-840-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-24-840-L-1200MM.ies;1200;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 34 830 / L-1200MM;19.4309.2313.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2313.34-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-34-830-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-34-830-L-1200MM.ies;1200;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 34 840 / L-1200MM;19.4309.2323.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2323.34-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-34-840-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-34-840-L-1200MM.ies;1200;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 04 830 / L-800MM;19.4309.1211.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1211.04-en-x-line-slight-surface-low-ugr-led-2000-louver-e-04-830-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-04-830-L-800MM.ies;800;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 04 840 / L-800MM;19.4309.1221.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1221.04-en-x-line-slight-surface-low-ugr-led-2000-louver-e-04-840-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-04-840-L-800MM.ies;800;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 21 830 / L-800MM;19.4309.1211.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1211.21-en-x-line-slight-surface-low-ugr-led-2000-louver-e-21-830-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-21-830-L-800MM.ies;800;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 21 840 / L-800MM;19.4309.1221.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1221.21-en-x-line-slight-surface-low-ugr-led-2000-louver-e-21-840-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-21-840-L-800MM.ies;800;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 24 830 / L-800MM;19.4309.1211.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1211.24-en-x-line-slight-surface-low-ugr-led-2000-louver-e-24-830-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-24-830-L-800MM.ies;800;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 24 840 / L-800MM;19.4309.1221.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1221.24-en-x-line-slight-surface-low-ugr-led-2000-louver-e-24-840-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-24-840-L-800MM.ies;800;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 34 830 / L-800MM;19.4309.1211.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1211.34-en-x-line-slight-surface-low-ugr-led-2000-louver-e-34-830-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-34-830-L-800MM.ies;800;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 34 840 / L-800MM;19.4309.1221.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1221.34-en-x-line-slight-surface-low-ugr-led-2000-louver-e-34-840-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-34-840-L-800MM.ies;800;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 04 830 / L-800MM;19.4309.1213.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1213.04-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-04-830-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-04-830-L-800MM.ies;800;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 04 840 / L-800MM;19.4309.1223.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1223.04-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-04-840-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-04-840-L-800MM.ies;800;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 21 830 / L-800MM;19.4309.1213.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1213.21-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-21-830-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-21-830-L-800MM.ies;800;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 21 840 / L-800MM;19.4309.1223.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1223.21-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-21-840-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-21-840-L-800MM.ies;800;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 24 830 / L-800MM;19.4309.1213.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1213.24-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-24-830-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-24-830-L-800MM.ies;800;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 24 840 / L-800MM;19.4309.1223.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1223.24-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-24-840-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-24-840-L-800MM.ies;800;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 34 830 / L-800MM;19.4309.1213.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1213.34-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-34-830-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-34-830-L-800MM.ies;800;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 34 840 / L-800MM;19.4309.1223.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);800 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.1223.34-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-34-840-l-800mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-34-840-L-800MM.ies;800;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 04 830 / L-1600MM;19.4309.3511.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3511.04-en-x-line-slight-surface-low-ugr-led-2400-louver-e-04-830-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-04-830-L-1600MM.ies;1600;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 04 840 / L-1600MM;19.4309.3521.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3521.04-en-x-line-slight-surface-low-ugr-led-2400-louver-e-04-840-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-04-840-L-1600MM.ies;1600;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 21 830 / L-1600MM;19.4309.3511.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3511.21-en-x-line-slight-surface-low-ugr-led-2400-louver-e-21-830-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-21-830-L-1600MM.ies;1600;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 21 840 / L-1600MM;19.4309.3521.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3521.21-en-x-line-slight-surface-low-ugr-led-2400-louver-e-21-840-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-21-840-L-1600MM.ies;1600;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 24 830 / L-1600MM;19.4309.3511.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3511.24-en-x-line-slight-surface-low-ugr-led-2400-louver-e-24-830-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-24-830-L-1600MM.ies;1600;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 24 840 / L-1600MM;19.4309.3521.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3521.24-en-x-line-slight-surface-low-ugr-led-2400-louver-e-24-840-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-24-840-L-1600MM.ies;1600;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 34 830 / L-1600MM;19.4309.3511.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3511.34-en-x-line-slight-surface-low-ugr-led-2400-louver-e-34-830-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-34-830-L-1600MM.ies;1600;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 34 840 / L-1600MM;19.4309.3521.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3521.34-en-x-line-slight-surface-low-ugr-led-2400-louver-e-34-840-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-34-840-L-1600MM.ies;1600;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 04 830 / L-1600MM;19.4309.3513.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3513.04-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-04-830-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-04-830-L-1600MM.ies;1600;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 04 840 / L-1600MM;19.4309.3523.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3523.04-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-04-840-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-04-840-L-1600MM.ies;1600;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 21 830 / L-1600MM;19.4309.3513.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3513.21-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-21-830-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-21-830-L-1600MM.ies;1600;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 21 840 / L-1600MM;19.4309.3523.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3523.21-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-21-840-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-21-840-L-1600MM.ies;1600;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 24 830 / L-1600MM;19.4309.3513.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3513.24-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-24-830-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-24-830-L-1600MM.ies;1600;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 24 840 / L-1600MM;19.4309.3523.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3523.24-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-24-840-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-24-840-L-1600MM.ies;1600;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 34 830 / L-1600MM;19.4309.3513.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3513.34-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-34-830-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-34-830-L-1600MM.ies;1600;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 34 840 / L-1600MM;19.4309.3523.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3523.34-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-34-840-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-34-840-L-1600MM.ies;1600;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 04 830 / L-1200MM;19.4309.2411.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2411.04-en-x-line-slight-surface-low-ugr-led-3000-louver-e-04-830-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-04-830-L-1200MM.ies;1200;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 04 830 / L-2000MM;19.4309.4411.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4411.04-en-x-line-slight-surface-low-ugr-led-3000-louver-e-04-830-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-04-830-L-2000MM.ies;2000;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 04 840 / L-1200MM;19.4309.2421.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2421.04-en-x-line-slight-surface-low-ugr-led-3000-louver-e-04-840-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-04-840-L-1200MM.ies;1200;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 04 840 / L-2000MM;19.4309.4421.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4421.04-en-x-line-slight-surface-low-ugr-led-3000-louver-e-04-840-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-04-840-L-2000MM.ies;2000;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 21 830 / L-1200MM;19.4309.2411.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2411.21-en-x-line-slight-surface-low-ugr-led-3000-louver-e-21-830-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-21-830-L-1200MM.ies;1200;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 21 830 / L-2000MM;19.4309.4411.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4411.21-en-x-line-slight-surface-low-ugr-led-3000-louver-e-21-830-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-21-830-L-2000MM.ies;2000;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 21 840 / L-1200MM;19.4309.2421.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2421.21-en-x-line-slight-surface-low-ugr-led-3000-louver-e-21-840-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-21-840-L-1200MM.ies;1200;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 21 840 / L-2000MM;19.4309.4421.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4421.21-en-x-line-slight-surface-low-ugr-led-3000-louver-e-21-840-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-21-840-L-2000MM.ies;2000;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 24 830 / L-1200MM;19.4309.2411.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2411.24-en-x-line-slight-surface-low-ugr-led-3000-louver-e-24-830-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-24-830-L-1200MM.ies;1200;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 24 830 / L-2000MM;19.4309.4411.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4411.24-en-x-line-slight-surface-low-ugr-led-3000-louver-e-24-830-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-24-830-L-2000MM.ies;2000;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 24 840 / L-1200MM;19.4309.2421.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2421.24-en-x-line-slight-surface-low-ugr-led-3000-louver-e-24-840-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-24-840-L-1200MM.ies;1200;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 24 840 / L-2000MM;19.4309.4421.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4421.24-en-x-line-slight-surface-low-ugr-led-3000-louver-e-24-840-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-24-840-L-2000MM.ies;2000;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 34 830 / L-1200MM;19.4309.2411.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2411.34-en-x-line-slight-surface-low-ugr-led-3000-louver-e-34-830-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-34-830-L-1200MM.ies;1200;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 34 830 / L-2000MM;19.4309.4411.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4411.34-en-x-line-slight-surface-low-ugr-led-3000-louver-e-34-830-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-34-830-L-2000MM.ies;2000;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 34 840 / L-1200MM;19.4309.2421.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2421.34-en-x-line-slight-surface-low-ugr-led-3000-louver-e-34-840-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-34-840-L-1200MM.ies;1200;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 34 840 / L-2000MM;19.4309.4421.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4421.34-en-x-line-slight-surface-low-ugr-led-3000-louver-e-34-840-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-34-840-L-2000MM.ies;2000;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 04 830 / L-1200MM;19.4309.2413.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2413.04-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-04-830-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-04-830-L-1200MM.ies;1200;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 04 830 / L-2000MM;19.4309.4413.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4413.04-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-04-830-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-04-830-L-2000MM.ies;2000;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 04 840 / L-1200MM;19.4309.2423.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2423.04-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-04-840-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-04-840-L-1200MM.ies;1200;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 04 840 / L-2000MM;19.4309.4423.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4423.04-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-04-840-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-04-840-L-2000MM.ies;2000;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 21 830 / L-1200MM;19.4309.2413.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2413.21-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-21-830-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-21-830-L-1200MM.ies;1200;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 21 830 / L-2000MM;19.4309.4413.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4413.21-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-21-830-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-21-830-L-2000MM.ies;2000;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 21 840 / L-1200MM;19.4309.2423.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2423.21-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-21-840-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-21-840-L-1200MM.ies;1200;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 21 840 / L-2000MM;19.4309.4423.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4423.21-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-21-840-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-21-840-L-2000MM.ies;2000;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 24 830 / L-1200MM;19.4309.2413.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2413.24-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-24-830-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-24-830-L-1200MM.ies;1200;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 24 830 / L-2000MM;19.4309.4413.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4413.24-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-24-830-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-24-830-L-2000MM.ies;2000;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 24 840 / L-1200MM;19.4309.2423.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2423.24-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-24-840-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-24-840-L-1200MM.ies;1200;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 24 840 / L-2000MM;19.4309.4423.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4423.24-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-24-840-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-24-840-L-2000MM.ies;2000;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 34 830 / L-1200MM;19.4309.2413.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2413.34-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-34-830-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-34-830-L-1200MM.ies;1200;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 34 830 / L-2000MM;19.4309.4413.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4413.34-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-34-830-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-34-830-L-2000MM.ies;2000;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 34 840 / L-1200MM;19.4309.2423.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1200 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.2423.34-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-34-840-l-1200mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-34-840-L-1200MM.ies;1200;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 34 840 / L-2000MM;19.4309.4423.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4423.34-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-34-840-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-34-840-L-2000MM.ies;2000;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 04 830 / L-1600MM;19.4309.3611.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3611.04-en-x-line-slight-surface-low-ugr-led-4000-louver-e-04-830-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-04-830-L-1600MM.ies;1600;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 04 840 / L-1600MM;19.4309.3621.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3621.04-en-x-line-slight-surface-low-ugr-led-4000-louver-e-04-840-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-04-840-L-1600MM.ies;1600;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 21 830 / L-1600MM;19.4309.3611.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3611.21-en-x-line-slight-surface-low-ugr-led-4000-louver-e-21-830-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-21-830-L-1600MM.ies;1600;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 21 840 / L-1600MM;19.4309.3621.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3621.21-en-x-line-slight-surface-low-ugr-led-4000-louver-e-21-840-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-21-840-L-1600MM.ies;1600;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 24 830 / L-1600MM;19.4309.3611.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3611.24-en-x-line-slight-surface-low-ugr-led-4000-louver-e-24-830-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-24-830-L-1600MM.ies;1600;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 24 840 / L-1600MM;19.4309.3621.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3621.24-en-x-line-slight-surface-low-ugr-led-4000-louver-e-24-840-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-24-840-L-1600MM.ies;1600;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 34 830 / L-1600MM;19.4309.3611.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3611.34-en-x-line-slight-surface-low-ugr-led-4000-louver-e-34-830-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-34-830-L-1600MM.ies;1600;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 34 840 / L-1600MM;19.4309.3621.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3621.34-en-x-line-slight-surface-low-ugr-led-4000-louver-e-34-840-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-34-840-L-1600MM.ies;1600;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 04 830 / L-1600MM;19.4309.3613.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3613.04-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-04-830-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-04-830-L-1600MM.ies;1600;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 04 840 / L-1600MM;19.4309.3623.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3623.04-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-04-840-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-04-840-L-1600MM.ies;1600;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 21 830 / L-1600MM;19.4309.3613.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3613.21-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-21-830-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-21-830-L-1600MM.ies;1600;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 21 840 / L-1600MM;19.4309.3623.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3623.21-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-21-840-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-21-840-L-1600MM.ies;1600;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 24 830 / L-1600MM;19.4309.3613.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3613.24-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-24-830-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-24-830-L-1600MM.ies;1600;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 24 840 / L-1600MM;19.4309.3623.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3623.24-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-24-840-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-24-840-L-1600MM.ies;1600;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 34 830 / L-1600MM;19.4309.3613.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3613.34-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-34-830-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-34-830-L-1600MM.ies;1600;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 34 840 / L-1600MM;19.4309.3623.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1600 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.3623.34-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-34-840-l-1600mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-34-840-L-1600MM.ies;1600;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 04 830 / L-2000MM;19.4309.4811.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4811.04-en-x-line-slight-surface-low-ugr-led-5000-louver-e-04-830-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-04-830-L-2000MM.ies;2000;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 04 840 / L-2000MM;19.4309.4821.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4821.04-en-x-line-slight-surface-low-ugr-led-5000-louver-e-04-840-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-04-840-L-2000MM.ies;2000;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 21 830 / L-2000MM;19.4309.4811.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4811.21-en-x-line-slight-surface-low-ugr-led-5000-louver-e-21-830-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-21-830-L-2000MM.ies;2000;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 21 840 / L-2000MM;19.4309.4821.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4821.21-en-x-line-slight-surface-low-ugr-led-5000-louver-e-21-840-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-21-840-L-2000MM.ies;2000;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 24 830 / L-2000MM;19.4309.4811.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4811.24-en-x-line-slight-surface-low-ugr-led-5000-louver-e-24-830-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-24-830-L-2000MM.ies;2000;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 24 840 / L-2000MM;19.4309.4821.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4821.24-en-x-line-slight-surface-low-ugr-led-5000-louver-e-24-840-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-24-840-L-2000MM.ies;2000;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 34 830 / L-2000MM;19.4309.4811.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4811.34-en-x-line-slight-surface-low-ugr-led-5000-louver-e-34-830-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-34-830-L-2000MM.ies;2000;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 34 840 / L-2000MM;19.4309.4821.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4821.34-en-x-line-slight-surface-low-ugr-led-5000-louver-e-34-840-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-34-840-L-2000MM.ies;2000;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 04 830 / L-2000MM;19.4309.4813.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4813.04-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-04-830-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-04-830-L-2000MM.ies;2000;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 04 840 / L-2000MM;19.4309.4823.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4823.04-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-04-840-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-04-840-L-2000MM.ies;2000;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 21 830 / L-2000MM;19.4309.4813.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4813.21-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-21-830-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-21-830-L-2000MM.ies;2000;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 21 840 / L-2000MM;19.4309.4823.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4823.21-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-21-840-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-21-840-L-2000MM.ies;2000;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 24 830 / L-2000MM;19.4309.4813.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4813.24-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-24-830-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-24-830-L-2000MM.ies;2000;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 24 840 / L-2000MM;19.4309.4823.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4823.24-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-24-840-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-24-840-L-2000MM.ies;2000;34;68;230;4000
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 34 830 / L-2000MM;19.4309.4813.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4813.34-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-34-830-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-34-830-L-2000MM.ies;2000;34;68;230;3000
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 34 840 / L-2000MM;19.4309.4823.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);2000 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4309.4823.34-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-34-840-l-2000mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-34-840-L-2000MM.ies;2000;34;68;230;4000
