;Assembly Code##OTHER##;Assembly##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Dimensions##OTHER##;Voltage (range)##OTHER##;Driver##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Power of luminaire##ELECTRICAL_WATTAGE##WATTS;Luminaire luminous flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Luminaire's light efficiency##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;Color of the light##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Efficiency##OTHER##;Power factor##OTHER##;Manufacturer##OTHER##;URL##OTHER##;Catalogue##OTHER## ;Photometric Web File##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;BM##OTHER##;S##OTHER##
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 04 830 LINE-BM / L-798MM;19.4423.5111.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.0;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.5111.04-en-x-line-slight-surface-low-ugr-led-1200-louver-e-04-830-line-bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-04-830-LINE-BM-L-798MM.ies;798;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 04 830 LINE-S / L-796MM;19.4423.1111.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.0;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.1111.04-en-x-line-slight-surface-low-ugr-led-1200-louver-e-04-830-line-s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-04-830-LINE-S-L-796MM.ies;796;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 04 840 LINE-BM / L-798MM;19.4423.5121.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.0;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.5121.04-en-x-line-slight-surface-low-ugr-led-1200-louver-e-04-840-line-bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-04-840-LINE-BM-L-798MM.ies;798;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 04 840 LINE-S / L-796MM;19.4423.1121.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.0;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.1121.04-en-x-line-slight-surface-low-ugr-led-1200-louver-e-04-840-line-s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-04-840-LINE-S-L-796MM.ies;796;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 21 830 LINE-BM / L-798MM;19.4423.5111.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.0;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.5111.21-en-x-line-slight-surface-low-ugr-led-1200-louver-e-21-830-line-bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-21-830-LINE-BM-L-798MM.ies;798;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 21 830 LINE-S / L-796MM;19.4423.1111.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.0;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.1111.21-en-x-line-slight-surface-low-ugr-led-1200-louver-e-21-830-line-s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-21-830-LINE-S-L-796MM.ies;796;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 21 840 LINE-BM / L-798MM;19.4423.5121.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.0;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.5121.21-en-x-line-slight-surface-low-ugr-led-1200-louver-e-21-840-line-bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-21-840-LINE-BM-L-798MM.ies;798;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 21 840 LINE-S / L-796MM;19.4423.1121.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.0;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.1121.21-en-x-line-slight-surface-low-ugr-led-1200-louver-e-21-840-line-s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-21-840-LINE-S-L-796MM.ies;796;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 24 830 LINE-BM / L-798MM;19.4423.5111.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.0;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.5111.24-en-x-line-slight-surface-low-ugr-led-1200-louver-e-24-830-line-bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-24-830-LINE-BM-L-798MM.ies;798;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 24 830 LINE-S / L-796MM;19.4423.1111.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.0;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.1111.24-en-x-line-slight-surface-low-ugr-led-1200-louver-e-24-830-line-s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-24-830-LINE-S-L-796MM.ies;796;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 24 840 LINE-BM / L-798MM;19.4423.5121.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.0;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.5121.24-en-x-line-slight-surface-low-ugr-led-1200-louver-e-24-840-line-bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-24-840-LINE-BM-L-798MM.ies;798;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 24 840 LINE-S / L-796MM;19.4423.1121.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.0;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.1121.24-en-x-line-slight-surface-low-ugr-led-1200-louver-e-24-840-line-s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-24-840-LINE-S-L-796MM.ies;796;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 34 830 LINE-BM / L-798MM;19.4423.5111.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.0;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.5111.34-en-x-line-slight-surface-low-ugr-led-1200-louver-e-34-830-line-bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-34-830-LINE-BM-L-798MM.ies;798;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 34 830 LINE-S / L-796MM;19.4423.1111.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.0;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.1111.34-en-x-line-slight-surface-low-ugr-led-1200-louver-e-34-830-line-s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-34-830-LINE-S-L-796MM.ies;796;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 34 840 LINE-BM / L-798MM;19.4423.5121.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.0;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.5121.34-en-x-line-slight-surface-low-ugr-led-1200-louver-e-34-840-line-bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-34-840-LINE-BM-L-798MM.ies;798;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER E 34 840 LINE-S / L-796MM;19.4423.1121.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;8.0;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.1121.34-en-x-line-slight-surface-low-ugr-led-1200-louver-e-34-840-line-s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-E-34-840-LINE-S-L-796MM.ies;796;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 04 830 LINE-1BM / L-798MM;19.4423.D113.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.0;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.D113.04-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-04-830-line-1bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-04-830-LINE-1BM-L-798MM.ies;798;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 04 830 LINE-1S / L-796MM;19.4423.9113.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.0;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.9113.04-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-04-830-line-1s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-04-830-LINE-1S-L-796MM.ies;796;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 04 840 LINE-1BM / L-798MM;19.4423.D123.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.0;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.D123.04-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-04-840-line-1bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-04-840-LINE-1BM-L-798MM.ies;798;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 04 840 LINE-1S / L-796MM;19.4423.9123.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.0;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.9123.04-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-04-840-line-1s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-04-840-LINE-1S-L-796MM.ies;796;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 21 830 LINE-1BM / L-798MM;19.4423.D113.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.0;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.D113.21-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-21-830-line-1bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-21-830-LINE-1BM-L-798MM.ies;798;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 21 830 LINE-1S / L-796MM;19.4423.9113.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.0;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.9113.21-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-21-830-line-1s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-21-830-LINE-1S-L-796MM.ies;796;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 21 840 LINE-1BM / L-798MM;19.4423.D123.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.0;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.D123.21-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-21-840-line-1bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-21-840-LINE-1BM-L-798MM.ies;798;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 21 840 LINE-1S / L-796MM;19.4423.9123.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.0;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.9123.21-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-21-840-line-1s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-21-840-LINE-1S-L-796MM.ies;796;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 24 830 LINE-1BM / L-798MM;19.4423.D113.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.0;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.D113.24-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-24-830-line-1bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-24-830-LINE-1BM-L-798MM.ies;798;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 24 830 LINE-1S / L-796MM;19.4423.9113.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.0;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.9113.24-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-24-830-line-1s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-24-830-LINE-1S-L-796MM.ies;796;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 24 840 LINE-1BM / L-798MM;19.4423.D123.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.0;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.D123.24-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-24-840-line-1bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-24-840-LINE-1BM-L-798MM.ies;798;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 24 840 LINE-1S / L-796MM;19.4423.9123.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.0;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.9123.24-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-24-840-line-1s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-24-840-LINE-1S-L-796MM.ies;796;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 34 830 LINE-1BM / L-798MM;19.4423.D113.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.0;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.D113.34-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-34-830-line-1bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-34-830-LINE-1BM-L-798MM.ies;798;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 34 830 LINE-1S / L-796MM;19.4423.9113.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.0;846.8;105.9;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.9113.34-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-34-830-line-1s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-34-830-LINE-1S-L-796MM.ies;796;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 34 840 LINE-1BM / L-798MM;19.4423.D123.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.0;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.D123.34-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-34-840-line-1bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-34-840-LINE-1BM-L-798MM.ies;798;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1200 LOUVER EDD 34 840 LINE-1S / L-796MM;19.4423.9123.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;8.0;891.4;111.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.9123.34-en-x-line-slight-surface-low-ugr-led-1200-louver-edd-34-840-line-1s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1200-LOUVER-EDD-34-840-LINE-1S-L-796MM.ies;796;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 04 830 LINE-BM / L-1198MM;19.4423.6311.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.6311.04-en-x-line-slight-surface-low-ugr-led-1800-louver-e-04-830-line-bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-04-830-LINE-BM-L-1198MM.ies;1198;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 04 830 LINE-S / L-1196MM;19.4423.2311.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.2311.04-en-x-line-slight-surface-low-ugr-led-1800-louver-e-04-830-line-s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-04-830-LINE-S-L-1196MM.ies;1196;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 04 840 LINE-BM / L-1198MM;19.4423.6321.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.6321.04-en-x-line-slight-surface-low-ugr-led-1800-louver-e-04-840-line-bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-04-840-LINE-BM-L-1198MM.ies;1198;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 04 840 LINE-S / L-1196MM;19.4423.2321.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.2321.04-en-x-line-slight-surface-low-ugr-led-1800-louver-e-04-840-line-s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-04-840-LINE-S-L-1196MM.ies;1196;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 21 830 LINE-BM / L-1198MM;19.4423.6311.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.6311.21-en-x-line-slight-surface-low-ugr-led-1800-louver-e-21-830-line-bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-21-830-LINE-BM-L-1198MM.ies;1198;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 21 830 LINE-S / L-1196MM;19.4423.2311.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.2311.21-en-x-line-slight-surface-low-ugr-led-1800-louver-e-21-830-line-s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-21-830-LINE-S-L-1196MM.ies;1196;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 21 840 LINE-BM / L-1198MM;19.4423.6321.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.6321.21-en-x-line-slight-surface-low-ugr-led-1800-louver-e-21-840-line-bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-21-840-LINE-BM-L-1198MM.ies;1198;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 21 840 LINE-S / L-1196MM;19.4423.2321.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.2321.21-en-x-line-slight-surface-low-ugr-led-1800-louver-e-21-840-line-s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-21-840-LINE-S-L-1196MM.ies;1196;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 24 830 LINE-BM / L-1198MM;19.4423.6311.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.6311.24-en-x-line-slight-surface-low-ugr-led-1800-louver-e-24-830-line-bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-24-830-LINE-BM-L-1198MM.ies;1198;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 24 830 LINE-S / L-1196MM;19.4423.2311.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.2311.24-en-x-line-slight-surface-low-ugr-led-1800-louver-e-24-830-line-s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-24-830-LINE-S-L-1196MM.ies;1196;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 24 840 LINE-BM / L-1198MM;19.4423.6321.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.6321.24-en-x-line-slight-surface-low-ugr-led-1800-louver-e-24-840-line-bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-24-840-LINE-BM-L-1198MM.ies;1198;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 24 840 LINE-S / L-1196MM;19.4423.2321.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.2321.24-en-x-line-slight-surface-low-ugr-led-1800-louver-e-24-840-line-s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-24-840-LINE-S-L-1196MM.ies;1196;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 34 830 LINE-BM / L-1198MM;19.4423.6311.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.6311.34-en-x-line-slight-surface-low-ugr-led-1800-louver-e-34-830-line-bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-34-830-LINE-BM-L-1198MM.ies;1198;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 34 830 LINE-S / L-1196MM;19.4423.2311.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.2311.34-en-x-line-slight-surface-low-ugr-led-1800-louver-e-34-830-line-s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-34-830-LINE-S-L-1196MM.ies;1196;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 34 840 LINE-BM / L-1198MM;19.4423.6321.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.6321.34-en-x-line-slight-surface-low-ugr-led-1800-louver-e-34-840-line-bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-34-840-LINE-BM-L-1198MM.ies;1198;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER E 34 840 LINE-S / L-1196MM;19.4423.2321.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.2321.34-en-x-line-slight-surface-low-ugr-led-1800-louver-e-34-840-line-s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-E-34-840-LINE-S-L-1196MM.ies;1196;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 04 830 LINE-1BM / L-1198MM;19.4423.E313.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.E313.04-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-04-830-line-1bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-04-830-LINE-1BM-L-1198MM.ies;1198;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 04 830 LINE-1S / L-1196MM;19.4423.A313.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.A313.04-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-04-830-line-1s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-04-830-LINE-1S-L-1196MM.ies;1196;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 04 840 LINE-1BM / L-1198MM;19.4423.E323.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.E323.04-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-04-840-line-1bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-04-840-LINE-1BM-L-1198MM.ies;1198;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 04 840 LINE-1S / L-1196MM;19.4423.A323.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.A323.04-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-04-840-line-1s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-04-840-LINE-1S-L-1196MM.ies;1196;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 21 830 LINE-1BM / L-1198MM;19.4423.E313.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.E313.21-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-21-830-line-1bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-21-830-LINE-1BM-L-1198MM.ies;1198;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 21 830 LINE-1S / L-1196MM;19.4423.A313.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.A313.21-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-21-830-line-1s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-21-830-LINE-1S-L-1196MM.ies;1196;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 21 840 LINE-1BM / L-1198MM;19.4423.E323.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.E323.21-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-21-840-line-1bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-21-840-LINE-1BM-L-1198MM.ies;1198;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 21 840 LINE-1S / L-1196MM;19.4423.A323.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.A323.21-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-21-840-line-1s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-21-840-LINE-1S-L-1196MM.ies;1196;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 24 830 LINE-1BM / L-1198MM;19.4423.E313.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.E313.24-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-24-830-line-1bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-24-830-LINE-1BM-L-1198MM.ies;1198;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 24 830 LINE-1S / L-1196MM;19.4423.A313.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.A313.24-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-24-830-line-1s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-24-830-LINE-1S-L-1196MM.ies;1196;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 24 840 LINE-1BM / L-1198MM;19.4423.E323.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.E323.24-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-24-840-line-1bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-24-840-LINE-1BM-L-1198MM.ies;1198;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 24 840 LINE-1S / L-1196MM;19.4423.A323.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.A323.24-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-24-840-line-1s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-24-840-LINE-1S-L-1196MM.ies;1196;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 34 830 LINE-1BM / L-1198MM;19.4423.E313.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.E313.34-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-34-830-line-1bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-34-830-LINE-1BM-L-1198MM.ies;1198;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 34 830 LINE-1S / L-1196MM;19.4423.A313.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1270.2;112.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.A313.34-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-34-830-line-1s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-34-830-LINE-1S-L-1196MM.ies;1196;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 34 840 LINE-1BM / L-1198MM;19.4423.E323.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.E323.34-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-34-840-line-1bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-34-840-LINE-1BM-L-1198MM.ies;1198;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 1800 LOUVER EDD 34 840 LINE-1S / L-1196MM;19.4423.A323.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;11.3;1336.8;118.3;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.A323.34-en-x-line-slight-surface-low-ugr-led-1800-louver-edd-34-840-line-1s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-1800-LOUVER-EDD-34-840-LINE-1S-L-1196MM.ies;1196;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 04 830 LINE-BM / L-798MM;19.4423.5211.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.5211.04-en-x-line-slight-surface-low-ugr-led-2000-louver-e-04-830-line-bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-04-830-LINE-BM-L-798MM.ies;798;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 04 830 LINE-S / L-796MM;19.4423.1211.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.1211.04-en-x-line-slight-surface-low-ugr-led-2000-louver-e-04-830-line-s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-04-830-LINE-S-L-796MM.ies;796;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 04 840 LINE-BM / L-798MM;19.4423.5221.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.5221.04-en-x-line-slight-surface-low-ugr-led-2000-louver-e-04-840-line-bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-04-840-LINE-BM-L-798MM.ies;798;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 04 840 LINE-S / L-796MM;19.4423.1221.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.1221.04-en-x-line-slight-surface-low-ugr-led-2000-louver-e-04-840-line-s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-04-840-LINE-S-L-796MM.ies;796;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 21 830 LINE-BM / L-798MM;19.4423.5211.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.5211.21-en-x-line-slight-surface-low-ugr-led-2000-louver-e-21-830-line-bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-21-830-LINE-BM-L-798MM.ies;798;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 21 830 LINE-S / L-796MM;19.4423.1211.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.1211.21-en-x-line-slight-surface-low-ugr-led-2000-louver-e-21-830-line-s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-21-830-LINE-S-L-796MM.ies;796;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 21 840 LINE-BM / L-798MM;19.4423.5221.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.5221.21-en-x-line-slight-surface-low-ugr-led-2000-louver-e-21-840-line-bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-21-840-LINE-BM-L-798MM.ies;798;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 21 840 LINE-S / L-796MM;19.4423.1221.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.1221.21-en-x-line-slight-surface-low-ugr-led-2000-louver-e-21-840-line-s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-21-840-LINE-S-L-796MM.ies;796;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 24 830 LINE-BM / L-798MM;19.4423.5211.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.5211.24-en-x-line-slight-surface-low-ugr-led-2000-louver-e-24-830-line-bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-24-830-LINE-BM-L-798MM.ies;798;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 24 830 LINE-S / L-796MM;19.4423.1211.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.1211.24-en-x-line-slight-surface-low-ugr-led-2000-louver-e-24-830-line-s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-24-830-LINE-S-L-796MM.ies;796;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 24 840 LINE-BM / L-798MM;19.4423.5221.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.5221.24-en-x-line-slight-surface-low-ugr-led-2000-louver-e-24-840-line-bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-24-840-LINE-BM-L-798MM.ies;798;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 24 840 LINE-S / L-796MM;19.4423.1221.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.1221.24-en-x-line-slight-surface-low-ugr-led-2000-louver-e-24-840-line-s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-24-840-LINE-S-L-796MM.ies;796;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 34 830 LINE-BM / L-798MM;19.4423.5211.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.5211.34-en-x-line-slight-surface-low-ugr-led-2000-louver-e-34-830-line-bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-34-830-LINE-BM-L-798MM.ies;798;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 34 830 LINE-S / L-796MM;19.4423.1211.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.1211.34-en-x-line-slight-surface-low-ugr-led-2000-louver-e-34-830-line-s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-34-830-LINE-S-L-796MM.ies;796;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 34 840 LINE-BM / L-798MM;19.4423.5221.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.5221.34-en-x-line-slight-surface-low-ugr-led-2000-louver-e-34-840-line-bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-34-840-LINE-BM-L-798MM.ies;798;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER E 34 840 LINE-S / L-796MM;19.4423.1221.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.1221.34-en-x-line-slight-surface-low-ugr-led-2000-louver-e-34-840-line-s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-E-34-840-LINE-S-L-796MM.ies;796;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 04 830 LINE-1BM / L-798MM;19.4423.D213.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.D213.04-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-04-830-line-1bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-04-830-LINE-1BM-L-798MM.ies;798;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 04 830 LINE-1S / L-796MM;19.4423.9213.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.9213.04-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-04-830-line-1s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-04-830-LINE-1S-L-796MM.ies;796;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 04 840 LINE-1BM / L-798MM;19.4423.D223.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.D223.04-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-04-840-line-1bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-04-840-LINE-1BM-L-798MM.ies;798;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 04 840 LINE-1S / L-796MM;19.4423.9223.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.9223.04-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-04-840-line-1s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-04-840-LINE-1S-L-796MM.ies;796;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 21 830 LINE-1S / L-796MM;19.4423.9213.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.9213.21-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-21-830-line-1s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-21-830-LINE-1S-L-796MM.ies;796;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 21 840 LINE-1BM / L-798MM;19.4423.D223.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.D223.21-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-21-840-line-1bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-21-840-LINE-1BM-L-798MM.ies;798;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 21 840 LINE-1S / L-796MM;19.4423.9223.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.9223.21-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-21-840-line-1s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-21-840-LINE-1S-L-796MM.ies;796;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 24 830 LINE-1BM / L-798MM;19.4423.D213.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.D213.24-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-24-830-line-1bm-l-798mm-2.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-24-830-LINE-1BM-L-798MM.ies;798;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 21 830 LINE-1BM / L-798MM;19.4423.D213.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.D213.21-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-21-830-line-1bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-24-830-LINE-1BM-L-798MM.ies;798;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 24 830 LINE-1S / L-796MM;19.4423.9213.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.9213.24-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-24-830-line-1s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-24-830-LINE-1S-L-796MM.ies;796;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 24 840 LINE-1BM / L-798MM;19.4423.D223.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.D223.24-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-24-840-line-1bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-24-840-LINE-1BM-L-798MM.ies;798;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 24 840 LINE-1S / L-796MM;19.4423.9223.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.9223.24-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-24-840-line-1s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-24-840-LINE-1S-L-796MM.ies;796;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 34 830 LINE-1BM / L-798MM;19.4423.D213.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.D213.34-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-34-830-line-1bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-34-830-LINE-1BM-L-798MM.ies;798;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 34 830 LINE-1S / L-796MM;19.4423.9213.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1377.5;104.4;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.9213.34-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-34-830-line-1s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-34-830-LINE-1S-L-796MM.ies;796;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 34 840 LINE-1BM / L-798MM;19.4423.D223.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);798 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.D223.34-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-34-840-line-1bm-l-798mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-34-840-LINE-1BM-L-798MM.ies;798;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2000 LOUVER EDD 34 840 LINE-1S / L-796MM;19.4423.9223.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);796 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;13.2;1450;109.8;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.9223.34-en-x-line-slight-surface-low-ugr-led-2000-louver-edd-34-840-line-1s-l-796mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2000-LOUVER-EDD-34-840-LINE-1S-L-796MM.ies;796;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 04 830 LINE-BM / L-1598MM;19.4423.7511.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.7511.04-en-x-line-slight-surface-low-ugr-led-2400-louver-e-04-830-line-bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-04-830-LINE-BM-L-1598MM.ies;1598;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 04 830 LINE-S / L-1596MM;19.4423.3511.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.3511.04-en-x-line-slight-surface-low-ugr-led-2400-louver-e-04-830-line-s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-04-830-LINE-S-L-1596MM.ies;1596;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 04 840 LINE-BM / L-1598MM;19.4423.7521.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.7521.04-en-x-line-slight-surface-low-ugr-led-2400-louver-e-04-840-line-bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-04-840-LINE-BM-L-1598MM.ies;1598;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 04 840 LINE-S / L-1596MM;19.4423.3521.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.3521.04-en-x-line-slight-surface-low-ugr-led-2400-louver-e-04-840-line-s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-04-840-LINE-S-L-1596MM.ies;1596;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 21 830 LINE-BM / L-1598MM;19.4423.7511.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.7511.21-en-x-line-slight-surface-low-ugr-led-2400-louver-e-21-830-line-bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-21-830-LINE-BM-L-1598MM.ies;1598;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 21 830 LINE-S / L-1596MM;19.4423.3511.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.3511.21-en-x-line-slight-surface-low-ugr-led-2400-louver-e-21-830-line-s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-21-830-LINE-S-L-1596MM.ies;1596;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 21 840 LINE-BM / L-1598MM;19.4423.7521.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.7521.21-en-x-line-slight-surface-low-ugr-led-2400-louver-e-21-840-line-bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-21-840-LINE-BM-L-1598MM.ies;1598;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 21 840 LINE-S / L-1596MM;19.4423.3521.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.3521.21-en-x-line-slight-surface-low-ugr-led-2400-louver-e-21-840-line-s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-21-840-LINE-S-L-1596MM.ies;1596;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 24 830 LINE-BM / L-1598MM;19.4423.7511.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.7511.24-en-x-line-slight-surface-low-ugr-led-2400-louver-e-24-830-line-bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-24-830-LINE-BM-L-1598MM.ies;1598;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 24 830 LINE-S / L-1596MM;19.4423.3511.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.3511.24-en-x-line-slight-surface-low-ugr-led-2400-louver-e-24-830-line-s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-24-830-LINE-S-L-1596MM.ies;1596;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 24 840 LINE-BM / L-1598MM;19.4423.7521.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.7521.24-en-x-line-slight-surface-low-ugr-led-2400-louver-e-24-840-line-bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-24-840-LINE-BM-L-1598MM.ies;1598;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 24 840 LINE-S / L-1596MM;19.4423.3521.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.3521.24-en-x-line-slight-surface-low-ugr-led-2400-louver-e-24-840-line-s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-24-840-LINE-S-L-1596MM.ies;1596;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 34 830 LINE-BM / L-1598MM;19.4423.7511.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.7511.34-en-x-line-slight-surface-low-ugr-led-2400-louver-e-34-830-line-bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-34-830-LINE-BM-L-1598MM.ies;1598;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 34 830 LINE-S / L-1596MM;19.4423.3511.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.3511.34-en-x-line-slight-surface-low-ugr-led-2400-louver-e-34-830-line-s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-34-830-LINE-S-L-1596MM.ies;1596;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 34 840 LINE-BM / L-1598MM;19.4423.7521.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.7521.34-en-x-line-slight-surface-low-ugr-led-2400-louver-e-34-840-line-bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-34-840-LINE-BM-L-1598MM.ies;1598;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER E 34 840 LINE-S / L-1596MM;19.4423.3521.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.3521.34-en-x-line-slight-surface-low-ugr-led-2400-louver-e-34-840-line-s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-E-34-840-LINE-S-L-1596MM.ies;1596;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 04 830 LINE-1BM / L-1598MM;19.4423.F513.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.F513.04-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-04-830-line-1bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-04-830-LINE-1BM-L-1598MM.ies;1598;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 04 830 LINE-1S / L-1596MM;19.4423.B513.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.B513.04-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-04-830-line-1s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-04-830-LINE-1S-L-1596MM.ies;1596;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 04 840 LINE-1BM / L-1598MM;19.4423.F523.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.F523.04-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-04-840-line-1bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-04-840-LINE-1BM-L-1598MM.ies;1598;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 04 840 LINE-1S / L-1596MM;19.4423.B523.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.B523.04-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-04-840-line-1s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-04-840-LINE-1S-L-1596MM.ies;1596;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 21 830 LINE-1BM / L-1598MM;19.4423.F513.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.F513.21-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-21-830-line-1bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-21-830-LINE-1BM-L-1598MM.ies;1598;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 21 830 LINE-1S / L-1596MM;19.4423.B513.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.B513.21-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-21-830-line-1s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-21-830-LINE-1S-L-1596MM.ies;1596;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 21 840 LINE-1BM / L-1598MM;19.4423.F523.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.F523.21-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-21-840-line-1bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-21-840-LINE-1BM-L-1598MM.ies;1598;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 21 840 LINE-1S / L-1596MM;19.4423.B523.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.B523.21-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-21-840-line-1s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-21-840-LINE-1S-L-1596MM.ies;1596;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 24 830 LINE-1BM / L-1598MM;19.4423.F513.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.F513.24-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-24-830-line-1bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-24-830-LINE-1BM-L-1598MM.ies;1598;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 24 830 LINE-1S / L-1596MM;19.4423.B513.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.B513.24-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-24-830-line-1s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-24-830-LINE-1S-L-1596MM.ies;1596;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 24 840 LINE-1BM / L-1598MM;19.4423.F523.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.F523.24-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-24-840-line-1bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-24-840-LINE-1BM-L-1598MM.ies;1598;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 24 840 LINE-1S / L-1596MM;19.4423.B523.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.B523.24-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-24-840-line-1s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-24-840-LINE-1S-L-1596MM.ies;1596;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 34 830 LINE-1BM / L-1598MM;19.4423.F513.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.F513.34-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-34-830-line-1bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-34-830-LINE-1BM-L-1598MM.ies;1598;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 34 830 LINE-1S / L-1596MM;19.4423.B513.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1693.6;116.8;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.B513.34-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-34-830-line-1s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-34-830-LINE-1S-L-1596MM.ies;1596;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 34 840 LINE-1BM / L-1598MM;19.4423.F523.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.F523.34-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-34-840-line-1bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-34-840-LINE-1BM-L-1598MM.ies;1598;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 2400 LOUVER EDD 34 840 LINE-1S / L-1596MM;19.4423.B523.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;14.5;1782.5;122.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.B523.34-en-x-line-slight-surface-low-ugr-led-2400-louver-edd-34-840-line-1s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-2400-LOUVER-EDD-34-840-LINE-1S-L-1596MM.ies;1596;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 04 830 LINE-BM / L-1198MM;19.4423.6411.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.6411.04-en-x-line-slight-surface-low-ugr-led-3000-louver-e-04-830-line-bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-04-830-LINE-BM-L-1198MM.ies;1198;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 04 830 LINE-BM / L-1998MM;19.4423.8411.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.8411.04-en-x-line-slight-surface-low-ugr-led-3000-louver-e-04-830-line-bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-04-830-LINE-BM-L-1998MM.ies;1998;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 04 830 LINE-S / L-1196MM;19.4423.2411.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.2411.04-en-x-line-slight-surface-low-ugr-led-3000-louver-e-04-830-line-s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-04-830-LINE-S-L-1196MM.ies;1196;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 04 830 LINE-S / L-1996MM;19.4423.4411.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.4411.04-en-x-line-slight-surface-low-ugr-led-3000-louver-e-04-830-line-s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-04-830-LINE-S-L-1996MM.ies;1996;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 04 840 LINE-BM / L-1198MM;19.4423.6421.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.6421.04-en-x-line-slight-surface-low-ugr-led-3000-louver-e-04-840-line-bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-04-840-LINE-BM-L-1198MM.ies;1198;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 04 840 LINE-BM / L-1998MM;19.4423.8421.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.8421.04-en-x-line-slight-surface-low-ugr-led-3000-louver-e-04-840-line-bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-04-840-LINE-BM-L-1998MM.ies;1998;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 04 840 LINE-S / L-1196MM;19.4423.2421.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.2421.04-en-x-line-slight-surface-low-ugr-led-3000-louver-e-04-840-line-s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-04-840-LINE-S-L-1196MM.ies;1196;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 04 840 LINE-S / L-1996MM;19.4423.4421.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.4421.04-en-x-line-slight-surface-low-ugr-led-3000-louver-e-04-840-line-s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-04-840-LINE-S-L-1996MM.ies;1996;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 21 830 LINE-BM / L-1198MM;19.4423.6411.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.6411.21-en-x-line-slight-surface-low-ugr-led-3000-louver-e-21-830-line-bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-21-830-LINE-BM-L-1198MM.ies;1198;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 21 830 LINE-BM / L-1998MM;19.4423.8411.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.8411.21-en-x-line-slight-surface-low-ugr-led-3000-louver-e-21-830-line-bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-21-830-LINE-BM-L-1998MM.ies;1998;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 21 830 LINE-S / L-1196MM;19.4423.2411.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.2411.21-en-x-line-slight-surface-low-ugr-led-3000-louver-e-21-830-line-s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-21-830-LINE-S-L-1196MM.ies;1196;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 21 830 LINE-S / L-1996MM;19.4423.4411.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.4411.21-en-x-line-slight-surface-low-ugr-led-3000-louver-e-21-830-line-s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-21-830-LINE-S-L-1996MM.ies;1996;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 21 840 LINE-BM / L-1198MM;19.4423.6421.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.6421.21-en-x-line-slight-surface-low-ugr-led-3000-louver-e-21-840-line-bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-21-840-LINE-BM-L-1198MM.ies;1198;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 21 840 LINE-BM / L-1998MM;19.4423.8421.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.8421.21-en-x-line-slight-surface-low-ugr-led-3000-louver-e-21-840-line-bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-21-840-LINE-BM-L-1998MM.ies;1998;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 21 840 LINE-S / L-1196MM;19.4423.2421.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.2421.21-en-x-line-slight-surface-low-ugr-led-3000-louver-e-21-840-line-s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-21-840-LINE-S-L-1196MM.ies;1196;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 21 840 LINE-S / L-1996MM;19.4423.4421.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.4421.21-en-x-line-slight-surface-low-ugr-led-3000-louver-e-21-840-line-s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-21-840-LINE-S-L-1996MM.ies;1996;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 24 830 LINE-BM / L-1198MM;19.4423.6411.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.6411.24-en-x-line-slight-surface-low-ugr-led-3000-louver-e-24-830-line-bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-24-830-LINE-BM-L-1198MM.ies;1198;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 24 830 LINE-BM / L-1998MM;19.4423.8411.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.8411.24-en-x-line-slight-surface-low-ugr-led-3000-louver-e-24-830-line-bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-24-830-LINE-BM-L-1998MM.ies;1998;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 24 830 LINE-S / L-1196MM;19.4423.2411.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.2411.24-en-x-line-slight-surface-low-ugr-led-3000-louver-e-24-830-line-s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-24-830-LINE-S-L-1196MM.ies;1196;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 24 830 LINE-S / L-1996MM;19.4423.4411.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.4411.24-en-x-line-slight-surface-low-ugr-led-3000-louver-e-24-830-line-s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-24-830-LINE-S-L-1996MM.ies;1996;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 24 840 LINE-BM / L-1198MM;19.4423.6421.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.6421.24-en-x-line-slight-surface-low-ugr-led-3000-louver-e-24-840-line-bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-24-840-LINE-BM-L-1198MM.ies;1198;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 24 840 LINE-BM / L-1998MM;19.4423.8421.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.8421.24-en-x-line-slight-surface-low-ugr-led-3000-louver-e-24-840-line-bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-24-840-LINE-BM-L-1998MM.ies;1998;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 24 840 LINE-S / L-1196MM;19.4423.2421.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.2421.24-en-x-line-slight-surface-low-ugr-led-3000-louver-e-24-840-line-s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-24-840-LINE-S-L-1196MM.ies;1196;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 24 840 LINE-S / L-1996MM;19.4423.4421.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.4421.24-en-x-line-slight-surface-low-ugr-led-3000-louver-e-24-840-line-s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-24-840-LINE-S-L-1996MM.ies;1996;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 34 830 LINE-BM / L-1198MM;19.4423.6411.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.6411.34-en-x-line-slight-surface-low-ugr-led-3000-louver-e-34-830-line-bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-34-830-LINE-BM-L-1198MM.ies;1198;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 34 830 LINE-BM / L-1998MM;19.4423.8411.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.8411.34-en-x-line-slight-surface-low-ugr-led-3000-louver-e-34-830-line-bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-34-830-LINE-BM-L-1998MM.ies;1998;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 34 830 LINE-S / L-1196MM;19.4423.2411.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.2411.34-en-x-line-slight-surface-low-ugr-led-3000-louver-e-34-830-line-s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-34-830-LINE-S-L-1196MM.ies;1196;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 34 830 LINE-S / L-1996MM;19.4423.4411.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.4411.34-en-x-line-slight-surface-low-ugr-led-3000-louver-e-34-830-line-s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-34-830-LINE-S-L-1996MM.ies;1996;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 34 840 LINE-BM / L-1198MM;19.4423.6421.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.6421.34-en-x-line-slight-surface-low-ugr-led-3000-louver-e-34-840-line-bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-34-840-LINE-BM-L-1198MM.ies;1198;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 34 840 LINE-BM / L-1998MM;19.4423.8421.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.8421.34-en-x-line-slight-surface-low-ugr-led-3000-louver-e-34-840-line-bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-34-840-LINE-BM-L-1998MM.ies;1998;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 34 840 LINE-S / L-1196MM;19.4423.2421.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.2421.34-en-x-line-slight-surface-low-ugr-led-3000-louver-e-34-840-line-s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-34-840-LINE-S-L-1196MM.ies;1196;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER E 34 840 LINE-S / L-1996MM;19.4423.4421.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.4421.34-en-x-line-slight-surface-low-ugr-led-3000-louver-e-34-840-line-s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-E-34-840-LINE-S-L-1996MM.ies;1996;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 04 830 LINE-1BM / L-1198MM;19.4423.E413.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.E413.04-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-04-830-line-1bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-04-830-LINE-1BM-L-1198MM.ies;1198;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 04 830 LINE-1BM / L-1998MM;19.4423.G413.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.G413.04-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-04-830-line-1bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-04-830-LINE-1BM-L-1998MM.ies;1998;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 04 830 LINE-1S / L-1196MM;19.4423.A413.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.A413.04-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-04-830-line-1s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-04-830-LINE-1S-L-1196MM.ies;1196;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 04 830 LINE-1S / L-1996MM;19.4423.C413.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.C413.04-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-04-830-line-1s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-04-830-LINE-1S-L-1996MM.ies;1996;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 04 840 LINE-1BM / L-1198MM;19.4423.E423.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.E423.04-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-04-840-line-1bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-04-840-LINE-1BM-L-1198MM.ies;1198;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 04 840 LINE-1BM / L-1998MM;19.4423.G423.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.G423.04-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-04-840-line-1bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-04-840-LINE-1BM-L-1998MM.ies;1998;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 04 840 LINE-1S / L-1196MM;19.4423.A423.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.A423.04-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-04-840-line-1s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-04-840-LINE-1S-L-1196MM.ies;1196;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 04 840 LINE-1S / L-1996MM;19.4423.C423.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.C423.04-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-04-840-line-1s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-04-840-LINE-1S-L-1996MM.ies;1996;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 21 830 LINE-1BM / L-1198MM;19.4423.E413.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.E413.21-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-21-830-line-1bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-21-830-LINE-1BM-L-1198MM.ies;1198;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 21 830 LINE-1BM / L-1998MM;19.4423.G413.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.G413.21-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-21-830-line-1bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-21-830-LINE-1BM-L-1998MM.ies;1998;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 21 830 LINE-1S / L-1196MM;19.4423.A413.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.A413.21-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-21-830-line-1s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-21-830-LINE-1S-L-1196MM.ies;1196;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 21 830 LINE-1S / L-1996MM;19.4423.C413.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.C413.21-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-21-830-line-1s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-21-830-LINE-1S-L-1996MM.ies;1996;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 21 840 LINE-1BM / L-1198MM;19.4423.E423.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.E423.21-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-21-840-line-1bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-21-840-LINE-1BM-L-1198MM.ies;1198;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 21 840 LINE-1BM / L-1998MM;19.4423.G423.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.G423.21-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-21-840-line-1bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-21-840-LINE-1BM-L-1998MM.ies;1998;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 21 840 LINE-1S / L-1196MM;19.4423.A423.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.A423.21-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-21-840-line-1s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-21-840-LINE-1S-L-1196MM.ies;1196;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 21 840 LINE-1S / L-1996MM;19.4423.C423.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.C423.21-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-21-840-line-1s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-21-840-LINE-1S-L-1996MM.ies;1996;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 24 830 LINE-1BM / L-1198MM;19.4423.E413.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.E413.24-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-24-830-line-1bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-24-830-LINE-1BM-L-1198MM.ies;1198;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 24 830 LINE-1BM / L-1998MM;19.4423.G413.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.G413.24-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-24-830-line-1bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-24-830-LINE-1BM-L-1998MM.ies;1998;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 24 830 LINE-1S / L-1196MM;19.4423.A413.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.A413.24-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-24-830-line-1s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-24-830-LINE-1S-L-1196MM.ies;1196;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 24 830 LINE-1S / L-1996MM;19.4423.C413.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.C413.24-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-24-830-line-1s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-24-830-LINE-1S-L-1996MM.ies;1996;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 24 840 LINE-1BM / L-1198MM;19.4423.E423.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.E423.24-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-24-840-line-1bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-24-840-LINE-1BM-L-1198MM.ies;1198;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 24 840 LINE-1BM / L-1998MM;19.4423.G423.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.G423.24-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-24-840-line-1bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-24-840-LINE-1BM-L-1998MM.ies;1998;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 24 840 LINE-1S / L-1196MM;19.4423.A423.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.A423.24-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-24-840-line-1s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-24-840-LINE-1S-L-1196MM.ies;1196;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 24 840 LINE-1S / L-1996MM;19.4423.C423.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.C423.24-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-24-840-line-1s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-24-840-LINE-1S-L-1996MM.ies;1996;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 34 830 LINE-1BM / L-1198MM;19.4423.E413.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.E413.34-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-34-830-line-1bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-34-830-LINE-1BM-L-1198MM.ies;1198;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 34 830 LINE-1BM / L-1998MM;19.4423.G413.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.G413.34-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-34-830-line-1bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-34-830-LINE-1BM-L-1998MM.ies;1998;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 34 830 LINE-1S / L-1196MM;19.4423.A413.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2066;108.2;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.A413.34-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-34-830-line-1s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-34-830-LINE-1S-L-1196MM.ies;1196;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 34 830 LINE-1S / L-1996MM;19.4423.C413.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2116.9;116.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.C413.34-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-34-830-line-1s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-34-830-LINE-1S-L-1996MM.ies;1996;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 34 840 LINE-1BM / L-1198MM;19.4423.E423.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1198 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.E423.34-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-34-840-line-1bm-l-1198mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-34-840-LINE-1BM-L-1198MM.ies;1198;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 34 840 LINE-1BM / L-1998MM;19.4423.G423.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.G423.34-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-34-840-line-1bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-34-840-LINE-1BM-L-1998MM.ies;1998;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 34 840 LINE-1S / L-1196MM;19.4423.A423.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1196 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;19.1;2174.7;113.9;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.A423.34-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-34-840-line-1s-l-1196mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-34-840-LINE-1S-L-1196MM.ies;1196;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 3000 LOUVER EDD 34 840 LINE-1S / L-1996MM;19.4423.C423.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;18.2;2228.1;122.4;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.C423.34-en-x-line-slight-surface-low-ugr-led-3000-louver-edd-34-840-line-1s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-3000-LOUVER-EDD-34-840-LINE-1S-L-1996MM.ies;1996;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 04 830 LINE-BM / L-1598MM;19.4423.7611.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.7611.04-en-x-line-slight-surface-low-ugr-led-4000-louver-e-04-830-line-bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-04-830-LINE-BM-L-1598MM.ies;1598;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 04 830 LINE-S / L-1596MM;19.4423.3611.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.3611.04-en-x-line-slight-surface-low-ugr-led-4000-louver-e-04-830-line-s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-04-830-LINE-S-L-1596MM.ies;1596;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 04 840 LINE-BM / L-1598MM;19.4423.7621.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.7621.04-en-x-line-slight-surface-low-ugr-led-4000-louver-e-04-840-line-bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-04-840-LINE-BM-L-1598MM.ies;1598;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 04 840 LINE-S / L-1596MM;19.4423.3621.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.3621.04-en-x-line-slight-surface-low-ugr-led-4000-louver-e-04-840-line-s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-04-840-LINE-S-L-1596MM.ies;1596;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 21 830 LINE-BM / L-1598MM;19.4423.7611.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.7611.21-en-x-line-slight-surface-low-ugr-led-4000-louver-e-21-830-line-bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-21-830-LINE-BM-L-1598MM.ies;1598;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 21 830 LINE-S / L-1596MM;19.4423.3611.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.3611.21-en-x-line-slight-surface-low-ugr-led-4000-louver-e-21-830-line-s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-21-830-LINE-S-L-1596MM.ies;1596;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 21 840 LINE-BM / L-1598MM;19.4423.7621.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.7621.21-en-x-line-slight-surface-low-ugr-led-4000-louver-e-21-840-line-bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-21-840-LINE-BM-L-1598MM.ies;1598;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 21 840 LINE-S / L-1596MM;19.4423.3621.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.3621.21-en-x-line-slight-surface-low-ugr-led-4000-louver-e-21-840-line-s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-21-840-LINE-S-L-1596MM.ies;1596;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 24 830 LINE-BM / L-1598MM;19.4423.7611.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.7611.24-en-x-line-slight-surface-low-ugr-led-4000-louver-e-24-830-line-bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-24-830-LINE-BM-L-1598MM.ies;1598;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 24 830 LINE-S / L-1596MM;19.4423.3611.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.3611.24-en-x-line-slight-surface-low-ugr-led-4000-louver-e-24-830-line-s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-24-830-LINE-S-L-1596MM.ies;1596;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 24 840 LINE-BM / L-1598MM;19.4423.7621.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.7621.24-en-x-line-slight-surface-low-ugr-led-4000-louver-e-24-840-line-bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-24-840-LINE-BM-L-1598MM.ies;1598;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 24 840 LINE-S / L-1596MM;19.4423.3621.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.3621.24-en-x-line-slight-surface-low-ugr-led-4000-louver-e-24-840-line-s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-24-840-LINE-S-L-1596MM.ies;1596;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 34 830 LINE-BM / L-1598MM;19.4423.7611.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.7611.34-en-x-line-slight-surface-low-ugr-led-4000-louver-e-34-830-line-bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-34-830-LINE-BM-L-1598MM.ies;1598;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 34 830 LINE-S / L-1596MM;19.4423.3611.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.3611.34-en-x-line-slight-surface-low-ugr-led-4000-louver-e-34-830-line-s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-34-830-LINE-S-L-1596MM.ies;1596;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 34 840 LINE-BM / L-1598MM;19.4423.7621.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.7621.34-en-x-line-slight-surface-low-ugr-led-4000-louver-e-34-840-line-bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-34-840-LINE-BM-L-1598MM.ies;1598;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER E 34 840 LINE-S / L-1596MM;19.4423.3621.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.3621.34-en-x-line-slight-surface-low-ugr-led-4000-louver-e-34-840-line-s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-E-34-840-LINE-S-L-1596MM.ies;1596;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 04 830 LINE-1BM / L-1598MM;19.4423.F613.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.F613.04-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-04-830-line-1bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-04-830-LINE-1BM-L-1598MM.ies;1598;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 04 830 LINE-1S / L-1596MM;19.4423.B613.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.B613.04-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-04-830-line-1s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-04-830-LINE-1S-L-1596MM.ies;1596;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 04 840 LINE-1BM / L-1598MM;19.4423.F623.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.F623.04-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-04-840-line-1bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-04-840-LINE-1BM-L-1598MM.ies;1598;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 04 840 LINE-1S / L-1596MM;19.4423.B623.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.B623.04-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-04-840-line-1s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-04-840-LINE-1S-L-1596MM.ies;1596;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 21 830 LINE-1BM / L-1598MM;19.4423.F613.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.F613.21-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-21-830-line-1bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-21-830-LINE-1BM-L-1598MM.ies;1598;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 21 830 LINE-1S / L-1596MM;19.4423.B613.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.B613.21-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-21-830-line-1s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-21-830-LINE-1S-L-1596MM.ies;1596;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 21 840 LINE-1BM / L-1598MM;19.4423.F623.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.F623.21-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-21-840-line-1bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-21-840-LINE-1BM-L-1598MM.ies;1598;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 21 840 LINE-1S / L-1596MM;19.4423.B623.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.B623.21-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-21-840-line-1s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-21-840-LINE-1S-L-1596MM.ies;1596;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 24 830 LINE-1BM / L-1598MM;19.4423.F613.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.F613.24-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-24-830-line-1bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-24-830-LINE-1BM-L-1598MM.ies;1598;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 24 830 LINE-1S / L-1596MM;19.4423.B613.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.B613.24-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-24-830-line-1s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-24-830-LINE-1S-L-1596MM.ies;1596;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 24 840 LINE-1BM / L-1598MM;19.4423.F623.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.F623.24-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-24-840-line-1bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-24-840-LINE-1BM-L-1598MM.ies;1598;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 24 840 LINE-1S / L-1596MM;19.4423.B623.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.B623.24-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-24-840-line-1s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-24-840-LINE-1S-L-1596MM.ies;1596;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 34 830 LINE-1BM / L-1598MM;19.4423.F613.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.F613.34-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-34-830-line-1bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-34-830-LINE-1BM-L-1598MM.ies;1598;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 34 830 LINE-1S / L-1596MM;19.4423.B613.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2754.7;108;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.B613.34-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-34-830-line-1s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-34-830-LINE-1S-L-1596MM.ies;1596;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 34 840 LINE-1BM / L-1598MM;19.4423.F623.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1598 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.F623.34-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-34-840-line-1bm-l-1598mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-34-840-LINE-1BM-L-1598MM.ies;1598;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 4000 LOUVER EDD 34 840 LINE-1S / L-1596MM;19.4423.B623.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1596 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;25.5;2899.5;113.7;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.B623.34-en-x-line-slight-surface-low-ugr-led-4000-louver-edd-34-840-line-1s-l-1596mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-4000-LOUVER-EDD-34-840-LINE-1S-L-1596MM.ies;1596;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 04 830 LINE-BM / L-1998MM;19.4423.8811.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.8811.04-en-x-line-slight-surface-low-ugr-led-5000-louver-e-04-830-line-bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-04-830-LINE-BM-L-1998MM.ies;1998;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 04 830 LINE-S / L-1996MM;19.4423.4811.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.4811.04-en-x-line-slight-surface-low-ugr-led-5000-louver-e-04-830-line-s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-04-830-LINE-S-L-1996MM.ies;1996;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 04 840 LINE-BM / L-1998MM;19.4423.8821.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.8821.04-en-x-line-slight-surface-low-ugr-led-5000-louver-e-04-840-line-bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-04-840-LINE-BM-L-1998MM.ies;1998;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 04 840 LINE-S / L-1996MM;19.4423.4821.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.4821.04-en-x-line-slight-surface-low-ugr-led-5000-louver-e-04-840-line-s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-04-840-LINE-S-L-1996MM.ies;1996;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 21 830 LINE-BM / L-1998MM;19.4423.8811.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.8811.21-en-x-line-slight-surface-low-ugr-led-5000-louver-e-21-830-line-bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-21-830-LINE-BM-L-1998MM.ies;1998;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 21 830 LINE-S / L-1996MM;19.4423.4811.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.4811.21-en-x-line-slight-surface-low-ugr-led-5000-louver-e-21-830-line-s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-21-830-LINE-S-L-1996MM.ies;1996;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 21 840 LINE-BM / L-1998MM;19.4423.8821.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.8821.21-en-x-line-slight-surface-low-ugr-led-5000-louver-e-21-840-line-bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-21-840-LINE-BM-L-1998MM.ies;1998;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 21 840 LINE-S / L-1996MM;19.4423.4821.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.4821.21-en-x-line-slight-surface-low-ugr-led-5000-louver-e-21-840-line-s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-21-840-LINE-S-L-1996MM.ies;1996;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 24 830 LINE-BM / L-1998MM;19.4423.8811.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.8811.24-en-x-line-slight-surface-low-ugr-led-5000-louver-e-24-830-line-bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-24-830-LINE-BM-L-1998MM.ies;1998;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 24 830 LINE-S / L-1996MM;19.4423.4811.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.4811.24-en-x-line-slight-surface-low-ugr-led-5000-louver-e-24-830-line-s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-24-830-LINE-S-L-1996MM.ies;1996;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 24 840 LINE-BM / L-1998MM;19.4423.8821.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.8821.24-en-x-line-slight-surface-low-ugr-led-5000-louver-e-24-840-line-bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-24-840-LINE-BM-L-1998MM.ies;1998;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 24 840 LINE-S / L-1996MM;19.4423.4821.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.4821.24-en-x-line-slight-surface-low-ugr-led-5000-louver-e-24-840-line-s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-24-840-LINE-S-L-1996MM.ies;1996;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 34 830 LINE-BM / L-1998MM;19.4423.8811.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.8811.34-en-x-line-slight-surface-low-ugr-led-5000-louver-e-34-830-line-bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-34-830-LINE-BM-L-1998MM.ies;1998;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 34 830 LINE-S / L-1996MM;19.4423.4811.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.4811.34-en-x-line-slight-surface-low-ugr-led-5000-louver-e-34-830-line-s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-34-830-LINE-S-L-1996MM.ies;1996;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 34 840 LINE-BM / L-1998MM;19.4423.8821.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.8821.34-en-x-line-slight-surface-low-ugr-led-5000-louver-e-34-840-line-bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-34-840-LINE-BM-L-1998MM.ies;1998;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER E 34 840 LINE-S / L-1996MM;19.4423.4821.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;standard on/off (E);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.4821.34-en-x-line-slight-surface-low-ugr-led-5000-louver-e-34-840-line-s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-E-34-840-LINE-S-L-1996MM.ies;1996;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 04 830 LINE-1BM / L-1998MM;19.4423.G813.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.G813.04-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-04-830-line-1bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-04-830-LINE-1BM-L-1998MM.ies;1998;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 04 830 LINE-1S / L-1996MM;19.4423.C813.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.C813.04-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-04-830-line-1s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-04-830-LINE-1S-L-1996MM.ies;1996;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 04 840 LINE-1BM / L-1998MM;19.4423.G823.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.G823.04-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-04-840-line-1bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-04-840-LINE-1BM-L-1998MM.ies;1998;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 04 840 LINE-1S / L-1996MM;19.4423.C823.04;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9005 (black);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.C823.04-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-04-840-line-1s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-04-840-LINE-1S-L-1996MM.ies;1996;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 21 830 LINE-1BM / L-1998MM;19.4423.G813.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.G813.21-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-21-830-line-1bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-21-830-LINE-1BM-L-1998MM.ies;1998;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 21 830 LINE-1S / L-1996MM;19.4423.C813.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.C813.21-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-21-830-line-1s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-21-830-LINE-1S-L-1996MM.ies;1996;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 21 840 LINE-1BM / L-1998MM;19.4423.G823.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.G823.21-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-21-840-line-1bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-21-840-LINE-1BM-L-1998MM.ies;1998;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 21 840 LINE-1S / L-1996MM;19.4423.C823.21;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9006 (grey);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.C823.21-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-21-840-line-1s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-21-840-LINE-1S-L-1996MM.ies;1996;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 24 830 LINE-1BM / L-1998MM;19.4423.G813.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.G813.24-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-24-830-line-1bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-24-830-LINE-1BM-L-1998MM.ies;1998;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 24 830 LINE-1S / L-1996MM;19.4423.C813.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.C813.24-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-24-830-line-1s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-24-830-LINE-1S-L-1996MM.ies;1996;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 24 840 LINE-1BM / L-1998MM;19.4423.G823.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.G823.24-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-24-840-line-1bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-24-840-LINE-1BM-L-1998MM.ies;1998;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 24 840 LINE-1S / L-1996MM;19.4423.C823.24;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_aluminum;LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.C823.24-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-24-840-line-1s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-24-840-LINE-1S-L-1996MM.ies;1996;34;68;230;4000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 34 830 LINE-1BM / L-1998MM;19.4423.G813.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.G813.34-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-34-830-line-1bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-34-830-LINE-1BM-L-1998MM.ies;1998;34;68;230;3000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 34 830 LINE-1S / L-1996MM;19.4423.C813.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3443.4;108.3;145000;L90/B10;3000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.C813.34-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-34-830-line-1s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-34-830-LINE-1S-L-1996MM.ies;1996;34;68;230;3000;0;1
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 34 840 LINE-1BM / L-1998MM;19.4423.G823.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1998 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.G823.34-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-34-840-line-1bm-l-1998mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-34-840-LINE-1BM-L-1998MM.ies;1998;34;68;230;4000;1;0
X-LINE SLIGHT SURFACE LOW UGR LED 5000 LOUVER EDD 34 840 LINE-1S / L-1996MM;19.4423.C823.34;surface mounted on ceiling;LUXIONA_aluminum;LUXIONA_RAL 9016 (white);LUXIONA_LOUVER (anti-glare louver);1996 x 34 x 68;220..240 V, 50..60 Hz;DIM DALI (EDD);LED;5 ÷ 35;31.8;3624.4;114;145000;L90/B10;4000;>80;3;(C0-C180) / (C90-C270) - 46° / 44,6°;IP40;IK04;I;RG0;0.716609;0.95;LUXIONA;https://luxiona.com/products/x-line-slight-surface-low-ugr-led-line;https://luxiona.com/files/Pim/PDF-karta-produktu/Luxiona-19.4423.C823.34-en-x-line-slight-surface-low-ugr-led-5000-louver-edd-34-840-line-1s-l-1996mm.pdf;X-LINE-SLIGHT-SURFACE-LOW-UGR-LED-5000-LOUVER-EDD-34-840-LINE-1S-L-1996MM.ies;1996;34;68;230;4000;0;1
