;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
X-LINE SLIM L-DOWN LED 2600 MICRO-PRM E 24 840 / L-1138MM S-1,5M;Surface mounted luminaires;19.3107.0001.24;1138 x 48 x 70;surface mounted on slings;14.4;1945;135;4000;4000;0.7432;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1138;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0001.24/;19.3107.0001.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 2600 MICRO-PRM EDD 24 840 / L-1138MM S-1,5M;Surface mounted luminaires;19.3107.0002.24;1138 x 48 x 70;surface mounted on slings;14.4;1945;135;4000;4000;0.7432;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1138;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0002.24/;19.3107.0002.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 2600 OPTICS-ASYM E 24 830 / L-1144MM S-1,5M;Surface mounted luminaires;19.3219.0061.24;1144 x 48 x 70;surface mounted on slings;14.4;1995;139;3000;3000;0.7901;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-20°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0061.24/;19.3219.0061.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 2600 OPTICS-ASYM E 24 840 / L-1144MM S-1,5M;Surface mounted luminaires;19.3219.0062.24;1144 x 48 x 70;surface mounted on slings;14.4;2068;144;4000;4000;0.7901;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-20°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0062.24/;19.3219.0062.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 2600 OPTICS-ASYM EDD 24 830 / L-1144MM S-1,5M;Surface mounted luminaires;19.3219.0063.24;1144 x 48 x 70;surface mounted on slings;14.4;1995;139;3000;3000;0.7901;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-20°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0063.24/;19.3219.0063.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 2600 OPTICS-ASYM EDD 24 840 / L-1144MM S-1,5M;Surface mounted luminaires;19.3219.0064.24;1144 x 48 x 70;surface mounted on slings;14.4;2068;144;4000;4000;0.7901;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-20°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0064.24/;19.3219.0064.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 2600 OPTICS-WIDE E 24 830 / L-1144MM S-1,5M;Surface mounted luminaires;19.3219.0011.24;1144 x 48 x 70;surface mounted on slings;14.4;2107;146;3000;3000;0.8344;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 101,8° / 88,4°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0011.24/;19.3219.0011.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 2600 OPTICS-WIDE E 24 840 / L-1144MM S-1,5M;Surface mounted luminaires;19.3219.0012.24;1144 x 48 x 70;surface mounted on slings;14.4;2184;152;4000;4000;0.8344;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 101,8° / 88,4°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0012.24/;19.3219.0012.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 2600 OPTICS-WIDE EDD 24 830 / L-1144MM S-1,5M;Surface mounted luminaires;19.3219.0013.24;1144 x 48 x 70;surface mounted on slings;14.4;2107;146;3000;3000;0.8344;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 101,8° / 88,4°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0013.24/;19.3219.0013.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 2600 OPTICS-WIDE EDD 24 840 / L-1144MM S-1,5M;Surface mounted luminaires;19.3219.0014.24;1144 x 48 x 70;surface mounted on slings;14.4;2184;152;4000;4000;0.8344;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 101,8° / 88,4°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0014.24/;19.3219.0014.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 2600 PLX E 24 840 / L-1138MM S-1,5M;Surface mounted luminaires;19.3107.0003.24;1138 x 48 x 70;surface mounted on slings;14.4;1679;117;4000;4000;0.6416;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1138;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0003.24/;19.3107.0003.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 2600 PLX EDD 24 840 / L-1138MM S-1,5M;Surface mounted luminaires;19.3107.0004.24;1138 x 48 x 70;surface mounted on slings;14.4;1679;117;4000;4000;0.6416;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1138;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0004.24/;19.3107.0004.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 3250 OPTICS-ASYM E 24 830 / L-1425MM S-1,5M;Surface mounted luminaires;19.3219.0065.24;1425 x 48 x 70;surface mounted on slings;18.3;2495;136;3000;3000;0.7901;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-20°;IP40;IK04;I;-;0,95;1425;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0065.24/;19.3219.0065.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 3250 OPTICS-ASYM E 24 840 / L-1425MM S-1,5M;Surface mounted luminaires;19.3219.0066.24;1425 x 48 x 70;surface mounted on slings;18.3;2586;141;4000;4000;0.7901;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-20°;IP40;IK04;I;-;0,95;1425;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0066.24/;19.3219.0066.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 3250 OPTICS-ASYM EDD 24 830 / L-1425MM S-1,5M;Surface mounted luminaires;19.3219.0067.24;1425 x 48 x 70;surface mounted on slings;18.3;2495;136;3000;3000;0.7901;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-20°;IP40;IK04;I;-;0,95;1425;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0067.24/;19.3219.0067.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 3250 OPTICS-ASYM EDD 24 840 / L-1425MM S-1,5M;Surface mounted luminaires;19.3219.0068.24;1425 x 48 x 70;surface mounted on slings;18.3;2586;141;4000;4000;0.7901;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-20°;IP40;IK04;I;-;0,95;1425;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0068.24/;19.3219.0068.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 3250 OPTICS-WIDE E 24 830 / L-1425MM S-1,5M;Surface mounted luminaires;19.3219.0016.24;1425 x 48 x 70;surface mounted on slings;18.3;2635;144;3000;3000;0.8344;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 101,8° / 88,4°;IP40;IK04;I;-;0,95;1425;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0016.24/;19.3219.0016.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 3250 OPTICS-WIDE E 24 840 / L-1425MM S-1,5M;Surface mounted luminaires;19.3219.0017.24;1425 x 48 x 70;surface mounted on slings;18.3;2731;149;4000;4000;0.8344;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 101,8° / 88,4°;IP40;IK04;I;-;0,95;1425;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0017.24/;19.3219.0017.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 3250 OPTICS-WIDE EDD 24 830 / L-1425MM S-1,5M;Surface mounted luminaires;19.3219.0018.24;1425 x 48 x 70;surface mounted on slings;18.3;2635;144;3000;3000;0.8344;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 101,8° / 88,4°;IP40;IK04;I;-;0,95;1425;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0018.24/;19.3219.0018.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 3250 OPTICS-WIDE EDD 24 840 / L-1425MM S-1,5M;Surface mounted luminaires;19.3219.0019.24;1425 x 48 x 70;surface mounted on slings;18.3;2731;149;4000;4000;0.8344;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 101,8° / 88,4°;IP40;IK04;I;-;0,95;1425;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0019.24/;19.3219.0019.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 3900 MICRO-PRM E 24 840 / L-1698MM S-1,5M;Surface mounted luminaires;19.3107.0005.24;1698 x 48 x 70;surface mounted on slings;21.7;2918;134;4000;4000;0.7432;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1698;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0005.24/;19.3107.0005.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 3900 MICRO-PRM EDD 24 840 / L-1698MM S-1,5M;Surface mounted luminaires;19.3107.0006.24;1698 x 48 x 70;surface mounted on slings;21.7;2918;134;4000;4000;0.7432;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1698;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0006.24/;19.3107.0006.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 3900 PLX E 24 840 / L-1698MM S-1,5M;Surface mounted luminaires;19.3107.0007.24;1698 x 48 x 70;surface mounted on slings;21.7;2519;116;4000;4000;0.6416;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1698;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0007.24/;19.3107.0007.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 3900 PLX EDD 24 840 / L-1698MM S-1,5M;Surface mounted luminaires;19.3107.0008.24;1698 x 48 x 70;surface mounted on slings;21.7;2519;116;4000;4000;0.6416;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1698;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0008.24/;19.3107.0008.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 4400 MICRO-PRM E 24 840 / L-1138MM S-1,5M;Surface mounted luminaires;19.3107.0009.24;1138 x 48 x 70;surface mounted on slings;24.7;3393;137;4000;4000;0.7432;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1138;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0009.24/;19.3107.0009.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 4400 MICRO-PRM EDD 24 840 / L-1138MM S-1,5M;Surface mounted luminaires;19.3107.0010.24;1138 x 48 x 70;surface mounted on slings;24.7;3393;137;4000;4000;0.7432;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1138;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0010.24/;19.3107.0010.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 4400 OPTICS-ASYM E 24 830 / L-1144MM S-1,5M;Surface mounted luminaires;19.3219.0069.24;1144 x 48 x 70;surface mounted on slings;24.7;3481;141;3000;3000;0.7901;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-20°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0069.24/;19.3219.0069.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 4400 OPTICS-ASYM E 24 840 / L-1144MM S-1,5M;Surface mounted luminaires;19.3219.0070.24;1144 x 48 x 70;surface mounted on slings;24.7;3607;146;4000;4000;0.7901;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-20°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0070.24/;19.3219.0070.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 4400 OPTICS-ASYM EDD 24 827-865 / L-1144MM S-1,5M TUNABLE WHITE;Surface mounted luminaires;19.3219.0073.24;1144 x 48 x 70;surface mounted on slings;32;3614;113;4000;2700÷6500;0.7901;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;50000;L80/B10;>80;3;asymmetric light distribution - Imax=-20°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0073.24/;19.3219.0073.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 4400 OPTICS-ASYM EDD 24 830 / L-1144MM S-1,5M;Surface mounted luminaires;19.3219.0071.24;1144 x 48 x 70;surface mounted on slings;24.7;3481;141;3000;3000;0.7901;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-20°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0071.24/;19.3219.0071.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 4400 OPTICS-ASYM EDD 24 840 / L-1144MM S-1,5M;Surface mounted luminaires;19.3219.0072.24;1425 x 48 x 70;surface mounted on slings;24.7;3607;146;4000;4000;0.7901;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-20°;IP40;IK04;I;-;0,95;1425;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0072.24/;19.3219.0072.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 4400 OPTICS-WIDE E 24 830 / L-1144MM S-1,5M;Surface mounted luminaires;19.3219.0021.24;1144 x 48 x 70;surface mounted on slings;24.7;3676;149;3000;3000;0.8344;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 101,8° / 88,4°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0021.24/;19.3219.0021.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 4400 OPTICS-WIDE E 24 840 / L-1144MM S-1,5M;Surface mounted luminaires;19.3219.0022.24;1144 x 48 x 70;surface mounted on slings;24.7;3809;154;4000;4000;0.8344;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 101,8° / 88,4°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0022.24/;19.3219.0022.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 4400 OPTICS-WIDE EDD 24 827-865 / L-1144MM S-1,5M TUNABLE WHITE;Surface mounted luminaires;19.3219.0025.24;1144 x 48 x 70;surface mounted on slings;32;3817;119;4000;2700÷6500;0.8344;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;50000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 101,8° / 88,4°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0025.24/;19.3219.0025.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 4400 OPTICS-WIDE EDD 24 830 / L-1144MM S-1,5M;Surface mounted luminaires;19.3219.0023.24;1144 x 48 x 70;surface mounted on slings;24.7;3676;149;3000;3000;0.8344;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 101,8° / 88,4°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0023.24/;19.3219.0023.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 4400 OPTICS-WIDE EDD 24 840 / L-1144MM S-1,5M;Surface mounted luminaires;19.3219.0024.24;1144 x 48 x 70;surface mounted on slings;24.7;3809;154;4000;4000;0.8344;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 101,8° / 88,4°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0024.24/;19.3219.0024.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 4400 PLX E 24 840 / L-1138MM S-1,5M;Surface mounted luminaires;19.3107.0011.24;1138 x 48 x 70;surface mounted on slings;24.7;2929;119;4000;4000;0.6416;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1138;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0011.24/;19.3107.0011.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 4400 PLX EDD 24 840 / L-1138MM S-1,5M;Surface mounted luminaires;19.3107.0012.24;1138 x 48 x 70;surface mounted on slings;24.7;2929;119;4000;4000;0.6416;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1138;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0012.24/;19.3107.0012.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 5200 MICRO-PRM E 24 840 / L-2258MM S-1,5M;Surface mounted luminaires;19.3107.0013.24;2258 x 48 x 70;surface mounted on slings;28.2;3890;138;4000;4000;0.7432;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;2258;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0013.24/;19.3107.0013.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 5200 MICRO-PRM EDD 24 840 / L-2258MM S-1,5M;Surface mounted luminaires;19.3107.0014.24;2258 x 48 x 70;surface mounted on slings;28.2;3890;138;4000;4000;0.7432;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;2258;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0014.24/;19.3107.0014.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 5200 PLX E 24 840 / L-2258MM S-1,5M;Surface mounted luminaires;19.3107.0015.24;2258 x 48 x 70;surface mounted on slings;28.2;3358;119;4000;4000;0.6416;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;2258;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0015.24/;19.3107.0015.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 5200 PLX EDD 24 840 / L-2258MM S-1,5M;Surface mounted luminaires;19.3107.0016.24;2258 x 48 x 70;surface mounted on slings;28.2;3358;119;4000;4000;0.6416;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;2258;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0016.24/;19.3107.0016.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 5500 OPTICS-ASYM E 24 830 / L-1425MM S-1,5M;Surface mounted luminaires;19.3219.0074.24;1425 x 48 x 70;surface mounted on slings;30.5;4366;143;3000;3000;0.7901;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-20°;IP40;IK04;I;-;0,95;1425;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0074.24/;19.3219.0074.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 5500 OPTICS-ASYM E 24 840 / L-1425MM S-1,5M;Surface mounted luminaires;19.3219.0075.24;1425 x 48 x 70;surface mounted on slings;30.5;4525;148;4000;4000;0.7901;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-20°;IP40;IK04;I;-;0,95;1425;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0075.24/;19.3219.0075.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 5500 OPTICS-ASYM EDD 24 827-865 / L-1425MM S-1,5M TUNABLE WHITE;Surface mounted luminaires;19.3219.0078.24;1425 x 48 x 70;surface mounted on slings;40;4517;113;4000;2700÷6500;0.7901;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;50000;L80/B10;>80;3;asymmetric light distribution - Imax=-20°;IP40;IK04;I;-;0,95;1425;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0078.24/;19.3219.0078.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 5500 OPTICS-ASYM EDD 24 830 / L-1425MM S-1,5M;Surface mounted luminaires;19.3219.0076.24;1425 x 48 x 70;surface mounted on slings;30.5;4366;143;3000;3000;0.7901;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-20°;IP40;IK04;I;-;0,95;1425;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0076.24/;19.3219.0076.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 5500 OPTICS-ASYM EDD 24 840 / L-1425MM S-1,5M;Surface mounted luminaires;19.3219.0077.24;1425 x 48 x 70;surface mounted on slings;30.5;4525;148;4000;4000;0.7901;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-20°;IP40;IK04;I;-;0,95;1425;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0077.24/;19.3219.0077.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 5500 OPTICS-WIDE E 24 830 / L-1425MM S-1,5M;Surface mounted luminaires;19.3219.0026.24;1425 x 48 x 70;surface mounted on slings;30.5;4611;151;3000;3000;0.8344;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 101,8° / 88,4°;IP40;IK04;I;-;0,95;1425;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0026.24/;19.3219.0026.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 5500 OPTICS-WIDE E 24 840 / L-1425MM S-1,5M;Surface mounted luminaires;19.3219.0027.24;1425 x 48 x 70;surface mounted on slings;30.5;4779;157;4000;4000;0.8344;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 101,8° / 88,4°;IP40;IK04;I;-;0,95;1425;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0027.24/;19.3219.0027.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 5500 OPTICS-WIDE EDD 24 827-865 / L-1425MM S-1,5M TUNABLE WHITE;Surface mounted luminaires;19.3219.0030.24;1425 x 48 x 70;surface mounted on slings;40;4770;119;4000;2700÷6500;0.8344;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;50000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 101,8° / 88,4°;IP40;IK04;I;-;0,95;1425;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0030.24/;19.3219.0030.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 5500 OPTICS-WIDE EDD 24 830 / L-1425MM S-1,5M;Surface mounted luminaires;19.3219.0028.24;1425 x 48 x 70;surface mounted on slings;30.5;4611;151;3000;3000;0.8344;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 101,8° / 88,4°;IP40;IK04;I;-;0,95;1425;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0028.24/;19.3219.0028.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 5500 OPTICS-WIDE EDD 24 840 / L-1425MM S-1,5M;Surface mounted luminaires;19.3219.0029.24;1425 x 48 x 70;surface mounted on slings;30.5;4779;157;4000;4000;0.8344;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 101,8° / 88,4°;IP40;IK04;I;-;0,95;1425;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3219.0029.24/;19.3219.0029.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 6600 MICRO-PRM E 24 840 / L-1698MM S-1,5M;Surface mounted luminaires;19.3107.0017.24;1698 x 48 x 70;surface mounted on slings;35.3;5089;144;4000;4000;0.7432;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1698;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0017.24/;19.3107.0017.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 6600 MICRO-PRM EDD 24 840 / L-1698MM S-1,5M;Surface mounted luminaires;19.3107.0018.24;1698 x 48 x 70;surface mounted on slings;35.3;5089;144;4000;4000;0.7432;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1698;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0018.24/;19.3107.0018.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 6600 PLX E 24 840 / L-1698MM S-1,5M;Surface mounted luminaires;19.3107.0019.24;1698 x 48 x 70;surface mounted on slings;35.3;4394;124;4000;4000;0.6416;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1698;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0019.24/;19.3107.0019.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 6600 PLX EDD 24 840 / L-1698MM S-1,5M;Surface mounted luminaires;19.3107.0020.24;1698 x 48 x 70;surface mounted on slings;35.3;4394;124;4000;4000;0.6416;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1698;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0020.24/;19.3107.0020.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 8800 MICRO-PRM E 24 840 / L-2258MM S-1,5M;Surface mounted luminaires;19.3107.0021.24;2258 x 48 x 70;surface mounted on slings;49.1;6785;138;4000;4000;0.7432;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;2258;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0021.24/;19.3107.0021.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 8800 MICRO-PRM EDD 24 840 / L-2258MM S-1,5M;Surface mounted luminaires;19.3107.0022.24;2258 x 48 x 70;surface mounted on slings;49.1;6785;138;4000;4000;0.7432;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;2258;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0022.24/;19.3107.0022.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 8800 PLX E 24 840 / L-2258MM S-1,5M;Surface mounted luminaires;19.3107.0023.24;2258 x 48 x 70;surface mounted on slings;49.1;5858;119;4000;4000;0.6416;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;2258;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0023.24/;19.3107.0023.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED 8800 PLX EDD 24 840 / L-2258MM S-1,5M;Surface mounted luminaires;19.3107.0024.24;2258 x 48 x 70;surface mounted on slings;49.1;5858;119;4000;4000;0.6416;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;2258;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-led/19.3107.0024.24/;19.3107.0024.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
