;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
X-LINE SLIM L-DOWN LED COMPACT 4000 MICRO-PRM E 04 840 / L-1418MM S-1,5M;Compact;19.3253.0047.04;1418 x 48 x 70;surface mounted on slings;26;3237;124;4000;4000;0.7432;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_Micro-PRM;LED;5 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1418;48;70;0;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/19.3253.0047.04/;19.3253.0047.04_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED COMPACT 4000 MICRO-PRM E 24 840 / L-1138MM S-1,5M;Compact;19.3253.0001.24;1138 x 48 x 70;surface mounted on slings;26;3237;124;4000;4000;0.7432;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;5 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1138;48;70;0;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/19.3253.0001.24/;19.3253.0001.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED COMPACT 4000 MICRO-PRM E 24 840 / L-1418MM S-1,5M;Compact;19.3253.0047.24;1418 x 48 x 70;surface mounted on slings;26;3237;124;4000;4000;0.7432;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;5 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1418;48;70;0;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/19.3253.0047.24/;19.3253.0047.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED COMPACT 4000 MICRO-PRM E 34 840 / L-1418MM S-1,5M;Compact;19.3253.0047.34;1418 x 48 x 70;surface mounted on slings;26;3237;124;4000;4000;0.7432;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1418;48;70;0;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/19.3253.0047.34/;19.3253.0047.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED COMPACT 4000 PLX E 04 840 / L-1418MM S-1,5M;Compact;19.3253.0046.04;1418 x 48 x 70;surface mounted on slings;26;2794;107;4000;4000;0.6416;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1418;48;70;0;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/19.3253.0046.04/;19.3253.0046.04_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED COMPACT 4000 PLX E 24 840 / L-1138MM S-1,5M;Compact;19.3253.0002.24;1138 x 48 x 70;surface mounted on slings;26;2794;107;4000;4000;0.6416;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1138;48;70;0;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/19.3253.0002.24/;19.3253.0002.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED COMPACT 4000 PLX E 24 840 / L-1418MM S-1,5M;Compact;19.3253.0046.24;1418 x 48 x 70;surface mounted on slings;26;2794;107;4000;4000;0.6416;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1418;48;70;0;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/19.3253.0046.24/;19.3253.0046.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED COMPACT 4000 PLX E 34 840 / L-1418MM S-1,5M;Compact;19.3253.0046.34;1418 x 48 x 70;surface mounted on slings;26;2794;107;4000;4000;0.6416;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1418;48;70;0;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/19.3253.0046.34/;19.3253.0046.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED COMPACT 6000 MICRO-PRM E 24 840 / L-1418MM S-1,5M;Compact;19.3253.0031.24;1418 x 48 x 70;surface mounted on slings;43;4638;108;4000;4000;0.7432;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;5 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1418;48;70;0;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/19.3253.0031.24/;19.3253.0031.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM L-DOWN LED COMPACT 6000 PLX E 24 840 / L-1418MM S-1,5M;Compact;19.3253.0029.24;1418 x 48 x 70;surface mounted on slings;43;4004;93;4000;4000;0.6416;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1418;48;70;0;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/;https://luxiona.pl/en/oferta/compact/x-line-slim-led-compact/19.3253.0029.24/;19.3253.0029.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
