;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
X-LINE SLIM LOW UGR L-DOWN LED 4200 RASTER DAISY-BLACK-WIDE E 04 840 / L-1144MM S-1,5M;Surface mounted luminaires;19.3113.0001.04;1144 x 48 x 70;surface mounted on slings;26;3445;133;4000;4000;0.8298;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/19.3113.0001.04/;19.3113.0001.04_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM LOW UGR L-DOWN LED 4200 RASTER DAISY-BLACK-WIDE E 24 840 / L-1144MM S-1,5M;Surface mounted luminaires;19.3113.0001.24;1144 x 48 x 70;surface mounted on slings;26;3445;133;4000;4000;0.8298;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/19.3113.0001.24/;19.3113.0001.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM LOW UGR L-DOWN LED 4200 RASTER DAISY-BLACK-WIDE E 34 840 / L-1144MM S-1,5M;Surface mounted luminaires;19.3113.0001.34;1144 x 48 x 70;surface mounted on slings;26;3445;133;4000;4000;0.8298;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/19.3113.0001.34/;19.3113.0001.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM LOW UGR L-DOWN LED 4200 RASTER DAISY-BLACK-WIDE EDD 04 840 / L-1144MM S-1,5M;Surface mounted luminaires;19.3113.0002.04;1144 x 48 x 70;surface mounted on slings;26;3445;133;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/19.3113.0002.04/;19.3113.0002.04_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM LOW UGR L-DOWN LED 4200 RASTER DAISY-BLACK-WIDE EDD 24 840 / L-1144MM S-1,5M;Surface mounted luminaires;19.3113.0002.24;1144 x 48 x 70;surface mounted on slings;26;3445;133;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/19.3113.0002.24/;19.3113.0002.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM LOW UGR L-DOWN LED 4200 RASTER DAISY-BLACK-WIDE EDD 34 840 / L-1145MM S-1,5M;Surface mounted luminaires;19.3113.0002.34;1144 x 48 x 70;surface mounted on slings;26;3445;133;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,95;1144;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/19.3113.0002.34/;19.3113.0002.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM LOW UGR L-DOWN LED 5250 RASTER DAISY-BLACK-WIDE E 04 840 / L-1424MM S-1,5M;Surface mounted luminaires;19.3113.0003.04;1424 x 48 x 70;surface mounted on slings;32;3788;118;4000;4000;0.8298;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,95;1424;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/19.3113.0003.04/;19.3113.0003.04_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM LOW UGR L-DOWN LED 5250 RASTER DAISY-BLACK-WIDE E 24 840 / L-1424MM S-1,5M;Surface mounted luminaires;19.3113.0003.24;1424 x 48 x 70;surface mounted on slings;32;3788;118;4000;4000;0.8298;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,95;1424;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/19.3113.0003.24/;19.3113.0003.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM LOW UGR L-DOWN LED 5250 RASTER DAISY-BLACK-WIDE E 34 840 / L-1424MM S-1,5M;Surface mounted luminaires;19.3113.0003.34;1424 x 48 x 70;surface mounted on slings;32;3788;118;4000;4000;0.8298;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,95;1424;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/19.3113.0003.34/;19.3113.0003.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM LOW UGR L-DOWN LED 5250 RASTER DAISY-BLACK-WIDE EDD 04 840 / L-1424MM S-1,5M;Surface mounted luminaires;19.3113.0004.04;1424 x 48 x 70;surface mounted on slings;32;3788;118;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,95;1424;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/19.3113.0004.04/;19.3113.0004.04_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM LOW UGR L-DOWN LED 5250 RASTER DAISY-BLACK-WIDE EDD 24 840 / L-1424MM S-1,5M;Surface mounted luminaires;19.3113.0004.24;1424 x 48 x 70;surface mounted on slings;32;3788;118;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,95;1424;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/19.3113.0004.24/;19.3113.0004.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM LOW UGR L-DOWN LED 5250 RASTER DAISY-BLACK-WIDE EDD 34 840 / L-1424MM S-1,5M;Surface mounted luminaires;19.3113.0004.34;1424 x 48 x 70;surface mounted on slings;32;3788;118;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,95;1424;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/19.3113.0004.34/;19.3113.0004.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM LOW UGR L-DOWN LED 8400 RASTER DAISY-BLACK-WIDE E 04 840 / L-2270MM S-1,5M;Surface mounted luminaires;19.3113.0005.04;2266 x 48 x 70;surface mounted on slings;45;6346;141;4000;4000;0.8298;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,95;2266;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/19.3113.0005.04/;19.3113.0005.04_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM LOW UGR L-DOWN LED 8400 RASTER DAISY-BLACK-WIDE E 24 840 / L-2270MM S-1,5M;Surface mounted luminaires;19.3113.0005.24;2266 x 48 x 70;surface mounted on slings;45;6346;141;4000;4000;0.8298;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,95;2266;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/19.3113.0005.24/;19.3113.0005.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM LOW UGR L-DOWN LED 8400 RASTER DAISY-BLACK-WIDE E 34 840 / L-2270MM S-1,5M;Surface mounted luminaires;19.3113.0005.34;2266 x 48 x 70;surface mounted on slings;45;6346;141;4000;4000;0.8298;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,95;2266;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/19.3113.0005.34/;19.3113.0005.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM LOW UGR L-DOWN LED 8400 RASTER DAISY-BLACK-WIDE EDD 04 840 / L-2270MM S-1,5M;Surface mounted luminaires;19.3113.0006.04;2266 x 48 x 70;surface mounted on slings;45;6346;141;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9005 (black);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,95;2266;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/19.3113.0006.04/;19.3113.0006.04_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM LOW UGR L-DOWN LED 8400 RASTER DAISY-BLACK-WIDE EDD 24 840 / L-2270MM S-1,5M;Surface mounted luminaires;19.3113.0006.24;2266 x 48 x 70;surface mounted on slings;45;6346;141;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,95;2266;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/19.3113.0006.24/;19.3113.0006.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM LOW UGR L-DOWN LED 8400 RASTER DAISY-BLACK-WIDE EDD 34 840 / L-2270MM S-1,5M;Surface mounted luminaires;19.3113.0006.34;2266 x 48 x 70;surface mounted on slings;45;6346;141;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_RASTER (anti-glare louvre);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,95;2266;48;70;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-low-ugr-l-down-led/19.3113.0006.34/;19.3113.0006.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
