;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
X-LINE SLIM RECESSED LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE E 34 830 / L-1164MM;Recessed luminaires;19.3218.0011.34;1164 x 70 x 75;mounted in plasterboard ceilings;26;3269;126;3000;3000;0.8298;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,9;1164;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-low-ugr-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-low-ugr-led/19.3218.0011.34/;19.3218.0011.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE E 34 840 / L-1164MM;Recessed luminaires;19.3218.0012.34;1164 x 70 x 75;mounted in plasterboard ceilings;26;3445;133;4000;4000;0.8298;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,9;1164;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-low-ugr-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-low-ugr-led/19.3218.0012.34/;19.3218.0012.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE EDD 34 827-865 / L-1164MM TUNABLE WHITE;Recessed luminaires;19.3218.0015.34;1164 x 70 x 75;mounted in plasterboard ceilings;46;5510;120;4000;2700 ÷ 6500;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;50000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,9;1164;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-low-ugr-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-low-ugr-led/19.3218.0015.34/;19.3218.0015.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE EDD 34 830 / L-1164MM;Recessed luminaires;19.3218.0013.34;1164 x 70 x 75;mounted in plasterboard ceilings;26;3269;126;3000;3000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,9;1164;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-low-ugr-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-low-ugr-led/19.3218.0013.34/;19.3218.0013.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LOW UGR LED 4200 RASTER DAISY-BLACK-WIDE EDD 34 840 / L-1164MM;Recessed luminaires;19.3218.0014.34;1164 x 70 x 75;mounted in plasterboard ceilings;26;3445;133;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,9;1164;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-low-ugr-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-low-ugr-led/19.3218.0014.34/;19.3218.0014.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LOW UGR LED 5250 RASTER DAISY-BLACK-WIDE E 34 830 / L-1444MM;Recessed luminaires;19.3218.0016.34;1444 x 70 x 75;mounted in plasterboard ceilings;33;4087;124;3000;3000;0.8298;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,9;1444;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-low-ugr-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-low-ugr-led/19.3218.0016.34/;19.3218.0016.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LOW UGR LED 5250 RASTER DAISY-BLACK-WIDE E 34 840 / L-1444MM;Recessed luminaires;19.3218.0017.34;1444 x 70 x 75;mounted in plasterboard ceilings;33;4307;131;4000;4000;0.8298;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,9;1444;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-low-ugr-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-low-ugr-led/19.3218.0017.34/;19.3218.0017.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LOW UGR LED 5250 RASTER DAISY-BLACK-WIDE EDD 34 830 / L-1444MM;Recessed luminaires;19.3218.0018.34;1444 x 70 x 75;mounted in plasterboard ceilings;33;4087;124;3000;3000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,9;1444;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-low-ugr-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-low-ugr-led/19.3218.0018.34/;19.3218.0018.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LOW UGR LED 5250 RASTER DAISY-BLACK-WIDE EDD 34 840 / L-1444MM;Recessed luminaires;19.3218.0019.34;1444 x 70 x 75;mounted in plasterboard ceilings;33;4307;131;4000;4000;0.8298;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 72,6° / 74,4°;IP40;IK04;I;-;0,9;1444;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-low-ugr-led/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-low-ugr-led/19.3218.0019.34/;19.3218.0019.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
