;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##;EP##OTHER##;EL##OTHER##
X-LINE SLIM UP&DOWN LED 1300/1300 PC/MICRO-PRM E 24 840 LINE-S / L-580mm S-1,5M;Surface mounted luminaires;19.3110.0003.24;564 x 48 x 70;surface mounted on slings;14.4;1881;131;4000;4000;0.7188;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;564;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0003.24/;19.3110.0003.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 1300/1300 PC/MICRO-PRM EDD 24 840 LINE-1S / L-580mm S-1,5M;Surface mounted luminaires;19.3110.0006.24;564 x 48 x 70;surface mounted on slings;14.4;1881;131;4000;4000;0.7188;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;564;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0006.24/;19.3110.0006.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 1300/1300 PC/PLX E 24 840 LINE-S / L-580mm S-1,5M;Surface mounted luminaires;19.3110.0009.24;564 x 48 x 70;surface mounted on slings;14.4;1748;121;4000;4000;0.6678;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;564;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0009.24/;19.3110.0009.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 1300/1300 PC/PLX EDD 24 840 LINE-1S / L-580mm S-1,5M;Surface mounted luminaires;19.3110.0012.24;564 x 48 x 70;surface mounted on slings;14.4;1748;121;4000;4000;0.6678;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;564;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0012.24/;19.3110.0012.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 2600/2600 PC/MICRO-PRM E 24 840 LINE-S / L-1140mm S-1,5M;Surface mounted luminaires;19.3110.0015.24;1124 x 48 x 70;surface mounted on slings;34;4083;120;4000;4000;0.7188;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1124;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0015.24/;19.3110.0015.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 2600/2600 PC/MICRO-PRM EDD 24 840 LINE-1S / L-1140mm S-1,5M;Surface mounted luminaires;19.3110.0018.24;1124 x 48 x 70;surface mounted on slings;34;4083;120;4000;4000;0.7188;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1124;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0018.24/;19.3110.0018.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 2600/2600 PC/PLX E 24 840 LINE-S / L-1140mm S-1,5M;Surface mounted luminaires;19.3110.0021.24;1124 x 48 x 70;surface mounted on slings;34;3793;112;4000;4000;0.6678;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1124;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0021.24/;19.3110.0021.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 2600/2600 PC/PLX EDD 24 840 LINE-1S / L-1140mm S-1,5M;Surface mounted luminaires;19.3110.0024.24;1124 x 48 x 70;surface mounted on slings;34;3793;112;4000;4000;0.6678;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1124;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0024.24/;19.3110.0024.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 3900/3900 PC/MICRO-PRM E 24 840 LINE-S / L-1700mm S-1,5M;Surface mounted luminaires;19.3110.0027.24;1684 x 48 x 70;surface mounted on slings;52;6124;118;4000;4000;0.7188;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1684;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0027.24/;19.3110.0027.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 3900/3900 PC/MICRO-PRM EDD 24 840 LINE-1S / L-1700mm S-1,5M;Surface mounted luminaires;19.3110.0030.24;1684 x 48 x 70;surface mounted on slings;52;6124;118;4000;4000;0.7188;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1684;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0030.24/;19.3110.0030.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 3900/3900 PC/PLX E 24 840 LINE-S / L-1700mm S-1,5M;Surface mounted luminaires;19.3110.0033.24;1684 x 48 x 70;surface mounted on slings;52;5690;109;4000;4000;0.6678;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1684;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0033.24/;19.3110.0033.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 3900/3900 PC/PLX EDD 24 840 LINE-1S / L-1700mm S-1,5M;Surface mounted luminaires;19.3110.0036.24;1684 x 48 x 70;surface mounted on slings;52;5690;109;4000;4000;0.6678;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1684;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0036.24/;19.3110.0036.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 5200/5200 PC/MICRO-PRM E 24 840 LINE-S / L-2244mm S-1,5M;Surface mounted luminaires;19.3110.0039.24;2244 x 48 x 70;surface mounted on slings;68;8166;120;4000;4000;0.7188;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;2244;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0039.24/;19.3110.0039.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 5200/5200 PC/MICRO-PRM EDD 24 840 LINE-1S / L-2244mm S-1,5M;Surface mounted luminaires;19.3110.0042.24;2244 x 48 x 70;surface mounted on slings;68;8166;120;4000;4000;0.7188;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;2244;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0042.24/;19.3110.0042.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 5200/5200 PC/PLX E 24 840 LINE-S / L-2244mm S-1,5M;Surface mounted luminaires;19.3110.0045.24;2244 x 48 x 70;surface mounted on slings;68;7586;112;4000;4000;0.6678;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;2244;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0045.24/;19.3110.0045.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 5200/5200 PC/PLX EDD 24 840 LINE-1S / L-2244mm S-1,5M;Surface mounted luminaires;19.3110.0048.24;2244 x 48 x 70;surface mounted on slings;68;7586;112;4000;4000;0.6678;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;2244;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0048.24/;19.3110.0048.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 7800/7800 PC/MICRO-PRM E 24 840 LINE-S / L-3395mm S-1,5M;Surface mounted luminaires;19.3110.0049.24;3395 x 48 x 70;surface mounted on slings;102;12248;120;4000;4000;0.7188;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;3395;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0049.24/;19.3110.0049.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 7800/7800 PC/MICRO-PRM EDD 24 840 LINE-S / L-3395mm S-1,5M;Surface mounted luminaires;19.3110.0050.24;3395 x 48 x 70;surface mounted on slings;102;12248;120;4000;4000;0.7188;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;3395;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0050.24/;19.3110.0050.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 7800/7800 PC/PLX E 24 840 LINE-S / L-3395mm S-1,5M;Surface mounted luminaires;19.3110.0051.24;3395 x 48 x 70;surface mounted on slings;102;11379;112;4000;4000;0.6678;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;3395;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0051.24/;19.3110.0051.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 7800/7800 PC/PLX EDD 24 840 LINE-S / L-3395mm S-1,5M;Surface mounted luminaires;19.3110.0052.24;3395 x 48 x 70;surface mounted on slings;102;11379;112;4000;4000;0.6678;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;3395;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0052.24/;19.3110.0052.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
X-LINE SLIM UP&DOWN LED 1300/1300 PC/MICRO-PRM E 24 840 LINE-EL / L-582mm S-1,5M;Surface mounted luminaires;19.3110.0001.24;572 x 48 x 70;surface mounted on slings;14.4;1881;131;4000;4000;0.7188;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;572;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0001.24/;19.3110.0001.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
X-LINE SLIM UP&DOWN LED 1300/1300 PC/MICRO-PRM EDD 24 840 LINE-1EL / L-582mm S-1,5M;Surface mounted luminaires;19.3110.0004.24;572 x 48 x 70;surface mounted on slings;14.4;1881;131;4000;4000;0.7188;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;572;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0004.24/;19.3110.0004.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
X-LINE SLIM UP&DOWN LED 1300/1300 PC/PLX E 24 840 LINE-EL / L-582mm S-1,5M;Surface mounted luminaires;19.3110.0007.24;572 x 48 x 70;surface mounted on slings;14.4;1748;121;4000;4000;0.6678;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;572;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0007.24/;19.3110.0007.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
X-LINE SLIM UP&DOWN LED 1300/1300 PC/PLX EDD 24 840 LINE-1EL / L-582mm S-1,5M;Surface mounted luminaires;19.3110.0010.24;572 x 48 x 70;surface mounted on slings;14.4;1748;121;4000;4000;0.6678;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;572;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0010.24/;19.3110.0010.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
X-LINE SLIM UP&DOWN LED 2600/2600 PC/MICRO-PRM E 24 840 LINE-EL / L-1142mm S-1,5M;Surface mounted luminaires;19.3110.0013.24;1132 x 48 x 70;surface mounted on slings;34;4083;120;4000;4000;0.7188;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1132;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0013.24/;19.3110.0013.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
X-LINE SLIM UP&DOWN LED 2600/2600 PC/MICRO-PRM EDD 24 840 LINE-1EL / L-1142mm S-1,5M;Surface mounted luminaires;19.3110.0016.24;1132 x 48 x 70;surface mounted on slings;34;4083;120;4000;4000;0.7188;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1132;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0016.24/;19.3110.0016.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
X-LINE SLIM UP&DOWN LED 2600/2600 PC/PLX E 24 840 LINE-EL / L-1142mm S-1,5M;Surface mounted luminaires;19.3110.0019.24;1132 x 48 x 70;surface mounted on slings;34;3793;112;4000;4000;0.6678;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1132;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0019.24/;19.3110.0019.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
X-LINE SLIM UP&DOWN LED 2600/2600 PC/PLX EDD 24 840 LINE-1EL / L-1142mm S-1,5M;Surface mounted luminaires;19.3110.0022.24;1132 x 48 x 70;surface mounted on slings;34;3793;112;4000;4000;0.6678;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1132;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0022.24/;19.3110.0022.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
X-LINE SLIM UP&DOWN LED 3900/3900 PC/MICRO-PRM E 24 840 LINE-EL / L-1702mm S-1,5M;Surface mounted luminaires;19.3110.0025.24;1692 x 48 x 70;surface mounted on slings;52;6124;118;4000;4000;0.7188;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1692;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0025.24/;19.3110.0025.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
X-LINE SLIM UP&DOWN LED 3900/3900 PC/MICRO-PRM EDD 24 840 LINE-1EL / L-1702mm S-1,5M;Surface mounted luminaires;19.3110.0028.24;1692 x 48 x 70;surface mounted on slings;52;6124;118;4000;4000;0.7188;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1692;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0028.24/;19.3110.0028.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
X-LINE SLIM UP&DOWN LED 3900/3900 PC/PLX E 24 840 LINE-EL / L-1702mm S-1,5M;Surface mounted luminaires;19.3110.0031.24;1692 x 48 x 70;surface mounted on slings;52;5690;109;4000;4000;0.6678;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1692;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0031.24/;19.3110.0031.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
X-LINE SLIM UP&DOWN LED 3900/3900 PC/PLX EDD 24 840 LINE-1EL / L-1702mm S-1,5M;Surface mounted luminaires;19.3110.0034.24;1692 x 48 x 70;surface mounted on slings;52;5690;109;4000;4000;0.6678;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1692;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0034.24/;19.3110.0034.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
X-LINE SLIM UP&DOWN LED 5200/5200 PC/MICRO-PRM E 24 840 LINE-EL / L-2252mm S-1,5M;Surface mounted luminaires;19.3110.0037.24;2252 x 48 x 70;surface mounted on slings;68;8166;120;4000;4000;0.7188;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;2252;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0037.24/;19.3110.0037.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
X-LINE SLIM UP&DOWN LED 5200/5200 PC/MICRO-PRM EDD 24 840 LINE-1EL / L-2252mm S-1,5M;Surface mounted luminaires;19.3110.0040.24;2252 x 48 x 70;surface mounted on slings;68;8166;120;4000;4000;0.7188;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;2252;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0040.24/;19.3110.0040.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
X-LINE SLIM UP&DOWN LED 5200/5200 PC/PLX E 24 840 LINE-EL / L-2252mm S-1,5M;Surface mounted luminaires;19.3110.0043.24;2252 x 48 x 70;surface mounted on slings;68;7586;112;4000;4000;0.6678;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;2252;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0043.24/;19.3110.0043.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
X-LINE SLIM UP&DOWN LED 5200/5200 PC/PLX EDD 24 840 LINE-1EL / L-2252mm S-1,5M;Surface mounted luminaires;19.3110.0046.24;2252 x 48 x 70;surface mounted on slings;68;7586;112;4000;4000;0.6678;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;2252;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0046.24/;19.3110.0046.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
X-LINE SLIM UP&DOWN LED 1300/1300 PC/MICRO-PRM E 24 840 LINE-EP / L-582mm S-1,5M;Surface mounted luminaires;19.3110.0002.24;572 x 48 x 70;surface mounted on slings;14.4;1881;131;4000;4000;0.7188;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;572;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0002.24/;19.3110.0002.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
X-LINE SLIM UP&DOWN LED 1300/1300 PC/MICRO-PRM EDD 24 840 LINE-1EP / L-582mm S-1,5M;Surface mounted luminaires;19.3110.0005.24;572 x 48 x 70;surface mounted on slings;14.4;1881;131;4000;4000;0.7188;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;572;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0005.24/;19.3110.0005.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
X-LINE SLIM UP&DOWN LED 1300/1300 PC/PLX E 24 840 LINE-EP / L-582mm S-1,5M;Surface mounted luminaires;19.3110.0008.24;572 x 48 x 70;surface mounted on slings;14.4;1748;121;4000;4000;0.6678;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;572;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0008.24/;19.3110.0008.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
X-LINE SLIM UP&DOWN LED 1300/1300 PC/PLX EDD 24 840 LINE-1EP / L-582mm S-1,5M;Surface mounted luminaires;19.3110.0011.24;572 x 48 x 70;surface mounted on slings;14.4;1748;121;4000;4000;0.6678;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;572;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0011.24/;19.3110.0011.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
X-LINE SLIM UP&DOWN LED 2600/2600 PC/MICRO-PRM E 24 840 LINE-EP / L-1142mm S-1,5M;Surface mounted luminaires;19.3110.0014.24;1132 x 48 x 70;surface mounted on slings;34;4083;120;4000;4000;0.7188;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1132;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0014.24/;19.3110.0014.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
X-LINE SLIM UP&DOWN LED 2600/2600 PC/MICRO-PRM EDD 24 840 LINE-1EP / L-1142mm S-1,5M;Surface mounted luminaires;19.3110.0017.24;1132 x 48 x 70;surface mounted on slings;34;4083;120;4000;4000;0.7188;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1132;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0017.24/;19.3110.0017.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
X-LINE SLIM UP&DOWN LED 2600/2600 PC/PLX E 24 840 LINE-EP / L-1142mm S-1,5M;Surface mounted luminaires;19.3110.0020.24;1132 x 48 x 70;surface mounted on slings;34;3793;112;4000;4000;0.6678;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1132;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0020.24/;19.3110.0020.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
X-LINE SLIM UP&DOWN LED 2600/2600 PC/PLX EDD 24 840 LINE-1EP / L-1142mm S-1,5M;Surface mounted luminaires;19.3110.0023.24;1132 x 48 x 70;surface mounted on slings;34;3793;112;4000;4000;0.6678;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1132;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0023.24/;19.3110.0023.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
X-LINE SLIM UP&DOWN LED 3900/3900 PC/MICRO-PRM E 24 840 LINE-EP / L-1702mm S-1,5M;Surface mounted luminaires;19.3110.0026.24;1692 x 48 x 70;surface mounted on slings;52;6124;118;4000;4000;0.7188;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1692;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0026.24/;19.3110.0026.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
X-LINE SLIM UP&DOWN LED 3900/3900 PC/MICRO-PRM EDD 24 840 LINE-1EP / L-1702mm S-1,5M;Surface mounted luminaires;19.3110.0029.24;1692 x 48 x 70;surface mounted on slings;52;6124;118;4000;4000;0.7188;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;1692;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0029.24/;19.3110.0029.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
X-LINE SLIM UP&DOWN LED 3900/3900 PC/PLX E 24 840 LINE-EP / L-1702mm S-1,5M;Surface mounted luminaires;19.3110.0032.24;1692 x 48 x 70;surface mounted on slings;52;5690;109;4000;4000;0.6678;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1692;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0032.24/;19.3110.0032.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
X-LINE SLIM UP&DOWN LED 3900/3900 PC/PLX EDD 24 840 LINE-1EP / L-1702mm S-1,5M;Surface mounted luminaires;19.3110.0035.24;1692 x 48 x 70;surface mounted on slings;52;5690;109;4000;4000;0.6678;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;1692;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0035.24/;19.3110.0035.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
X-LINE SLIM UP&DOWN LED 5200/5200 PC/MICRO-PRM E 24 840 LINE-EP / L-2252mm S-1,5M;Surface mounted luminaires;19.3110.0038.24;2252 x 48 x 70;surface mounted on slings;68;8166;120;4000;4000;0.7188;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;2252;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0038.24/;19.3110.0038.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
X-LINE SLIM UP&DOWN LED 5200/5200 PC/MICRO-PRM EDD 24 840 LINE-1EP / L-2252mm S-1,5M;Surface mounted luminaires;19.3110.0041.24;2252 x 48 x 70;surface mounted on slings;68;8166;120;4000;4000;0.7188;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,95;2252;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0041.24/;19.3110.0041.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
X-LINE SLIM UP&DOWN LED 5200/5200 PC/PLX E 24 840 LINE-EP / L-2252mm S-1,5M;Surface mounted luminaires;19.3110.0044.24;2252 x 48 x 70;surface mounted on slings;68;7586;112;4000;4000;0.6678;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;2252;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0044.24/;19.3110.0044.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
X-LINE SLIM UP&DOWN LED 5200/5200 PC/PLX EDD 24 840 LINE-1EP / L-2252mm S-1,5M;Surface mounted luminaires;19.3110.0047.24;2252 x 48 x 70;surface mounted on slings;68;7586;112;4000;4000;0.6678;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC/PLX;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 96,4° / 90,2°;IP40;IK04;I;-;0,95;2252;48;70;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-line-slim-updown-led-line/19.3110.0047.24/;19.3110.0047.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
