;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
X-WALL K9 LED 1300 PLX E IP44 24 830 / L-575MM;Surface mounted luminaires;19.3117.0001.24;574 x 50 x 60;mounted on wall;9;881;98;3000;3000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;574;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0001.24/;19.3117.0001.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 1300 PLX E IP44 24 840 / L-575MM;Surface mounted luminaires;19.3117.0002.24;574 x 50 x 60;mounted on wall;9;927;103;4000;4000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;574;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0002.24/;19.3117.0002.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 1300 PLX EDD IP44 24 830 / L-575MM;Surface mounted luminaires;19.3117.0003.24;574 x 50 x 60;mounted on wall;9;881;98;3000;3000;0.653;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;574;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0003.24/;19.3117.0003.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 1300 PLX EDD IP44 24 840 / L-575MM;Surface mounted luminaires;19.3117.0004.24;574 x 50 x 60;mounted on wall;9;927;103;4000;4000;0.653;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;574;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0004.24/;19.3117.0004.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 1950 PLX E IP44 24 830 / L-855MM;Surface mounted luminaires;19.3117.0005.24;855 x 50 x 60;mounted on wall;11.1;1237;111;3000;3000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;855;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0005.24/;19.3117.0005.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 1950 PLX E IP44 24 840 / L-855MM;Surface mounted luminaires;19.3117.0006.24;855 x 50 x 60;mounted on wall;11.1;1282;116;4000;4000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;855;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0006.24/;19.3117.0006.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 2200 PLX E IP44 24 830 / L-575MM;Surface mounted luminaires;19.3117.0007.24;574 x 50 x 60;mounted on wall;12.6;1439;114;3000;3000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;574;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0007.24/;19.3117.0007.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 2200 PLX E IP44 24 840 / L-575MM;Surface mounted luminaires;19.3117.0008.24;574 x 50 x 60;mounted on wall;12.6;1491;118;4000;4000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;574;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0008.24/;19.3117.0008.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 2200 PLX EDD IP44 24 830 / L-575MM;Surface mounted luminaires;19.3117.0009.24;574 x 50 x 60;mounted on wall;12.6;1439;114;3000;3000;0.653;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;574;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0009.24/;19.3117.0009.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 2200 PLX EDD IP44 24 840 / L-575MM;Surface mounted luminaires;19.3117.0010.24;574 x 50 x 60;mounted on wall;12.6;1491;118;4000;4000;0.653;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;574;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0010.24/;19.3117.0010.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 2600 PLX E IP44 24 830 / L-1135MM;Surface mounted luminaires;19.3117.0011.24;1134 x 50 x 60;mounted on wall;14.4;1649;115;3000;3000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;1134;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0011.24/;19.3117.0011.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 2600 PLX E IP44 24 840 / L-1135MM;Surface mounted luminaires;19.3117.0012.24;1134 x 50 x 60;mounted on wall;14.4;1709;119;4000;4000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;1134;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0012.24/;19.3117.0012.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 2600 PLX EDD IP44 24 840 / L-1135MM;Surface mounted luminaires;19.3117.0013.24;1134 x 50 x 60;mounted on wall;14.4;1709;119;4000;4000;0.653;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;1134;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0013.24/;19.3117.0013.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 3250 PLX E IP44 24 830 / L-1415MM;Surface mounted luminaires;19.3117.0014.24;1415 x 50 x 60;mounted on wall;18.3;2062;113;3000;3000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;1415;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0014.24/;19.3117.0014.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 3250 PLX E IP44 24 840 / L-1415MM;Surface mounted luminaires;19.3117.0015.24;1415 x 50 x 60;mounted on wall;18.3;2137;117;4000;4000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;1415;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0015.24/;19.3117.0015.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 3900 PLX E IP44 24 830 / L-1695MM;Surface mounted luminaires;19.3117.0016.24;1694 x 50 x 60;mounted on wall;21.7;2474;114;3000;3000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;1694;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0016.24/;19.3117.0016.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 3900 PLX E IP44 24 840 / L-1695MM;Surface mounted luminaires;19.3117.0017.24;1694 x 50 x 60;mounted on wall;21.7;2564;118;4000;4000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;1694;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0017.24/;19.3117.0017.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 3900 PLX EDD IP44 24 840 / L-1695MM;Surface mounted luminaires;19.3117.0018.24;1694 x 50 x 60;mounted on wall;21.7;2564;118;4000;4000;0.653;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;1694;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0018.24/;19.3117.0018.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 4400 PLX E IP44 24 830 / L-1135MM;Surface mounted luminaires;19.3117.0019.24;1134 x 50 x 60;mounted on wall;24.7;2877;116;3000;3000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;1134;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0019.24/;19.3117.0019.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 4400 PLX E IP44 24 840 / L-1135MM;Surface mounted luminaires;19.3117.0020.24;1134 x 50 x 60;mounted on wall;24.7;2981;121;4000;4000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;1134;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0020.24/;19.3117.0020.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 4400 PLX EDD IP44 24 830 / L-1135MM;Surface mounted luminaires;19.3117.0021.24;1134 x 50 x 60;mounted on wall;24.7;2877;116;3000;3000;0.653;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;1134;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0021.24/;19.3117.0021.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 5200 PLX E IP44 24 830 / L-2255MM;Surface mounted luminaires;19.3117.0022.24;2255 x 50 x 60;mounted on wall;28.2;3298;117;3000;3000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;2255;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0022.24/;19.3117.0022.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 5200 PLX E IP44 24 840 / L-2255MM;Surface mounted luminaires;19.3117.0023.24;2255 x 50 x 60;mounted on wall;28.2;3418;121;4000;4000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;2255;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0023.24/;19.3117.0023.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 5500 PLX E IP44 24 830 / L-1415MM;Surface mounted luminaires;19.3117.0024.24;1415 x 50 x 60;mounted on wall;30.5;3608;118;3000;3000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;1415;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0024.24/;19.3117.0024.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 5500 PLX E IP44 24 840 / L-1415MM;Surface mounted luminaires;19.3117.0025.24;1415 x 50 x 60;mounted on wall;30.5;3740;123;4000;4000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;1415;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0025.24/;19.3117.0025.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 6500 PLX E IP44 24 830 / L-2821MM;Surface mounted luminaires;19.3117.0026.24;2821 x 50 x 60;mounted on wall;34.8;4123;118;3000;3000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;2821;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0026.24/;19.3117.0026.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 6500 PLX E IP44 24 840 / L-2821MM;Surface mounted luminaires;19.3117.0027.24;2821 x 50 x 60;mounted on wall;34.8;4273;123;4000;4000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;2821;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0027.24/;19.3117.0027.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 6600 PLX E IP44 24 830 / L-1695MM;Surface mounted luminaires;19.3117.0028.24;1694 x 50 x 60;mounted on wall;35.3;4315;122;3000;3000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;1694;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0028.24/;19.3117.0028.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 6600 PLX E IP44 24 840 / L-1695MM;Surface mounted luminaires;19.3117.0029.24;1694 x 50 x 60;mounted on wall;35.3;4472;127;4000;4000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;1694;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0029.24/;19.3117.0029.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 6600 PLX EDD IP44 24 830 / L-1695MM;Surface mounted luminaires;19.3117.0030.24;1694 x 50 x 60;mounted on wall;35.3;4315;122;3000;3000;0.653;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;1694;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0030.24/;19.3117.0030.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 6600 PLX EDD IP44 24 840 / L-1695MM;Surface mounted luminaires;19.3117.0031.24;1694 x 50 x 60;mounted on wall;35.3;4472;127;4000;4000;0.653;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;1694;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0031.24/;19.3117.0031.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 8800 PLX E IP44 24 830 / L-2255MM;Surface mounted luminaires;19.3117.0032.24;2255 x 50 x 60;mounted on wall;49.1;5754;117;3000;3000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;2255;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0032.24/;19.3117.0032.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 8800 PLX E IP44 24 840 / L-2255MM;Surface mounted luminaires;19.3117.0033.24;2255 x 50 x 60;mounted on wall;49.1;5962;121;4000;4000;0.653;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;2255;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0033.24/;19.3117.0033.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL K9 LED 8800 PLX EDD IP44 24 830 / L-2255MM;Surface mounted luminaires;19.3117.0034.24;2255 x 50 x 60;mounted on wall;49.1;5754;117;3000;3000;0.653;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;asymmetric light distribution - Imax=-47°;IP44;IK04;I;-;0,95;2255;50;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-k9-led/19.3117.0034.24/;19.3117.0034.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
