;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
X-WALL R LED 1300 PC OPAL E IP44 24 830 / L-580MM;Surface mounted luminaires;19.3214.0001.24;580 x 56 x 60;mounted on wall;9;994;110;3000;3000;0.7366;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;580;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0001.24/;19.3214.0001.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL R LED 1300 PC OPAL E IP44 24 840 / L-580MM;Surface mounted luminaires;19.3214.0002.24;580 x 56 x 60;mounted on wall;9;1046;116;4000;4000;0.7366;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;580;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0002.24/;19.3214.0002.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL R LED 1950 PC OPAL E IP44 24 830 / L-862MM;Surface mounted luminaires;19.3214.0006.24;862 x 56 x 60;mounted on wall;11.1;1396;126;3000;3000;0.7366;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;862;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0006.24/;19.3214.0006.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL R LED 1950 PC OPAL E IP44 24 840 / L-862MM;Surface mounted luminaires;19.3214.0007.24;862 x 56 x 60;mounted on wall;11.1;1447;130;4000;4000;0.7366;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;862;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0007.24/;19.3214.0007.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL R LED 2200 PC OPAL E IP44 24 830 / L-580MM;Surface mounted luminaires;19.3214.0003.24;580 x 56 x 60;mounted on wall;12.6;1623;129;3000;3000;0.7366;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;580;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0003.24/;19.3214.0003.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL R LED 2200 PC OPAL E IP44 24 840 / L-580MM;Surface mounted luminaires;19.3214.0004.24;580 x 56 x 60;mounted on wall;12.6;1682;133;4000;4000;0.7366;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;580;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0004.24/;19.3214.0004.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL R LED 2200 PC OPAL EDD IP44 24 827-865 / L-580mm TUNABLE WHITE;Surface mounted luminaires;19.3214.0005.24;580 x 56 x 60;mounted on wall;16;1676;105;4000;2700 ÷ 6500;0.7366;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;50000;L80/B10;>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;580;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0005.24/;19.3214.0005.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL R LED 2600 PC OPAL E IP44 24 830 / L-1140MM;Surface mounted luminaires;19.3214.0011.24;1140 x 56 x 60;mounted on wall;14.4;1860;129;3000;3000;0.7366;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;1140;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0011.24/;19.3214.0011.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL R LED 2600 PC OPAL E IP44 24 840 / L-1140MM;Surface mounted luminaires;19.3214.0012.24;1140 x 56 x 60;mounted on wall;14.4;1928;134;4000;4000;0.7366;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;1140;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0012.24/;19.3214.0012.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL R LED 3250 PC OPAL E IP44 24 830 / L-1424MM;Surface mounted luminaires;19.3214.0016.24;1424 x 56 x 60;mounted on wall;18.3;2326;127;3000;3000;0.7366;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;1424;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0016.24/;19.3214.0016.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL R LED 3250 PC OPAL E IP44 24 840 / L-1424MM;Surface mounted luminaires;19.3214.0017.24;1424 x 56 x 60;mounted on wall;18.3;2411;132;4000;4000;0.7366;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;1424;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0017.24/;19.3214.0017.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL R LED 3300 PC OPAL E IP44 24 830 / L-862MM;Surface mounted luminaires;19.3214.0008.24;862 x 56 x 60;mounted on wall;19.2;2443;127;3000;3000;0.7366;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;862;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0008.24/;19.3214.0008.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL R LED 3300 PC OPAL E IP44 24 840 / L-862MM;Surface mounted luminaires;19.3214.0009.24;862 x 56 x 60;mounted on wall;19.2;2531;132;4000;4000;0.7366;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;862;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0009.24/;19.3214.0009.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL R LED 3300 PC OPAL EDD IP44 24 827-865 / L-862mm TUNABLE WHITE;Surface mounted luminaires;19.3214.0010.24;862 x 56 x 60;mounted on wall;19.2;2653;138;4000;2700 ÷ 6500;0.7366;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;50000;L80/B10;>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;862;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0010.24/;19.3214.0010.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL R LED 4400 PC OPAL E IP44 24 830 / L-1140MM;Surface mounted luminaires;19.3214.0013.24;1140 x 56 x 60;mounted on wall;24.7;3245;131;3000;3000;0.7366;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;1140;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0013.24/;19.3214.0013.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL R LED 4400 PC OPAL E IP44 24 840 / L-1140MM;Surface mounted luminaires;19.3214.0014.24;1140 x 56 x 60;mounted on wall;24.7;3363;136;4000;4000;0.7366;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;1140;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0014.24/;19.3214.0014.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL R LED 4400 PC OPAL EDD IP44 24 827-865 / L-1140mm TUNABLE WHITE;Surface mounted luminaires;19.3214.0015.24;1140 x 56 x 60;mounted on wall;32;3369;105;4000;2700 ÷ 6500;0.7366;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;50000;L80/B10;>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;1140;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0015.24/;19.3214.0015.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL R LED 5500 PC OPAL E IP44 24 830 / L-1424MM;Surface mounted luminaires;19.3214.0018.24;1424 x 56 x 60;mounted on wall;30.5;4070;133;3000;3000;0.7366;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;1424;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0018.24/;19.3214.0018.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL R LED 5500 PC OPAL E IP44 24 840 / L-1424MM;Surface mounted luminaires;19.3214.0019.24;1424 x 56 x 60;mounted on wall;30.5;4219;138;4000;4000;0.7366;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;1424;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0019.24/;19.3214.0019.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-WALL R LED 5500 PC OPAL EDD IP44 24 827-865 / L-1424mm TUNABLE WHITE;Surface mounted luminaires;19.3214.0020.24;1424 x 56 x 60;mounted on wall;30.5;4422;145;4000;2700 ÷ 6500;0.7366;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PC (opalescent polycarbonate);LED;5 ÷ 30;50000;L80/B10;>80;3;asymmetric light distribution - Imax=-49,5°;IP44;IK04;I;-;0,95;1424;56;60;0;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/;https://luxiona.pl/en/oferta/oprawy-nastropowe/x-wall-r-led/19.3214.0020.24/;19.3214.0020.24_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
