;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
ARTSHAPE OVAL LED SMALL FULL SUSPENDED 3000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3002.1006.34;630 x 250 x 85;surface mounted on slings;28;2184;78;4000;4000;0.7354;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP40;IK04;I;RG0;0,95;630;250;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-oval-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-oval-led/19.3002.1006.34/;19.3002.1006.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE OVAL LED MEDIUM FULL SUSPENDED 4500 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3002.2004.34;900 x 250 x 85;surface mounted on slings;35;3273;94;4000;4000;0.7354;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP40;IK04;I;RG0;0,95;900;250;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-oval-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-oval-led/19.3002.2004.34/;19.3002.2004.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE OVAL LED MEDIUM FULL SUSPENDED 9000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3002.2001.34;900 x 250 x 85;surface mounted on slings;70;6552;94;4000;4000;0.7354;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP40;IK04;I;RG0;0,95;900;250;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-oval-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-oval-led/19.3002.2001.34/;19.3002.2001.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE OVAL LED LARGE FULL SUSPENDED 6000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3002.3002.34;1170 x 250 x 85;surface mounted on slings;50;4368;87;4000;4000;0.7354;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP40;IK04;I;RG0;0,95;1170;250;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-oval-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-oval-led/19.3002.3002.34/;19.3002.3002.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE OVAL LED SMALL UP&DOWN 2200/6000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3002.1009.34;630 x 250 x 85;surface mounted on slings;70;6392;91;4000;4000;0.7776;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;35000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP40;IK04;I;RG0;0,95;630;250;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-oval-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-oval-led/19.3002.1009.34/;19.3002.1009.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE OVAL LED MEDIUM UP&DOWN 3000/9000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3002.2007.34;900 x 250 x 85;surface mounted on slings;96;9252;96;4000;4000;0.7742;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;35000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP40;IK04;I;RG0;0,95;900;250;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-oval-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-oval-led/19.3002.2007.34/;19.3002.2007.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE OVAL LED LARGE UP&DOWN 4000/12000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3002.3005.34;1170 x 250 x 85;surface mounted on slings;128;12244;96;4000;4000;0.7734;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;35000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP40;IK04;I;RG0;0,95;1170;250;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-oval-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-oval-led/19.3002.3005.34/;19.3002.3005.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
