;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
ARTSHAPE ROUND LED SMALL FULL SUSPENDED 4000 PLX E 34 830 / S-1,5M;Architectural luminaires;19.3003.1050.34;?650 x 85;surface mounted on slings;35.0;3148;90;3000;3000;0.7354;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP20;IK04;I;RG0;0,95;0;0;85;650;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.1050.34/;19.3003.1050.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED SMALL FULL SUSPENDED 4000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3003.1049.34;?650 x 85;surface mounted on slings;35.0;3277;94;4000;4000;0.7354;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP20;IK04;I;RG0;0,95;0;0;85;650;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.1049.34/;19.3003.1049.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED SMALL FULL SUSPENDED 6000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3003.1056.34;?650 x 85;surface mounted on slings;47.0;4377;93;4000;4000;0.7354;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP20;IK04;I;RG0;0,95;0;0;85;650;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.1056.34/;19.3003.1056.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED SMALL FULL SUSPENDED 6000 PLX EDD 34 840 / S-1,5M;Architectural luminaires;19.3003.1058.34;?650 x 85;surface mounted on slings;47.0;4377;93;4000;4000;0.7354;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP20;IK04;I;RG0;0,95;0;0;85;650;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.1058.34/;19.3003.1058.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED SMALL FULL SUSPENDED 9000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3003.1064.34;?650 x 85;surface mounted on slings;74.0;6917;93;4000;4000;0.7354;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP20;IK04;I;RG0;0,95;0;0;85;650;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.1064.34/;19.3003.1064.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED SMALL FULL SUSPENDED 9000 PLX EDD 34 840 / S-1,5M;Architectural luminaires;19.3003.1066.34;?650 x 85;surface mounted on slings;74.0;6917;93;4000;4000;0.7354;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP20;IK04;I;RG0;0,95;0;0;85;650;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.1066.34/;19.3003.1066.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED MEDIUM FULL SUSPENDED 14000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3003.2050.34;?900 x 85;surface mounted on slings;115.0;10557;92;4000;4000;0.7354;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP20;IK04;I;RG0;0,95;0;0;85;900;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.2050.34/;19.3003.2050.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED MEDIUM FULL SUSPENDED 14000 PLX EDD 34 830 / S-1,5M;Architectural luminaires;19.3003.2053.34;?900 x 85;surface mounted on slings;115.0;10097;88;3000;3000;0.7354;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP20;IK04;I;RG0;0,95;0;0;85;900;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.2053.34/;19.3003.2053.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED LARGE FULL SUSPENDED 24000 PLX EDD 34 830 / S-1,5M;Architectural luminaires;19.3003.3055.34;?1200 x 85;surface mounted on slings;195.0;17475;90;3000;3000;0.7354;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP20;IK04;I;RG0;0,95;0;0;85;1200;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.3055.34/;19.3003.3055.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED SMALL FULL UP&DOWN 3000/6000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3003.1090.34;?650 x 85;surface mounted on slings;73.0;7074;97;4000;4000;0.7867;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;35000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP20;IK04;I;0;0,95;0;0;85;650;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.1090.34/;19.3003.1090.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED MEDIUM FULL UP&DOWN 4000/14000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3003.2073.34;?900 x 85;surface mounted on slings;150.0;14333;96;4000;4000;0.7701;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;35000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP20;IK04;I;0;0,95;0;0;85;900;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.2073.34/;19.3003.2073.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED LARGE FULL UP&DOWN 5500/24000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3003.3065.34;?1200 x 85;surface mounted on slings;245.0;23194;95;4000;4000;0.7635;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;35000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 111,2° / 114,2°;IP20;IK04;I;0;0,95;0;0;85;1200;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.3065.34/;19.3003.3065.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
