;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
ARTSHAPE ROUND LED SMALL EDGE SUSPENDED 3000 PLX E 34 830 / S-1,5M;Architectural luminaires;19.3003.1005.34;?650 x 85;surface mounted on slings;25;1492;60;3000;3000;0.5244;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;0;0;85;650;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.1005.34/;19.3003.1005.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED SMALL EDGE SUSPENDED 3000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3003.1001.34;?650 x 85;surface mounted on slings;25;1557;62;4000;4000;0.5244;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;0;0;85;650;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.1001.34/;19.3003.1001.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED SMALL EDGE SUSPENDED 3000 PLX EDD 34 830 / S-1,5M;Architectural luminaires;19.3003.1013.34;?650 x 85;surface mounted on slings;25;1492;60;3000;3000;0.5244;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;0;0;85;650;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.1013.34/;19.3003.1013.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED SMALL EDGE SUSPENDED 6000 PLX E 34 830 / S-1,5M;Architectural luminaires;19.3003.1004.34;?650 x 85;surface mounted on slings;50;2979;60;3000;3000;0.5244;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;0;0;85;650;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.1004.34/;19.3003.1004.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED SMALL EDGE SUSPENDED 6000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3003.1003.34;?650 x 85;surface mounted on slings;50;3115;62;4000;4000;0.5244;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;0;0;85;650;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.1003.34/;19.3003.1003.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED MEDIUM EDGE SUSPENDED 4500 PLX E 34 830 / S-1,5M;Architectural luminaires;19.3003.2006.34;?900 x 85;surface mounted on slings;35;2235;64;3000;3000;0.5244;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;0;0;85;900;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.2006.34/;19.3003.2006.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED MEDIUM EDGE SUSPENDED 4500 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3003.2007.34;?900 x 85;surface mounted on slings;35;2336;67;4000;4000;0.5244;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;0;0;85;900;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.2007.34/;19.3003.2007.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED MEDIUM EDGE SUSPENDED 4500 PLX EDD 34 840 / S-1,5M;Architectural luminaires;19.3003.2010.34;?900 x 85;surface mounted on slings;35;2336;67;4000;4000;0.5244;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;0;0;85;900;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.2010.34/;19.3003.2010.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED MEDIUM EDGE SUSPENDED 9000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3003.2015.34;?900 x 85;surface mounted on slings;70;4672;67;4000;4000;0.5244;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;0;0;85;900;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.2015.34/;19.3003.2015.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED MEDIUM EDGE SUSPENDED 9000 PLX EDD 34 830 / S-1,5M;Architectural luminaires;19.3003.2022.34;?900 x 85;surface mounted on slings;70;4468;64;3000;3000;0.5244;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;0;0;85;900;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.2022.34/;19.3003.2022.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED MEDIUM EDGE SUSPENDED 9000 PLX EDD 34 840 / S-1,5M;Architectural luminaires;19.3003.2021.34;?900 x 85;surface mounted on slings;70;4672;67;4000;4000;0.5244;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;0;0;85;900;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.2021.34/;19.3003.2021.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED LARGE EDGE SUSPENDED 6000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3003.3024.34;?1200 x 85;surface mounted on slings;50;3115;62;4000;4000;0.5244;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;0;0;85;1200;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.3024.34/;19.3003.3024.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED LARGE EDGE SUSPENDED 6000 PLX EDD 34 840 / S-1,5M;Architectural luminaires;19.3003.3028.34;?1200 x 85;surface mounted on slings;50;3115;62;4000;4000;0.5244;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;0;0;85;1200;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.3028.34/;19.3003.3028.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED LARGE EDGE SUSPENDED 12000 PLX E 34 830 / S-1,5M;Architectural luminaires;19.3003.3001.34;?1200 x 85;surface mounted on slings;93;5956;64;3000;3000;0.5244;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;0;0;85;1200;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.3001.34/;19.3003.3001.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED LARGE EDGE SUSPENDED 12000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3003.3002.34;?1200 x 85;surface mounted on slings;93;6230;67;4000;4000;0.5244;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;0;0;85;1200;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.3002.34/;19.3003.3002.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED LARGE EDGE SUSPENDED 12000 PLX EDD 34 840 / S-1,5M;Architectural luminaires;19.3003.3008.34;?1200 x 85;surface mounted on slings;93;6230;67;4000;4000;0.5244;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;0;0;85;1200;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.3008.34/;19.3003.3008.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED SMALL EDGE SUSPENDED TW 4000 PLX EDD 34 827-865 / S-1,5M;Architectural luminaires;19.3003.1023.34;?650 x 85;surface mounted on slings;42;2265;54;4000;2700 ÷ 6500;0.5244;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK05;I;-;0,95;0;0;85;650;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.1023.34/;19.3003.1023.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED MEDIUM EDGE SUSPENDED TW 6000 PLX EDD 34 827-865 / S-1,5M;Architectural luminaires;19.3003.2029.34;?900 x 85;surface mounted on slings;59;3209;54;4000;2700 ÷ 6500;0.5244;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK06;I;-;0,95;0;0;85;900;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.2029.34/;19.3003.2029.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED LARGE EDGE SUSPENDED TW 8000 PLX EDD 34 827-865 / S-1,5M;Architectural luminaires;19.3003.3066.34;?1200 x 85;surface mounted on slings;82;4468;54;4000;2700 ÷ 6500;0.5244;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK07;I;-;0,95;0;0;85;1200;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.3066.34/;19.3003.3066.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED SMALL EDGE UP&DOWN 3000/6000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3003.1040.34;?650 x 85;surface mounted on slings;76;5813;76;4000;4000;0.6473;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;35000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;-;0,95;0;0;85;650;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.1040.34/;19.3003.1040.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED MEDIUM EDGE UP&DOWN 4200/9000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3003.2041.34;?900 x 85;surface mounted on slings;106;8449;80;4000;4000;0.6417;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;35000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;-;0,95;0;0;85;900;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.2041.34/;19.3003.2041.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE ROUND LED LARGE EDGE UP&DOWN 5500/12000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3003.3048.34;?1200 x 85;surface mounted on slings;140;11220;80;4000;4000;0.641;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;35000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;-;0,95;0;0;85;1200;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-round-led/19.3003.3048.34/;19.3003.3048.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
