;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
ARTSHAPE SIX LED SMALL EDGE SUSPENDED 3000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3004.1001.34;650 x 592 x 85;surface mounted on slings;25;1557;62;4000;4000;0.5244;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;650;592;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.1001.34/;19.3004.1001.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE SIX LED SMALL EDGE SUSPENDED 6000 PLX E 34 830 / S-1,5M;Architectural luminaires;19.3004.1007.34;650 x 592 x 85;surface mounted on slings;50;2979;60;3000;3000;0.5244;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;650;592;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.1007.34/;19.3004.1007.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE SIX LED SMALL EDGE SUSPENDED 9000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3004.1009.34;650 x 592 x 85;surface mounted on slings;70;4672;67;4000;4000;0.5244;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;650;592;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.1009.34/;19.3004.1009.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE SIX LED MEDIUM EDGE SUSPENDED 4500 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3004.2002.34;900 x 809 x 85;surface mounted on slings;35;2336;67;4000;4000;0.5244;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;900;809;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.2002.34/;19.3004.2002.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE SIX LED MEDIUM EDGE SUSPENDED 4500 PLX EDD 34 840 / S-1,5M;Architectural luminaires;19.3004.2004.34;900 x 809 x 85;surface mounted on slings;35;2336;67;4000;4000;0.5244;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;900;809;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.2004.34/;19.3004.2004.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE SIX LED MEDIUM EDGE SUSPENDED 9000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3004.2007.34;900 x 809 x 85;surface mounted on slings;70;4672;67;4000;4000;0.5244;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;900;809;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.2007.34/;19.3004.2007.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE SIX LED MEDIUM EDGE SUSPENDED 9000 PLX EDD 34 840 / S-1,5M;Architectural luminaires;19.3004.2008.34;900 x 809 x 85;surface mounted on slings;70;4672;67;4000;4000;0.5244;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;900;809;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.2008.34/;19.3004.2008.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE SIX LED LARGE EDGE SUSPENDED 6000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3004.3005.34;1170 x 1043 x 85;surface mounted on slings;50;3115;62;4000;4000;0.5244;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;1170;1043;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.3005.34/;19.3004.3005.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE SIX LED LARGE EDGE SUSPENDED 6000 PLX EDD 34 840 / S-1,5M;Architectural luminaires;19.3004.3006.34;1170 x 1043 x 85;surface mounted on slings;50;3115;62;4000;4000;0.5244;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;1170;1043;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.3006.34/;19.3004.3006.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE SIX LED LARGE EDGE SUSPENDED 12000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3004.3001.34;1170 x 1043 x 85;surface mounted on slings;92;6230;68;4000;4000;0.5244;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;1170;1043;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.3001.34/;19.3004.3001.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE SIX LED LARGE EDGE SUSPENDED 12000 PLX EDD 34 840 / S-1,5M;Architectural luminaires;19.3004.3004.34;1170 x 1043 x 85;surface mounted on slings;92;6230;68;4000;4000;0.5244;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;RG0;0,95;1170;1043;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.3004.34/;19.3004.3004.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE SIX LED SMALL EDGE SUSPENDED TW 4000 PLX EDD 34 827-865 / S-1,5M;Architectural luminaires;19.3004.1010.34;650 x 592 x 85;surface mounted on slings;40;2202;55;4000;2700 ÷ 6500;0.5244;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;-;0,95;650;592;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.1010.34/;19.3004.1010.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE SIX LED MEDIUM EDGE SUSPENDED TW 6000 PLX EDD 34 827-865 / S-1,5M;Architectural luminaires;19.3004.2009.34;900 x 809 x 85;surface mounted on slings;57;3083;54;4000;2700 ÷ 6500;0.5244;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;-;0,95;900;809;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.2009.34/;19.3004.2009.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE SIX LED LARGE EDGE SUSPENDED TW 8000 PLX EDD 34 827-865 / S-1,5M;Architectural luminaires;19.3004.3008.34;1170 x 1043 x 85;surface mounted on slings;77;4216;55;4000;2700 ÷ 6500;0.5244;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;60000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;-;0,95;1170;1043;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.3008.34/;19.3004.3008.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE SIX LED SMALL EDGE UP&DOWN 2800/6000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3004.1015.34;650 x 592 x 85;surface mounted on slings;75;5678;76;4000;4000;0.6432;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;35000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;-;0,95;650;592;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.1015.34/;19.3004.1015.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE SIX LED MEDIUM EDGE UP&DOWN 4000/9000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3004.2014.34;900 x 809 x 85;surface mounted on slings;105;8313;79;4000;4000;0.6388;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;35000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;-;0,95;900;809;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.2014.34/;19.3004.2014.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
ARTSHAPE SIX LED LARGE EDGE UP&DOWN 5200/12000 PLX E 34 840 / S-1,5M;Architectural luminaires;19.3004.3012.34;1170 x 1043 x 85;surface mounted on slings;138;10951;79;4000;4000;0.6367;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;0 ÷ 30;35000;L80/B10;>80;0;(C0-C180) / (C90-C270) - 113,4° / 111,8°;IP40;IK04;I;-;0,95;1170;1043;85;0;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/;https://luxiona.pl/en/oferta/oprawy-architektoniczne/artshape-six-led/19.3004.3012.34/;19.3004.3012.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
