;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
LOTOS ELEGANCE SQUARE PC LED COMPACT V2 1200 E IP54 840;Compact;19.3209.0024.34;220 x 220 x 54;surface mounted on ceiling or on wall;12.5;1408;113;4000;4000;0.6407;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_white;LUXIONA_PC (opalescent polycarbonate);LED;0;30000;L70/B10;>80;0;(C0-C180) / (C90-C270) - 108° / 113,2°;IP54;IK08;II;0;0;220;220;54;https://luxiona.pl/oferta/compact/lotos-elegance-square-pc-led-compact-v2/;https://luxiona.pl/oferta/compact/lotos-elegance-square-pc-led-compact-v2/19.3209.0024.34/;19.3209.0024.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LOTOS ELEGANCE SQUARE PC LED COMPACT V2 1200 E CMW IP54 840;Compact;19.3209.0026.34;220 x 220 x 54;surface mounted on ceiling or on wall;12.5;1408;113;4000;4000;0.6407;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_white;LUXIONA_PC (opalescent polycarbonate);LED;0;30000;L70/B10;>80;0;(C0-C180) / (C90-C270) - 108° / 113,2°;IP54;IK08;II;0;0;220;220;54;https://luxiona.pl/oferta/compact/lotos-elegance-square-pc-led-compact-v2/;https://luxiona.pl/oferta/compact/lotos-elegance-square-pc-led-compact-v2/19.3209.0026.34/;19.3209.0026.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LOTOS ELEGANCE SQUARE PC LED COMPACT V2 1800 E IP54 840;Compact;19.3209.0006.34;280 x 280 x 54;surface mounted on ceiling or on wall;17.3;1868;108;4000;4000;0.6407;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_white;LUXIONA_PC (opalescent polycarbonate);LED;0;30000;L70/B10;>80;0;(C0-C180) / (C90-C270) - 108° / 113,2°;IP54;IK08;II;0;0;280;280;54;https://luxiona.pl/oferta/compact/lotos-elegance-square-pc-led-compact-v2/;https://luxiona.pl/oferta/compact/lotos-elegance-square-pc-led-compact-v2/19.3209.0006.34/;19.3209.0006.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LOTOS ELEGANCE SQUARE PC LED COMPACT V2 1800 E CMW IP54 840;Compact;19.3209.0014.34;280 x 280 x 54;surface mounted on ceiling or on wall;17.3;1868;108;4000;4000;0.6407;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_white;LUXIONA_PC (opalescent polycarbonate);LED;0;30000;L70/B10;>80;0;(C0-C180) / (C90-C270) - 108° / 113,2°;IP54;IK08;II;0;0;280;280;54;https://luxiona.pl/oferta/compact/lotos-elegance-square-pc-led-compact-v2/;https://luxiona.pl/oferta/compact/lotos-elegance-square-pc-led-compact-v2/19.3209.0014.34/;19.3209.0014.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LOTOS ELEGANCE SQUARE PC LED COMPACT V2 2400 E IP54 840;Compact;19.3209.0008.34;280 x 280 x 54;surface mounted on ceiling or on wall;23.1;2470;107;4000;4000;0.6407;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_white;LUXIONA_PC (opalescent polycarbonate);LED;0;30000;L70/B10;>80;0;(C0-C180) / (C90-C270) - 108° / 113,2°;IP54;IK08;II;0;0;280;280;54;https://luxiona.pl/oferta/compact/lotos-elegance-square-pc-led-compact-v2/;https://luxiona.pl/oferta/compact/lotos-elegance-square-pc-led-compact-v2/19.3209.0008.34/;19.3209.0008.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
LOTOS ELEGANCE SQUARE PC LED COMPACT V2 2400 E CMW IP54 840;Compact;19.3209.0016.34;280 x 280 x 54;surface mounted on ceiling or on wall;23.1;2470;107;4000;4000;0.6407;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_white;LUXIONA_PC (opalescent polycarbonate);LED;0;30000;L70/B10;>80;0;(C0-C180) / (C90-C270) - 108° / 113,2°;IP54;IK08;II;0;0;280;280;54;https://luxiona.pl/oferta/compact/lotos-elegance-square-pc-led-compact-v2/;https://luxiona.pl/oferta/compact/lotos-elegance-square-pc-led-compact-v2/19.3209.0016.34/;19.3209.0016.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
