;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
NEPTUN LED COMPACT V2 1300 PC-FROZEN E 21 IP66 830 / L-600;Compact;19.3207.0009.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;10.7;1515;142;3000;3000;0.9162;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0009.21/;19.3207.0009.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 1300 PC-FROZEN E 21 IP66 830 / L-600 ZASILANIE PRZELOTOWE 16A;Compact;19.3207.0021.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;11.0;1515;138;3000;3000;0.9162;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0021.21/;19.3207.0021.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 1300 PC-FROZEN E 21 IP66 840 / L-600;Compact;19.3207.0010.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;10.7;1722;161;4000;4000;0.9162;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0010.21/;19.3207.0010.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 1300 PC-FROZEN E 21 IP66 840 / L-600 ZASILANIE PRZELOTOWE 16A;Compact;19.3207.0022.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;11.0;1722;157;4000;4000;0.9162;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0022.21/;19.3207.0022.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 1300 PC-FROZEN EDD 21 IP66 830 / L-600;Compact;19.3207.0011.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;10.7;1515;142;3000;3000;0.9162;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0011.21/;19.3207.0011.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 1300 PC-FROZEN EDD 21 IP66 830 / L-600 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3207.0023.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;11.0;1515;138;3000;3000;0.9162;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0023.21/;19.3207.0023.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 1300 PC-FROZEN EDD 21 IP66 840 / L-600;Compact;19.3207.0012.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;10.7;1722;161;4000;4000;0.9162;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0012.21/;19.3207.0012.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 1300 PC-FROZEN EDD 21 IP66 840 / L-600 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3207.0024.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;11.0;1722;157;4000;4000;0.9162;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0024.21/;19.3207.0024.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 2600 PC-FROZEN E 21 IP66 830 / L-1200;Compact;19.3205.0001.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;17.3;2554;148;3000;3000;0.9169;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0001.21/;19.3205.0001.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 2600 PC-FROZEN E 21 IP66 830 / L-1200 ZASILANIE PRZELOTOWE 16A;Compact;19.3205.0017.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;17.0;2554;150;3000;3000;0.9169;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0017.21/;19.3205.0017.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 2600 PC-FROZEN E 21 IP66 830 / L-600;Compact;19.3207.0001.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;16.3;2272;139;3000;3000;0.9162;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0001.21/;19.3207.0001.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 2600 PC-FROZEN E 21 IP66 830 / L-600 ZASILANIE PRZELOTOWE 16A;Compact;19.3207.0013.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;16.0;2272;142;3000;3000;0.9162;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0013.21/;19.3207.0013.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 2600 PC-FROZEN E 21 IP66 840 / L-1200;Compact;19.3205.0002.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;17.3;2673;154;4000;4000;0.9169;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0002.21/;19.3205.0002.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 2600 PC-FROZEN E 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 16A;Compact;19.3205.0018.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;17.0;2673;157;4000;4000;0.9169;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0018.21/;19.3205.0018.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 2600 PC-FROZEN E 21 IP66 840 / L-600;Compact;19.3207.0002.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;16.3;2548;156;4000;4000;0.9162;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0002.21/;19.3207.0002.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 2600 PC-FROZEN E 21 IP66 840 / L-600 ZASILANIE PRZELOTOWE 16A;Compact;19.3207.0014.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;16.0;2548;159;4000;4000;0.9162;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0014.21/;19.3207.0014.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 2600 PC-FROZEN EDD 21 IP66 830 / L-1200;Compact;19.3205.0003.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;17.3;2554;148;3000;3000;0.9169;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0003.21/;19.3205.0003.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 2600 PC-FROZEN EDD 21 IP66 830 / L-1200 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3205.0019.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;17.0;2554;150;3000;3000;0.9169;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0019.21/;19.3205.0019.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 2600 PC-FROZEN EDD 21 IP66 830 / L-600;Compact;19.3207.0003.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;16.3;2272;139;3000;3000;0.9162;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0003.21/;19.3207.0003.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 2600 PC-FROZEN EDD 21 IP66 830 / L-600 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3207.0015.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;16.0;2272;142;3000;3000;0.9162;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0015.21/;19.3207.0015.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 2600 PC-FROZEN EDD 21 IP66 840 / L-1200;Compact;19.3205.0004.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;17.3;2673;154;4000;4000;0.9169;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0004.21/;19.3205.0004.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 2600 PC-FROZEN EDD 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3205.0020.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;17.0;2673;157;4000;4000;0.9169;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0020.21/;19.3205.0020.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 2600 PC-FROZEN EDD 21 IP66 840 / L-600;Compact;19.3207.0004.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;16.3;2548;156;4000;4000;0.9162;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0004.21/;19.3207.0004.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 2600 PC-FROZEN EDD 21 IP66 840 / L-600 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3207.0016.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;16.0;2548;159;4000;4000;0.9162;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0016.21/;19.3207.0016.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 2600 PC-FROZEN EDD 21 IP66 840 / L-600 ZASILANIE PRZELOTOWE 24A 5X, M20 DO PRZEW.FI 11,5 ;Compact;19.3207.0025.21;620 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;16.0;2548;159;4000;4000;0.9162;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123,6° / 116°;IP66;IK10;I;0;0,95;620;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0025.21/;19.3207.0025.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 4000 PC-FROZEN E 21 IP66 830 / L-1200;Compact;19.3205.0005.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;25.4;3717;146;3000;3000;0.9169;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0005.21/;19.3205.0005.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 4000 PC-FROZEN E 21 IP66 830 / L-1200 ZASILANIE PRZELOTOWE 16A;Compact;19.3205.0021.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;25.0;3717;149;3000;3000;0.9169;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0021.21/;19.3205.0021.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 4000 PC-FROZEN E 21 IP66 830 / L-600;Compact;19.3207.0005.21;620 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;25.4;3727;147;3000;3000;0.8902;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123° / 107,2°;IP66;IK10;I;0;0,95;620;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0005.21/;19.3207.0005.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 4000 PC-FROZEN E 21 IP66 830 / L-600 ZASILANIE PRZELOTOWE 16A;Compact;19.3207.0017.21;620 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;25.0;3727;149;3000;3000;0.8902;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123° / 107,2°;IP66;IK10;I;0;0,95;620;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0017.21/;19.3207.0017.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 4000 PC-FROZEN E 21 IP66 840 / L-1200;Compact;19.3205.0006.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;25.4;4223;166;4000;4000;0.9169;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0006.21/;19.3205.0006.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 4000 PC-FROZEN E 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 16A;Compact;19.3205.0022.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;25.0;4223;169;4000;4000;0.9169;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0022.21/;19.3205.0022.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 4000 PC-FROZEN E 21 IP66 840 / L-600;Compact;19.3207.0006.21;620 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;25.4;4304;169;4000;4000;0.8902;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123° / 107,2°;IP66;IK10;I;0;0,95;620;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0006.21/;19.3207.0006.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 4000 PC-FROZEN E 21 IP66 840 / L-600 ZASILANIE PRZELOTOWE 16A;Compact;19.3207.0018.21;620 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;25.0;4304;172;4000;4000;0.8902;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123° / 107,2°;IP66;IK10;I;0;0,95;620;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0018.21/;19.3207.0018.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 4000 PC-FROZEN EDD 21 IP66 830 / L-1200;Compact;19.3205.0007.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;25.4;3717;146;3000;3000;0.9169;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0007.21/;19.3205.0007.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 4000 PC-FROZEN EDD 21 IP66 830 / L-1200 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3205.0023.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;25.0;3717;149;3000;3000;0.9169;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0023.21/;19.3205.0023.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 4000 PC-FROZEN EDD 21 IP66 830 / L-600;Compact;19.3207.0007.21;620 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;25.4;3727;147;3000;3000;0.8902;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123° / 107,2°;IP66;IK10;I;0;0,95;620;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0007.21/;19.3207.0007.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 4000 PC-FROZEN EDD 21 IP66 830 / L-600 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3207.0019.21;620 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;25.0;3727;149;3000;3000;0.8902;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123° / 107,2°;IP66;IK10;I;0;0,95;620;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0019.21/;19.3207.0019.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 4000 PC-FROZEN EDD 21 IP66 840 / L-1200;Compact;19.3205.0008.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;25.4;4223;166;4000;4000;0.9169;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0008.21/;19.3205.0008.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 4000 PC-FROZEN EDD 21 IP66 840 / L-1200 ZASILANE PRZELOTOWE 16A 5X;Compact;19.3205.0024.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;25.0;4223;169;4000;4000;0.9169;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0024.21/;19.3205.0024.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 4000 PC-FROZEN EDD 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 24A 5X, M20 DO PRZEW.FI 11,5;Compact;19.3205.0035.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;25.0;4223;169;4000;4000;0.9169;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0035.21/;19.3205.0035.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 4000 PC-FROZEN EDD 21 IP66 840 / L-600;Compact;19.3207.0008.21;620 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;25.4;4304;169;4000;4000;0.8902;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123° / 107,2°;IP66;IK10;I;0;0,95;620;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0008.21/;19.3207.0008.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 4000 PC-FROZEN EDD 21 IP66 840 / L-600 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3207.0020.21;620 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;25.0;4304;172;4000;4000;0.8902;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 40;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 123° / 107,2°;IP66;IK10;I;0;0,95;620;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3207.0020.21/;19.3207.0020.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 5500 PC-FROZEN E 21 IP66 830 / L-1500;Compact;19.3203.0001.21;1520 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;33.2;4787;144;3000;3000;0.9418;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 116,4° / 102,2°;IP66;IK10;I;0;0,95;1520;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0001.21/;19.3203.0001.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 5500 PC-FROZEN E 21 IP66 830 / L-1500 ZASILANIE PRZELOTOWE 16A;Compact;19.3203.0013.21;1520 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;33.0;4787;145;3000;3000;0.9418;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 116,4° / 102,2°;IP66;IK10;I;0;0,95;1520;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0013.21/;19.3203.0013.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 5500 PC-FROZEN E 21 IP66 840 / L-1500;Compact;19.3203.0002.21;1520 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;33.2;5440;164;4000;4000;0.9418;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 116,4° / 102,2°;IP66;IK10;I;0;0,95;1520;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0002.21/;19.3203.0002.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 5500 PC-FROZEN E 21 IP66 840 / L-1500 ZASILANIE PRZELOTOWE 16A;Compact;19.3203.0014.21;1520 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;33.0;5440;165;4000;4000;0.9418;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 116,4° / 102,2°;IP66;IK10;I;0;0,95;1520;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0014.21/;19.3203.0014.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 5500 PC-FROZEN EDD 21 IP66 830 / L-1500;Compact;19.3203.0003.21;1520 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;33.2;4787;144;3000;3000;0.9418;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 116,4° / 102,2°;IP66;IK10;I;0;0,95;1520;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0003.21/;19.3203.0003.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 5500 PC-FROZEN EDD 21 IP66 830 / L-1500 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3203.0015.21;1520 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;33.0;4787;145;3000;3000;0.9418;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 116,4° / 102,2°;IP66;IK10;I;0;0,95;1520;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0015.21/;19.3203.0015.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 5500 PC-FROZEN EDD 21 IP66 840 / L-1500;Compact;19.3203.0004.21;1520 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;33.2;5440;164;4000;4000;0.9418;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 116,4° / 102,2°;IP66;IK10;I;0;0,95;1520;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0004.21/;19.3203.0004.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 5500 PC-FROZEN EDD 21 IP66 840 / L-1500 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3203.0016.21;1520 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;33.0;5440;165;4000;4000;0.9418;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 116,4° / 102,2°;IP66;IK10;I;0;0,95;1520;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0016.21/;19.3203.0016.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 6000 PC-FROZEN E 21 IP66 830 / L-1200;Compact;19.3205.0009.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;36.3;5059;139;3000;3000;0.9169;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0009.21/;19.3205.0009.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 6000 PC-FROZEN E 21 IP66 830 / L-1200 ZASILANIE PRZELOTOWE 16A;Compact;19.3205.0025.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;36.0;5059;141;3000;3000;0.9169;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0025.21/;19.3205.0025.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 6000 PC-FROZEN E 21 IP66 840 / L-1200;Compact;19.3205.0010.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;36.3;5750;158;4000;4000;0.9169;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0010.21/;19.3205.0010.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 6000 PC-FROZEN E 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 16A;Compact;19.3205.0026.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;36.0;5750;160;4000;4000;0.9169;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0026.21/;19.3205.0026.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 6000 PC-FROZEN EDD 21 IP66 830 / L-1200;Compact;19.3205.0011.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;36.3;5059;139;3000;3000;0.9169;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0011.21/;19.3205.0011.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 6000 PC-FROZEN EDD 21 IP66 830 / L-1200 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3205.0027.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;36.0;5059;141;3000;3000;0.9169;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0027.21/;19.3205.0027.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 6000 PC-FROZEN EDD 21 IP66 840 / L-1200;Compact;19.3205.0012.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;36.3;5750;158;4000;4000;0.9169;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0012.21/;19.3205.0012.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 6000 PC-FROZEN EDD 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3205.0028.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;36.0;5750;160;4000;4000;0.9169;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0028.21/;19.3205.0028.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 6000 PC-FROZEN EDD 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 24A 5X, M20 DO PRZEW.FI 11,5;Compact;19.3205.0036.21;1220 x 72 x 60;directly mounted to ceiling construction or surface mounted on slings;36.0;5750;160;4000;4000;0.9169;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,6° / 102,8°;IP66;IK10;I;0;0,95;1220;72;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0036.21/;19.3205.0036.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 7500 PC-FROZEN E 21 IP66 830 / L-1500;Compact;19.3203.0009.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;50.2;7804;155;3000;3000;0.9398;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0009.21/;19.3203.0009.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 7500 PC-FROZEN E 21 IP66 830 / L-1500 ZASILANIE PRZELOTOWE 16A;Compact;19.3203.0021.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;50.0;7804;156;3000;3000;0.9398;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0021.21/;19.3203.0021.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 7500 PC-FROZEN E 21 IP66 840 / L-1500;Compact;19.3203.0010.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;50.2;8868;177;4000;4000;0.9398;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0010.21/;19.3203.0010.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 7500 PC-FROZEN E 21 IP66 840 / L-1500 ZASILANIE PRZELOTOWE 16A;Compact;19.3203.0022.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;50.0;8868;177;4000;4000;0.9398;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0022.21/;19.3203.0022.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 7500 PC-FROZEN EDD 21 IP66 830 / L-1500;Compact;19.3203.0011.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;50.2;7804;155;3000;3000;0.9398;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0011.21/;19.3203.0011.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 7500 PC-FROZEN EDD 21 IP66 830 / L-1500 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3203.0023.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;50.0;7804;156;3000;3000;0.9398;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0023.21/;19.3203.0023.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 7500 PC-FROZEN EDD 21 IP66 840 / L-1500;Compact;19.3203.0012.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;50.2;8868;177;4000;4000;0.9398;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0012.21/;19.3203.0012.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 7500 PC-FROZEN EDD 21 IP66 840 / L-1500 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3203.0024.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;50.0;8868;177;4000;4000;0.9398;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0024.21/;19.3203.0024.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 8000 PC-FROZEN E 21 IP66 830 / L-1200;Compact;19.3205.0013.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;52.3;7538;144;3000;3000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0013.21/;19.3205.0013.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 8000 PC-FROZEN E 21 IP66 830 / L-1200 ZASILANIE PRZELOTOWE 16A;Compact;19.3205.0029.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;52.0;7538;145;3000;3000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0029.21/;19.3205.0029.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 8000 PC-FROZEN E 21 IP66 840 / L-1200;Compact;19.3205.0014.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;52.3;8566;164;4000;4000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0014.21/;19.3205.0014.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 8000 PC-FROZEN E 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 16A;Compact;19.3205.0030.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;52.0;8566;165;4000;4000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0030.21/;19.3205.0030.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 8000 PC-FROZEN EDD 21 IP66 830 / L-1200;Compact;19.3205.0015.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;52.3;7538;144;3000;3000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0015.21/;19.3205.0015.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 8000 PC-FROZEN EDD 21 IP66 830 / L-1200 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3205.0031.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;52.0;7538;145;3000;3000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0031.21/;19.3205.0031.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 8000 PC-FROZEN EDD 21 IP66 840 / L-1200;Compact;19.3205.0016.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;52.3;8566;164;4000;4000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0016.21/;19.3205.0016.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 8000 PC-FROZEN EDD 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3205.0032.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;52.0;8566;165;4000;4000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 35;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0032.21/;19.3205.0032.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 10000 PC-FROZEN E 21 IP66 830 / L-1200;Compact;19.3205.0040.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;64.0;8652;135;3000;3000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0040.21/;19.3205.0040.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 10000 PC-FROZEN E 21 IP66 830 / L-1200 ZASILANIE PRZELOTOWE 16A;Compact;19.3205.0044.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;64.0;8652;135;3000;3000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0044.21/;19.3205.0044.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 10000 PC-FROZEN E 21 IP66 840 / L-1200;Compact;19.3205.0039.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;64.0;9005;141;4000;4000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0039.21/;19.3205.0039.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 10000 PC-FROZEN E 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 16A;Compact;19.3205.0043.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;64.0;9005;141;4000;4000;0.9297;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0043.21/;19.3205.0043.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 10000 PC-FROZEN EDD 21 IP66 830 / L-1200;Compact;19.3205.0042.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;64.0;8652;135;3000;3000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0042.21/;19.3205.0042.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 10000 PC-FROZEN EDD 21 IP66 830 / L-1200 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3205.0046.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;64.0;8652;135;3000;3000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0046.21/;19.3205.0046.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 10000 PC-FROZEN EDD 21 IP66 840 / L-1200;Compact;19.3205.0041.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;64.0;9005;141;4000;4000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0041.21/;19.3205.0041.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 10000 PC-FROZEN EDD 21 IP66 840 / L-1200 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3205.0045.21;1220 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;64.0;9005;141;4000;4000;0.9297;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 119,4° / 104°;IP66;IK10;I;0;0,95;1220;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3205.0045.21/;19.3205.0045.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 11000 PC-FROZEN E 21 IP66 830 / L-1500;Compact;19.3203.0005.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;64.4;9555;148;3000;3000;0.9398;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0005.21/;19.3203.0005.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 11000 PC-FROZEN E 21 IP66 830 / L-1500 ZASILANIE PRZELOTOWE 16A;Compact;19.3203.0017.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;64.0;9555;149;3000;3000;0.9398;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0017.21/;19.3203.0017.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 11000 PC-FROZEN E 21 IP66 840 / L-1500;Compact;19.3203.0006.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;64.4;10858;169;4000;4000;0.9398;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0006.21/;19.3203.0006.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 11000 PC-FROZEN E 21 IP66 840 / L-1500 ZASILANIE PRZELOTOWE 16A;Compact;19.3203.0018.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;64.0;10858;170;4000;4000;0.9398;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0018.21/;19.3203.0018.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 11000 PC-FROZEN EDD 21 IP66 830 / L-1500;Compact;19.3203.0007.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;64.4;9555;148;3000;3000;0.9398;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0007.21/;19.3203.0007.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 11000 PC-FROZEN EDD 21 IP66 830 / L-1500 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3203.0019.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;64.0;9555;149;3000;3000;0.9398;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0019.21/;19.3203.0019.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 11000 PC-FROZEN EDD 21 IP66 840 / L-1500;Compact;19.3203.0008.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;64.4;10858;169;4000;4000;0.9398;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0008.21/;19.3203.0008.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
NEPTUN LED COMPACT V2 11000 PC-FROZEN EDD 21 IP66 840 / L-1500 ZASILANIE PRZELOTOWE 16A 5X;Compact;19.3203.0020.21;1520 x 92 x 60;directly mounted to ceiling construction or surface mounted on slings;64.0;10858;170;4000;4000;0.9398;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Polycarbonate;LUXIONA_RAL 9006 (grey);LUXIONA_PC-FROZEN;LED;-25 ÷ 30;70000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 120,2° / 106,2°;IP66;IK10;I;0;0,95;1520;92;60;0;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/;https://luxiona.pl/oferta/compact/neptun-led-compact-v2/19.3203.0020.21/;19.3203.0020.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA

