;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
PATOS-LINE LED 5200 MICRO-PRM E 830 LINE-S / CONNECTOR TYPE-X 600/600/600/600;Architectural luminaires;19.0034.0004.34;1126/1126 x 76 x 83;mounted in plasterboard ceilings;28.2;3804;135;3000;3000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;1126;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-x/19.0034.0004.34/;19.0034.0004.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 5200 MICRO-PRM E 840 LINE-S / CONNECTOR TYPE-X 600/600/600/600;Architectural luminaires;19.0034.0003.34;1126/1126 x 76 x 83;mounted in plasterboard ceilings;28.2;3942;140;4000;4000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;1126;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-x/19.0034.0003.34/;19.0034.0003.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 5200 PLX E 830 LINE-S / CONNECTOR TYPE-X 600/600/600/600;Architectural luminaires;19.0034.0002.34;1126/1126 x 76 x 83;mounted in plasterboard ceilings;28.2;3367;119;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1126;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-x/19.0034.0002.34/;19.0034.0002.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 5200 PLX E 840 LINE-S / CONNECTOR TYPE-X 600/600/600/600;Architectural luminaires;19.0034.0001.34;1126/1126 x 76 x 83;mounted in plasterboard ceilings;28.2;3489;124;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1126;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-x/19.0034.0001.34/;19.0034.0001.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 8800 MICRO-PRM E 830 LINE-S / CONNECTOR TYPE-X 600/600/600/600;Architectural luminaires;19.0034.0006.34;1126/1126 x 76 x 83;mounted in plasterboard ceilings;49.1;6636;135;3000;3000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;1126;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-x/19.0034.0006.34/;19.0034.0006.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 8800 MICRO-PRM E 840 LINE-S / CONNECTOR TYPE-X 600/600/600/600;Architectural luminaires;19.0034.0005.34;1126/1126 x 76 x 83;mounted in plasterboard ceilings;49.1;6877;140;4000;4000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;1126;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-x/19.0034.0005.34/;19.0034.0005.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 8800 PLX E 830 LINE-S / CONNECTOR TYPE-X 600/600/600/600;Architectural luminaires;19.0034.0008.34;1126/1126 x 76 x 83;mounted in plasterboard ceilings;49.1;5873;120;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1126;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-x/19.0034.0008.34/;19.0034.0008.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 8800 PLX E 840 LINE-S / CONNECTOR TYPE-X 600/600/600/600;Architectural luminaires;19.0034.0007.34;1126/1126 x 76 x 83;mounted in plasterboard ceilings;49.1;6086;124;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1126;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-x/19.0034.0007.34/;19.0034.0007.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
