;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
PATOS-LINE LED 1950 MICRO-PRM E 830 LINE-S / CONNECTOR TYPE-LC 600/300;Architectural luminaires;19.0032.0306.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1427;129;3000;3000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0306.34/;19.0032.0306.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 MICRO-PRM E 830 LINE-S / CONNECTOR TYPE-LD 600/300;Architectural luminaires;19.0032.0406.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1427;129;3000;3000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0406.34/;19.0032.0406.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 MICRO-PRM E 830 LINE-S / CONNECTOR TYPE-LE 600/300;Architectural luminaires;19.0032.0506.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1427;129;3000;3000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0506.34/;19.0032.0506.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 MICRO-PRM E 830 LINE-S / CONNECTOR TYPE-LF 600/300;Architectural luminaires;19.0032.0605.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1427;129;3000;3000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0605.34/;19.0032.0605.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 MICRO-PRM E 840 LINE-S / CONNECTOR TYPE-LC 600/300;Architectural luminaires;19.0032.0305.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1479;133;4000;4000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0305.34/;19.0032.0305.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 MICRO-PRM E 840 LINE-S / CONNECTOR TYPE-LD 600/300;Architectural luminaires;19.0032.0405.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1479;133;4000;4000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0405.34/;19.0032.0405.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 MICRO-PRM E 840 LINE-S / CONNECTOR TYPE-LE 600/300;Architectural luminaires;19.0032.0505.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1479;133;4000;4000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0505.34/;19.0032.0505.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 MICRO-PRM E 840 LINE-S / CONNECTOR TYPE-LF 600/300;Architectural luminaires;19.0032.0606.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1479;133;4000;4000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0606.34/;19.0032.0606.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 MICRO-PRM EDD 830 LINE-1S / CONNECTOR TYPE-LC 600/300;Architectural luminaires;19.0032.0308.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1427;129;3000;3000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0308.34/;19.0032.0308.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 MICRO-PRM EDD 830 LINE-1S / CONNECTOR TYPE-LD 600/300;Architectural luminaires;19.0032.0408.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1427;129;3000;3000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0408.34/;19.0032.0408.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 MICRO-PRM EDD 830 LINE-1S / CONNECTOR TYPE-LE 600/300;Architectural luminaires;19.0032.0508.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1427;129;3000;3000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0508.34/;19.0032.0508.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 MICRO-PRM EDD 830 LINE-1S / CONNECTOR TYPE-LF 600/300;Architectural luminaires;19.0032.0608.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1427;129;3000;3000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0608.34/;19.0032.0608.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 MICRO-PRM EDD 840 LINE-1S / CONNECTOR TYPE-LC 600/300;Architectural luminaires;19.0032.0307.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1479;133;4000;4000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0307.34/;19.0032.0307.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 MICRO-PRM EDD 840 LINE-1S / CONNECTOR TYPE-LD 600/300;Architectural luminaires;19.0032.0407.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1479;133;4000;4000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0407.34/;19.0032.0407.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 MICRO-PRM EDD 840 LINE-1S / CONNECTOR TYPE-LE 600/300;Architectural luminaires;19.0032.0507.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1479;133;4000;4000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0507.34/;19.0032.0507.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 MICRO-PRM EDD 840 LINE-1S / CONNECTOR TYPE-LF 600/300;Architectural luminaires;19.0032.0607.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1479;133;4000;4000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0607.34/;19.0032.0607.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 PLX E 830 LINE-S / CONNECTOR TYPE-LC 600/300;Architectural luminaires;19.0032.0302.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1263;114;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0302.34/;19.0032.0302.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 PLX E 830 LINE-S / CONNECTOR TYPE-LD 600/300;Architectural luminaires;19.0032.0402.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1263;114;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0402.34/;19.0032.0402.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 PLX E 830 LINE-S / CONNECTOR TYPE-LE 600/300;Architectural luminaires;19.0032.0502.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1263;114;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0502.34/;19.0032.0502.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 PLX E 830 LINE-S / CONNECTOR TYPE-LF 600/300;Architectural luminaires;19.0032.0602.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1263;114;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0602.34/;19.0032.0602.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 PLX E 840 LINE-S / CONNECTOR TYPE-LC 600/300;Architectural luminaires;19.0032.0301.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1309;118;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0301.34/;19.0032.0301.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 PLX E 840 LINE-S / CONNECTOR TYPE-LD 600/300;Architectural luminaires;19.0032.0401.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1309;118;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0401.34/;19.0032.0401.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 PLX E 840 LINE-S / CONNECTOR TYPE-LE 600/300;Architectural luminaires;19.0032.0501.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1309;118;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0501.34/;19.0032.0501.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 PLX E 840 LINE-S / CONNECTOR TYPE-LF 600/300;Architectural luminaires;19.0032.0601.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1309;118;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0601.34/;19.0032.0601.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 PLX EDD 830 LINE-1S / CONNECTOR TYPE-LC 600/300;Architectural luminaires;19.0032.0304.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1263;114;3000;3000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0304.34/;19.0032.0304.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 PLX EDD 830 LINE-1S / CONNECTOR TYPE-LD 600/300;Architectural luminaires;19.0032.0404.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1263;114;3000;3000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0404.34/;19.0032.0404.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 PLX EDD 830 LINE-1S / CONNECTOR TYPE-LE 600/300;Architectural luminaires;19.0032.0504.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1263;114;3000;3000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0504.34/;19.0032.0504.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 PLX EDD 830 LINE-1S / CONNECTOR TYPE-LF 600/300;Architectural luminaires;19.0032.0604.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1263;114;3000;3000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0604.34/;19.0032.0604.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 PLX EDD 840 LINE-1S / CONNECTOR TYPE-LC 600/300;Architectural luminaires;19.0032.0303.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1309;118;4000;4000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0303.34/;19.0032.0303.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 PLX EDD 840 LINE-1S / CONNECTOR TYPE-LD 600/300;Architectural luminaires;19.0032.0403.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1309;118;4000;4000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0403.34/;19.0032.0403.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 PLX EDD 840 LINE-1S / CONNECTOR TYPE-LE 600/300;Architectural luminaires;19.0032.0503.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1309;118;4000;4000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0503.34/;19.0032.0503.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1950 PLX EDD 840 LINE-1S / CONNECTOR TYPE-LF 600/300;Architectural luminaires;19.0032.0603.34;602/301 x 76 x 83;mounted in plasterboard ceilings;11.1;1309;118;4000;4000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0603.34/;19.0032.0603.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2600 MICRO-PRM E 830 LINE-S / CONNECTOR TYPE-LA 600/600;Architectural luminaires;19.0032.0106.34;602/602 x 76 x 83;mounted in plasterboard ceilings;14.4;1902;132;3000;3000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0106.34/;19.0032.0106.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2600 MICRO-PRM E 830 LINE-S / CONNECTOR TYPE-LB 600/600;Architectural luminaires;19.0032.0206.34;602/602 x 76 x 83;mounted in plasterboard ceilings;14.4;1902;132;3000;3000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0206.34/;19.0032.0206.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2600 MICRO-PRM E 840 LINE-S / CONNECTOR TYPE-LA 600/600;Architectural luminaires;19.0032.0105.34;602/602 x 76 x 83;mounted in plasterboard ceilings;14.4;1971;137;4000;4000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0105.34/;19.0032.0105.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2600 MICRO-PRM E 840 LINE-S / CONNECTOR TYPE-LB 600/600;Architectural luminaires;19.0032.0205.34;602/602 x 76 x 83;mounted in plasterboard ceilings;14.4;1971;137;4000;4000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0205.34/;19.0032.0205.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2600 MICRO-PRM EDD 830 LINE-1S / CONNECTOR TYPE-LA 600/600;Architectural luminaires;19.0032.0104.34;602/602 x 76 x 83;mounted in plasterboard ceilings;14.4;1902;132;3000;3000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0104.34/;19.0032.0104.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2600 MICRO-PRM EDD 830 LINE-1S / CONNECTOR TYPE-LB 600/600;Architectural luminaires;19.0032.0204.34;602/602 x 76 x 83;mounted in plasterboard ceilings;14.4;1902;132;3000;3000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0204.34/;19.0032.0204.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2600 MICRO-PRM EDD 840 LINE-1S / CONNECTOR TYPE-LA 600/600;Architectural luminaires;19.0032.0103.34;602/602 x 76 x 83;mounted in plasterboard ceilings;14.4;1971;137;4000;4000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0103.34/;19.0032.0103.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2600 MICRO-PRM EDD 840 LINE-1S / CONNECTOR TYPE-LB 600/600;Architectural luminaires;19.0032.0203.34;602/602 x 76 x 83;mounted in plasterboard ceilings;14.4;1971;137;4000;4000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0203.34/;19.0032.0203.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2600 PLX E 830 LINE-S / CONNECTOR TYPE-LA 600/600;Architectural luminaires;19.0032.0102.34;602/602 x 76 x 83;mounted in plasterboard ceilings;14.4;1683;117;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0102.34/;19.0032.0102.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2600 PLX E 830 LINE-S / CONNECTOR TYPE-LB 600/600;Architectural luminaires;19.0032.0202.34;602/602 x 76 x 83;mounted in plasterboard ceilings;14.4;1683;117;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0202.34/;19.0032.0202.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2600 PLX E 840 LINE-S / CONNECTOR TYPE-LB 600/600;Architectural luminaires;19.0032.0201.34;602/602 x 76 x 83;mounted in plasterboard ceilings;14.4;1744;121;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0201.34/;19.0032.0201.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2600 PLX EDD 830 LINE-1S / CONNECTOR TYPE-LA 600/600;Architectural luminaires;19.0032.0107.34;602/602 x 76 x 83;mounted in plasterboard ceilings;14.4;1683;117;3000;3000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0107.34/;19.0032.0107.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2600 PLX EDD 830 LINE-1S / CONNECTOR TYPE-LB 600/600;Architectural luminaires;19.0032.0207.34;602/602 x 76 x 83;mounted in plasterboard ceilings;14.4;1683;117;3000;3000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0207.34/;19.0032.0207.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2600 PLX EDD 840 LINE-1S / CONNECTOR TYPE-LA 600/600;Architectural luminaires;19.0032.0108.34;602/602 x 76 x 83;mounted in plasterboard ceilings;14.4;1744;121;4000;4000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0108.34/;19.0032.0108.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2600 PLX EDD 840 LINE-1S / CONNECTOR TYPE-LB 600/600;Architectural luminaires;19.0032.0209.34;602/602 x 76 x 83;mounted in plasterboard ceilings;14.4;1744;121;4000;4000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0209.34/;19.0032.0209.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 MICRO-PRM E 830 LINE-S / CONNECTOR TYPE-LC 600/300;Architectural luminaires;19.0032.0310.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2498;130;3000;3000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0310.34/;19.0032.0310.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 MICRO-PRM E 830 LINE-S / CONNECTOR TYPE-LD 600/300;Architectural luminaires;19.0032.0410.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2498;130;3000;3000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0410.34/;19.0032.0410.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 MICRO-PRM E 830 LINE-S / CONNECTOR TYPE-LE 600/300;Architectural luminaires;19.0032.0510.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2498;130;3000;3000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0510.34/;19.0032.0510.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 MICRO-PRM E 830 LINE-S / CONNECTOR TYPE-LF 600/300;Architectural luminaires;19.0032.0610.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2498;130;3000;3000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0610.34/;19.0032.0610.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 MICRO-PRM E 840 LINE-S / CONNECTOR TYPE-LC 600/300;Architectural luminaires;19.0032.0309.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2588;135;4000;4000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0309.34/;19.0032.0309.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 MICRO-PRM E 840 LINE-S / CONNECTOR TYPE-LD 600/300;Architectural luminaires;19.0032.0409.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2588;135;4000;4000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0409.34/;19.0032.0409.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 MICRO-PRM E 840 LINE-S / CONNECTOR TYPE-LE 600/300;Architectural luminaires;19.0032.0509.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2588;135;4000;4000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0509.34/;19.0032.0509.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 MICRO-PRM E 840 LINE-S / CONNECTOR TYPE-LF 600/300;Architectural luminaires;19.0032.0609.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2588;135;4000;4000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0609.34/;19.0032.0609.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 MICRO-PRM EDD 830 LINE-1S / CONNECTOR TYPE-LC 600/300;Architectural luminaires;19.0032.0312.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2498;130;3000;3000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0312.34/;19.0032.0312.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 MICRO-PRM EDD 830 LINE-1S / CONNECTOR TYPE-LD 600/300;Architectural luminaires;19.0032.0412.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2498;130;3000;3000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0412.34/;19.0032.0412.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 MICRO-PRM EDD 830 LINE-1S / CONNECTOR TYPE-LE 600/300;Architectural luminaires;19.0032.0512.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2498;130;3000;3000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0512.34/;19.0032.0512.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 MICRO-PRM EDD 830 LINE-1S / CONNECTOR TYPE-LF 600/300;Architectural luminaires;19.0032.0612.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2498;130;3000;3000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0612.34/;19.0032.0612.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 MICRO-PRM EDD 840 LINE-1S / CONNECTOR TYPE-LC 600/300;Architectural luminaires;19.0032.0311.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2588;135;4000;4000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0311.34/;19.0032.0311.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 MICRO-PRM EDD 840 LINE-1S / CONNECTOR TYPE-LD 600/300;Architectural luminaires;19.0032.0411.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2588;135;4000;4000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0411.34/;19.0032.0411.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 MICRO-PRM EDD 840 LINE-1S / CONNECTOR TYPE-LE 600/300;Architectural luminaires;19.0032.0511.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2588;135;4000;4000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0511.34/;19.0032.0511.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 MICRO-PRM EDD 840 LINE-1S / CONNECTOR TYPE-LF 600/300;Architectural luminaires;19.0032.0611.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2588;135;4000;4000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0611.34/;19.0032.0611.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 PLX E 830 LINE-S / CONNECTOR TYPE-LC 600/300;Architectural luminaires;19.0032.0314.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2210;115;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0314.34/;19.0032.0314.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 PLX E 830 LINE-S / CONNECTOR TYPE-LD 600/300;Architectural luminaires;19.0032.0414.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2210;115;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0414.34/;19.0032.0414.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 PLX E 830 LINE-S / CONNECTOR TYPE-LE 600/300;Architectural luminaires;19.0032.0514.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2210;115;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0514.34/;19.0032.0514.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 PLX E 830 LINE-S / CONNECTOR TYPE-LF 600/300;Architectural luminaires;19.0032.0614.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2210;115;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0614.34/;19.0032.0614.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 PLX E 840 LINE-S / CONNECTOR TYPE-LC 600/300;Architectural luminaires;19.0032.0313.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2290;119;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0313.34/;19.0032.0313.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 PLX E 840 LINE-S / CONNECTOR TYPE-LD 600/300;Architectural luminaires;19.0032.0413.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2290;119;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0413.34/;19.0032.0413.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 PLX E 840 LINE-S / CONNECTOR TYPE-LE 600/300;Architectural luminaires;19.0032.0513.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2290;119;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0513.34/;19.0032.0513.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 PLX E 840 LINE-S / CONNECTOR TYPE-LF 600/300;Architectural luminaires;19.0032.0613.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2290;119;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0613.34/;19.0032.0613.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 PLX EDD 830 LINE-1S / CONNECTOR TYPE-LC 600/300;Architectural luminaires;19.0032.0316.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2210;115;3000;3000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0316.34/;19.0032.0316.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 PLX EDD 830 LINE-1S / CONNECTOR TYPE-LD 600/300;Architectural luminaires;19.0032.0416.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2210;115;3000;3000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0416.34/;19.0032.0416.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 PLX EDD 830 LINE-1S / CONNECTOR TYPE-LE 600/300;Architectural luminaires;19.0032.0516.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2210;115;3000;3000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0516.34/;19.0032.0516.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 PLX EDD 830 LINE-1S / CONNECTOR TYPE-LF 600/300;Architectural luminaires;19.0032.0616.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2210;115;3000;3000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0616.34/;19.0032.0616.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 PLX EDD 840 LINE-1S / CONNECTOR TYPE-LC 600/300;Architectural luminaires;19.0032.0315.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2290;119;4000;4000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0315.34/;19.0032.0315.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 PLX EDD 840 LINE-1S / CONNECTOR TYPE-LD 600/300;Architectural luminaires;19.0032.0415.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2290;119;4000;4000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0415.34/;19.0032.0415.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 PLX EDD 840 LINE-1S / CONNECTOR TYPE-LE 600/300;Architectural luminaires;19.0032.0515.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2290;119;4000;4000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0515.34/;19.0032.0515.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3300 PLX EDD 840 LINE-1S / CONNECTOR TYPE-LF 600/300;Architectural luminaires;19.0032.0615.34;602/301 x 76 x 83;mounted in plasterboard ceilings;19.2;2290;119;4000;4000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;301;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0615.34/;19.0032.0615.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 4400 MICRO-PRM E 830 LINE-S / CONNECTOR TYPE-LA 600/600;Architectural luminaires;19.0032.0111.34;602/602 x 76 x 83;mounted in plasterboard ceilings;24.7;3319;134;3000;3000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0111.34/;19.0032.0111.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 4400 MICRO-PRM E 830 LINE-S / CONNECTOR TYPE-LB 600/600;Architectural luminaires;19.0032.0211.34;602/602 x 76 x 83;mounted in plasterboard ceilings;24.7;3319;134;3000;3000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0211.34/;19.0032.0211.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 4400 MICRO-PRM E 840 LINE-S / CONNECTOR TYPE-LA 600/600;Architectural luminaires;19.0032.0110.34;602/602 x 76 x 83;mounted in plasterboard ceilings;24.7;3438;139;4000;4000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0110.34/;19.0032.0110.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 4400 MICRO-PRM E 840 LINE-S / CONNECTOR TYPE-LB 600/600;Architectural luminaires;19.0032.0210.34;602/602 x 76 x 83;mounted in plasterboard ceilings;24.7;3438;139;4000;4000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0210.34/;19.0032.0210.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 4400 MICRO-PRM EDD 830 LINE-1S / CONNECTOR TYPE-LA 600/600;Architectural luminaires;19.0032.0113.34;602/602 x 76 x 83;mounted in plasterboard ceilings;24.7;3319;134;3000;3000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0113.34/;19.0032.0113.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 4400 MICRO-PRM EDD 830 LINE-1S / CONNECTOR TYPE-LB 600/600;Architectural luminaires;19.0032.0213.34;602/602 x 76 x 83;mounted in plasterboard ceilings;24.7;3319;134;3000;3000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0213.34/;19.0032.0213.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 4400 MICRO-PRM EDD 840 LINE-1S / CONNECTOR TYPE-LA 600/600;Architectural luminaires;19.0032.0112.34;602/602 x 76 x 83;mounted in plasterboard ceilings;24.7;3438;139;4000;4000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0112.34/;19.0032.0112.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 4400 MICRO-PRM EDD 840 LINE-1S / CONNECTOR TYPE-LB 600/600;Architectural luminaires;19.0032.0212.34;602/602 x 76 x 83;mounted in plasterboard ceilings;24.7;3438;139;4000;4000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0212.34/;19.0032.0212.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 4400 PLX E 830 LINE-S / CONNECTOR TYPE-LA 600/600;Architectural luminaires;19.0032.0115.34;602/602 x 76 x 83;mounted in plasterboard ceilings;24.7;2937;119;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0115.34/;19.0032.0115.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 4400 PLX E 830 LINE-S / CONNECTOR TYPE-LB 600/600;Architectural luminaires;19.0032.0215.34;602/602 x 76 x 83;mounted in plasterboard ceilings;24.7;2937;119;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0215.34/;19.0032.0215.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 4400 PLX E 840 LINE-S / CONNECTOR TYPE-LB 600/600;Architectural luminaires;19.0032.0214.34;602/602 x 76 x 83;mounted in plasterboard ceilings;24.7;3043;123;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0214.34/;19.0032.0214.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 4400 PLX EDD 830 LINE-1S / CONNECTOR TYPE-LA 600/600;Architectural luminaires;19.0032.0117.34;602/602 x 76 x 83;mounted in plasterboard ceilings;24.7;2937;119;3000;3000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0117.34/;19.0032.0117.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 4400 PLX EDD 830 LINE-1S / CONNECTOR TYPE-LB 600/600;Architectural luminaires;19.0032.0217.34;602/602 x 76 x 83;mounted in plasterboard ceilings;24.7;2937;119;3000;3000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0217.34/;19.0032.0217.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 4400 PLX EDD 840 LINE-1S / CONNECTOR TYPE-LA 600/600;Architectural luminaires;19.0032.0116.34;602/602 x 76 x 83;mounted in plasterboard ceilings;24.7;3043;123;4000;4000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0116.34/;19.0032.0116.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 4400 PLX EDD 840 LINE-1S / CONNECTOR TYPE-LB 600/600;Architectural luminaires;19.0032.0216.34;602/602 x 76 x 83;mounted in plasterboard ceilings;24.7;3043;123;4000;4000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;602;76;83;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-connector-l/19.0032.0216.34/;19.0032.0216.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
