;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
PATOS-LINE LED 1300 PLX E 830 LINE-EL / L-563,1 mm;Architectural luminaires;19.3031.0104.34;563 x 77 x 81;mounted in plasterboard ceilings;9;899;100;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,9;563;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0104.34/;19.3031.0104.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 1300 PLX E 840 LINE-EL / L-563,1 mm;Architectural luminaires;19.3031.0101.34;563 x 77 x 81;mounted in plasterboard ceilings;9;947;105;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,9;563;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0101.34/;19.3031.0101.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2200 PLX E 830 LINE-EL / L-563,1 mm;Architectural luminaires;19.3031.0112.34;563 x 77 x 81;mounted in plasterboard ceilings;12.6;1469;117;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,9;563;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0112.34/;19.3031.0112.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2200 PLX E 840 LINE-EL / L-563,1 mm;Architectural luminaires;19.3031.0115.34;563 x 77 x 81;mounted in plasterboard ceilings;12.6;1522;121;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,9;563;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0115.34/;19.3031.0115.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2600 PLX E 830 LINE-EL / L-1123,1MM;Architectural luminaires;19.3031.0304.34;1123 x 77 x 81;mounted in plasterboard ceilings;14.4;1683;117;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1123;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0304.34/;19.3031.0304.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 2600 PLX E 840 LINE-EL / L-1123,1 mm;Architectural luminaires;19.3031.0301.34;1123 x 77 x 81;mounted in plasterboard ceilings;14.4;1744;121;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1123;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0301.34/;19.3031.0301.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3250 PLX E 830 LINE-EL / L-1403,1 mm;Architectural luminaires;19.3031.0404.34;1403 x 77 x 81;mounted in plasterboard ceilings;18.3;2105;115;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1403;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0404.34/;19.3031.0404.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3250 PLX E 840 LINE-EL / L-1403,1 mm;Architectural luminaires;19.3031.0401.34;1403 x 77 x 81;mounted in plasterboard ceilings;18.3;2182;119;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1403;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0401.34/;19.3031.0401.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3900 PLX E 830 LINE-EL / L-1683,1MM;Architectural luminaires;19.3031.0504.34;1683 x 77 x 81;mounted in plasterboard ceilings;21.7;2525;116;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1683;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0504.34/;19.3031.0504.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 3900 PLX E 840 LINE-EL / L-1683,1 mm;Architectural luminaires;19.3031.0501.34;1683 x 77 x 81;mounted in plasterboard ceilings;21.7;2617;121;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1683;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0501.34/;19.3031.0501.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 4400 PLX E 830 LINE-EL / L-1123,1MM;Architectural luminaires;19.3031.0322.34;1123 x 77 x 81;mounted in plasterboard ceilings;24.7;2937;119;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1123;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0322.34/;19.3031.0322.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 4400 PLX E 840 LINE-EL / L-1123,1 mm;Architectural luminaires;19.3031.0325.34;1123 x 77 x 81;mounted in plasterboard ceilings;24.7;3043;123;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1123;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0325.34/;19.3031.0325.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 5500 PLX E 840 LINE-EL / L-1403,1MM;Architectural luminaires;19.3031.0427.34;1123 x 77 x 81;mounted in plasterboard ceilings;30.5;3818;125;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1123;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0427.34/;19.3031.0427.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 5500 PLX E 830 LINE-EL / L-1403,1 mm;Architectural luminaires;19.3031.0424.34;1403 x 77 x 81;mounted in plasterboard ceilings;30.5;3684;121;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1403;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0424.34/;19.3031.0424.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 6600 PLX E 830 LINE-EL / L-1683,1 mm;Architectural luminaires;19.3031.0513.34;1683 x 77 x 81;mounted in plasterboard ceilings;35.3;4405;125;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1683;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0513.34/;19.3031.0513.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
PATOS-LINE LED 6600 PLX E 840 LINE-EL / L-1683,1 mm;Architectural luminaires;19.3031.0510.34;1683 x 77 x 81;mounted in plasterboard ceilings;35.3;4565;129;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_white;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP20;IK04;I;0;0,95;1683;77;81;0;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/;https://luxiona.pl/oferta/oprawy-architektoniczne/patos-line-led-line/19.3031.0510.34/;19.3031.0510.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
