;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
RUBIN LOOK LED SMOOTH COMPACT 2500 MICRO-PRM E 21 830;Compact;19.3249.0001.21;365 x 365 x 50;surface mounted on ceiling;14.2;1799;127;3000;3000;0.8013;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9006 (gray, metallic, fine structure);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 95,2° / 94,6°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0001.21/;19.3249.0001.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 2500 MICRO-PRM E 21 840;Compact;19.3249.0002.21;365 x 365 x 50;surface mounted on ceiling;14.2;1905;134;4000;4000;0.8013;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9006 (gray, metallic, fine structure);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 95,2° / 94,6°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0002.21/;19.3249.0002.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 2500 MICRO-PRM E 34 830;Compact;19.3249.0001.34;365 x 365 x 50;surface mounted on ceiling;14.2;1799;127;3000;3000;0.8013;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 95,2° / 94,6°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0001.34/;19.3249.0001.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 2500 MICRO-PRM E 34 840;Compact;19.3249.0002.34;365 x 365 x 50;surface mounted on ceiling;14.2;1905;134;4000;4000;0.8013;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 95,2° / 94,6°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0002.34/;19.3249.0002.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 2500 PLX E 21 830;Compact;19.3249.0003.21;365 x 365 x 50;surface mounted on ceiling;14.2;1698;120;3000;3000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9006 (gray, metallic, fine structure);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0003.21/;19.3249.0003.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 2500 PLX E 21 840;Compact;19.3249.0004.21;365 x 365 x 50;surface mounted on ceiling;14.2;1798;127;4000;4000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9006 (gray, metallic, fine structure);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0004.21/;19.3249.0004.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 2500 PLX E 34 830;Compact;19.3249.0003.34;365 x 365 x 50;surface mounted on ceiling;14.2;1698;120;3000;3000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0003.34/;19.3249.0003.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 2500 PLX E 34 840;Compact;19.3249.0004.34;365 x 365 x 50;surface mounted on ceiling;14.2;1798;127;4000;4000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0004.34/;19.3249.0004.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 2500 PLX E PIR 21 830;Compact;19.3249.0005.21;365 x 365 x 50;surface mounted on ceiling;14.2;1698;120;3000;3000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9006 (gray, metallic, fine structure);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0005.21/;19.3249.0005.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 2500 PLX E PIR 21 840;Compact;19.3249.0006.21;365 x 365 x 50;surface mounted on ceiling;14.2;1798;127;4000;4000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9006 (gray, metallic, fine structure);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0006.21/;19.3249.0006.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 2500 PLX E PIR 34 830;Compact;19.3249.0005.34;365 x 365 x 50;surface mounted on ceiling;14.2;1698;120;3000;3000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0005.34/;19.3249.0005.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 2500 PLX E PIR 34 840;Compact;19.3249.0006.34;365 x 365 x 50;surface mounted on ceiling;14.2;1798;127;4000;4000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0006.34/;19.3249.0006.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 3000 MICRO-PRM E 21 830;Compact;19.3249.0007.21;365 x 365 x 50;surface mounted on ceiling;20.1;2559;127;3000;3000;0.8013;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9006 (gray, metallic, fine structure);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 95,2° / 94,6°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0007.21/;19.3249.0007.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 3000 MICRO-PRM E 21 840;Compact;19.3249.0008.21;365 x 365 x 50;surface mounted on ceiling;20.1;2709;135;4000;4000;0.8013;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9006 (gray, metallic, fine structure);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 95,2° / 94,6°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0008.21/;19.3249.0008.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 3000 MICRO-PRM E 34 830;Compact;19.3249.0007.34;365 x 365 x 50;surface mounted on ceiling;20.1;2559;127;3000;3000;0.8013;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 95,2° / 94,6°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0007.34/;19.3249.0007.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 3000 MICRO-PRM E 34 840;Compact;19.3249.0008.34;365 x 365 x 50;surface mounted on ceiling;20.1;2709;135;4000;4000;0.8013;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 95,2° / 94,6°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0008.34/;19.3249.0008.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 3000 PLX E 21 830;Compact;19.3249.0009.21;365 x 365 x 50;surface mounted on ceiling;20.1;2416;120;3000;3000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9006 (gray, metallic, fine structure);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0009.21/;19.3249.0009.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 3000 PLX E 21 840;Compact;19.3249.0010.21;365 x 365 x 50;surface mounted on ceiling;20.1;2558;127;4000;4000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9006 (gray, metallic, fine structure);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0010.21/;19.3249.0010.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 3000 PLX E 34 830;Compact;19.3249.0009.34;365 x 365 x 50;surface mounted on ceiling;20.1;2416;120;3000;3000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0009.34/;19.3249.0009.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 3000 PLX E 34 840;Compact;19.3249.0010.34;365 x 365 x 50;surface mounted on ceiling;20.1;2558;127;4000;4000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0010.34/;19.3249.0010.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 3000 PLX E PIR 21 830;Compact;19.3249.0011.21;365 x 365 x 50;surface mounted on ceiling;20.1;2416;120;3000;3000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9006 (gray, metallic, fine structure);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0011.21/;19.3249.0011.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 3000 PLX E PIR 21 840;Compact;19.3249.0012.21;365 x 365 x 50;surface mounted on ceiling;20.1;2558;127;4000;4000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9006 (gray, metallic, fine structure);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0012.21/;19.3249.0012.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 3000 PLX E PIR 34 830;Compact;19.3249.0011.34;365 x 365 x 50;surface mounted on ceiling;20.1;2416;120;3000;3000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0011.34/;19.3249.0011.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 3000 PLX E PIR 34 840;Compact;19.3249.0012.34;365 x 365 x 50;surface mounted on ceiling;20.1;2558;127;4000;4000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0012.34/;19.3249.0012.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 4000 MICRO-PRM E 21 830;Compact;19.3249.0013.21;365 x 365 x 50;surface mounted on ceiling;28.9;3552;123;3000;3000;0.8013;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9006 (gray, metallic, fine structure);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 95,2° / 94,6°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0013.21/;19.3249.0013.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 4000 MICRO-PRM E 21 840;Compact;19.3249.0014.21;365 x 365 x 50;surface mounted on ceiling;28.9;3762;130;4000;4000;0.8013;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9006 (gray, metallic, fine structure);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 95,2° / 94,6°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0014.21/;19.3249.0014.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 4000 MICRO-PRM E 34 830;Compact;19.3249.0013.34;365 x 365 x 50;surface mounted on ceiling;28.9;3552;123;3000;3000;0.8013;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 95,2° / 94,6°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0013.34/;19.3249.0013.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 4000 MICRO-PRM E 34 840;Compact;19.3249.0014.34;365 x 365 x 50;surface mounted on ceiling;28.9;3762;130;4000;4000;0.8013;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 95,2° / 94,6°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0014.34/;19.3249.0014.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 4000 PLX E 21 830;Compact;19.3249.0015.21;365 x 365 x 50;surface mounted on ceiling;28.9;3354;116;3000;3000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9006 (gray, metallic, fine structure);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0015.21/;19.3249.0015.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 4000 PLX E 21 840;Compact;19.3249.0016.21;365 x 365 x 50;surface mounted on ceiling;28.9;3552;123;4000;4000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9006 (gray, metallic, fine structure);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0016.21/;19.3249.0016.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 4000 PLX E 34 830;Compact;19.3249.0015.34;365 x 365 x 50;surface mounted on ceiling;28.9;3354;116;3000;3000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0015.34/;19.3249.0015.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 4000 PLX E 34 840;Compact;19.3249.0016.34;365 x 365 x 50;surface mounted on ceiling;28.9;3552;123;4000;4000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0016.34/;19.3249.0016.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 4000 PLX E PIR 21 830;Compact;19.3249.0017.21;365 x 365 x 50;surface mounted on ceiling;28.9;3354;116;3000;3000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9006 (gray, metallic, fine structure);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0017.21/;19.3249.0017.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 4000 PLX E PIR 21 840;Compact;19.3249.0018.21;365 x 365 x 50;surface mounted on ceiling;28.9;3552;123;4000;4000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9006 (gray, metallic, fine structure);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0018.21/;19.3249.0018.21.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 4000 PLX E PIR 34 830;Compact;19.3249.0017.34;365 x 365 x 50;surface mounted on ceiling;28.9;3354;116;3000;3000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0017.34/;19.3249.0017.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
RUBIN LOOK LED SMOOTH COMPACT 4000 PLX E PIR 34 840;Compact;19.3249.0018.34;365 x 365 x 50;surface mounted on ceiling;28.9;3552;123;4000;4000;0.7565;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Steel sheet;LUXIONA_RAL 9016 (white);LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 80000 (2);L70/B10 (1) / L80/B10 (2);>80;0;(C0-C180) / (C90-C270) - 111,6° / 112,4°;IP40;IK04;I;RG0;0,95;365;365;50;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/;https://luxiona.pl/oferta/compact/rubin-look-led-smooth-compact/19.3249.0018.34/;19.3249.0018.34.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
