;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
STREETPARK M LED PREMIUM HE 5000 STREET-M E IP66 22 757;Outdoor luminaires;19.3174.0001.22;718 x 311 x 103;mounted on poles;35;4026;115;5700;5700;0.7614;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9007 (dark gray);LUXIONA_hardened transparent glass;LED;-40 ÷ 40;60000;L70/B10;>70;0;Rozsył uliczny;IP66;IK09;I;0;0.95;718;311;103;https://luxiona.pl/oferta/oprawy-zewnetrzne/streetpark-m-led-premium/;https://luxiona.pl/oferta/oprawy-zewnetrzne/streetpark-m-led-premium/19.3174.0001.22/;19.3174.0001.22.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
STREETPARK M LED PREMIUM HE 5000 STREET-S E IP66 22 757;Outdoor luminaires;19.3174.0002.22;718 x 311 x 103;mounted on poles;35;4038;115;5700;5700;0.7638;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9007 (dark gray);LUXIONA_hardened transparent glass;LED;-40 ÷ 40;60000;L70/B10;>70;0;Rozsył uliczny;IP66;IK09;I;0;0.95;718;311;103;https://luxiona.pl/oferta/oprawy-zewnetrzne/streetpark-m-led-premium/;https://luxiona.pl/oferta/oprawy-zewnetrzne/streetpark-m-led-premium/19.3174.0002.22/;19.3174.0002.22.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
STREETPARK M LED PREMIUM HE 5000 STREET-ZEBRA-CROSSING-L E IP66 22 740;Outdoor luminaires;19.3174.0003.22;718 x 311 x 103;mounted on poles;35;3544;101;4000;4000;0.823;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9007 (dark gray);LUXIONA_hardened transparent glass;LED;-40 ÷ 40;54000;L80/B10;>70;0;Rozsył uliczny;IP66;IK09;I;0;0.95;718;311;103;https://luxiona.pl/oferta/oprawy-zewnetrzne/streetpark-m-led-premium/;https://luxiona.pl/oferta/oprawy-zewnetrzne/streetpark-m-led-premium/19.3174.0003.22/;19.3174.0003.22.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
STREETPARK M LED PREMIUM HE 5000 STREET-ZEBRA-CROSSING-P E IP66 22 740;Outdoor luminaires;19.3174.0004.22;718 x 311 x 103;mounted on poles;35;3605;103;4000;4000;0.8371;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9007 (dark gray);LUXIONA_hardened transparent glass;LED;-40 ÷ 40;54000;L80/B10;>70;0;Rozsył uliczny;IP66;IK09;I;0;0.95;718;311;103;https://luxiona.pl/oferta/oprawy-zewnetrzne/streetpark-m-led-premium/;https://luxiona.pl/oferta/oprawy-zewnetrzne/streetpark-m-led-premium/19.3174.0004.22/;19.3174.0004.22.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
STREETPARK M LED PREMIUM HE 10000 STREET-S E IP66 22 757;Outdoor luminaires;19.3174.0005.22;718 x 311 x 103;mounted on poles;71;8076;114;5700;5700;0.7638;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9007 (dark gray);LUXIONA_hardened transparent glass;LED;-40 ÷ 40;60000;L70/B10;>70;0;Rozsył uliczny;IP66;IK09;I;0;0.95;718;311;103;https://luxiona.pl/oferta/oprawy-zewnetrzne/streetpark-m-led-premium/;https://luxiona.pl/oferta/oprawy-zewnetrzne/streetpark-m-led-premium/19.3174.0005.22/;19.3174.0005.22.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
STREETPARK M LED PREMIUM HE 15000 NARROW E IP66 22 757;Outdoor luminaires;19.3174.0006.22;718 x 311 x 103;mounted on poles;106;12621;119;5700;5700;0.7957;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9007 (dark gray);LUXIONA_hardened transparent glass;LED;-40 ÷ 40;60000;L70/B10;>70;0;(C0-C180) / (C90-C270) - 48° / 44,2°;IP66;IK09;I;0;0.95;718;311;103;https://luxiona.pl/oferta/oprawy-zewnetrzne/streetpark-m-led-premium/;https://luxiona.pl/oferta/oprawy-zewnetrzne/streetpark-m-led-premium/19.3174.0006.22/;19.3174.0006.22.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
STREETPARK M LED PREMIUM HO 7500 STREET-M E IP66 22 757;Outdoor luminaires;19.3174.0007.22;718 x 311 x 103;mounted on poles;54;5672;105;5700;5700;0.7614;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9007 (dark gray);LUXIONA_hardened transparent glass;LED;-40 ÷ 40;60000;L70/B10;>70;0;Rozsył uliczny;IP66;IK09;I;0;0.95;718;311;103;https://luxiona.pl/oferta/oprawy-zewnetrzne/streetpark-m-led-premium/;https://luxiona.pl/oferta/oprawy-zewnetrzne/streetpark-m-led-premium/19.3174.0007.22/;19.3174.0007.22.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
STREETPARK M LED PREMIUM HO 15000 STREET-S E IP66 22 757;Outdoor luminaires;19.3174.0008.22;718 x 311 x 103;mounted on poles;107;11381;106;5700;5700;0.7638;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9007 (dark gray);LUXIONA_hardened transparent glass;LED;-40 ÷ 40;60000;L70/B10;>70;0;Rozsył uliczny;IP66;IK09;I;0;0.95;718;311;103;https://luxiona.pl/oferta/oprawy-zewnetrzne/streetpark-m-led-premium/;https://luxiona.pl/oferta/oprawy-zewnetrzne/streetpark-m-led-premium/19.3174.0008.22/;19.3174.0008.22.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
STREETPARK M LED PREMIUM HO 22000 FLOOD E IP66 22 757;Outdoor luminaires;19.3174.0009.22;718 x 311 x 103;mounted on poles;161;17891;111;5700;5700;0.8005;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9007 (dark gray);LUXIONA_hardened transparent glass;LED;-40 ÷ 40;60000;L70/B10;>70;0;(C0-C180) / (C90-C270) - 70° / 70°;IP66;IK09;I;0;0.95;718;311;103;https://luxiona.pl/oferta/oprawy-zewnetrzne/streetpark-m-led-premium/;https://luxiona.pl/oferta/oprawy-zewnetrzne/streetpark-m-led-premium/19.3174.0009.22/;19.3174.0009.22.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
