;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##;EL##OTHER##;EP##OTHER##
UNIVERSAL LINE LED 4400 MICRO-PRM E 24 IP20 840 / L-1159MM;Surface mounted luminaires;19.3127.0001.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;24.7;3792;154;4000;4000;0.8306;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 95,2° / 94,4°;IP20;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0001.24/;19.3127.0001.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE LED 4400 OPTICS-1L E 24 IP20 840 / L-1159MM;Surface mounted luminaires;19.3127.0002.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;24.7;3722;151;4000;4000;0.8154;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 86,8° / 101,6°;IP20;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0002.24/;19.3127.0002.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE LED 4400 OPTICS-1L E 24 IP20 840 LINE-EL / L-1159MM;Surface mounted luminaires;19.3127.0003.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;24.7;3722;151;4000;4000;0.8154;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 86,8° / 101,6°;IP20;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0003.24/;19.3127.0003.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
UNIVERSAL LINE LED 4400 OPTICS-1L E 24 IP20 840 LINE-EP / L-1159MM;Surface mounted luminaires;19.3127.0004.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;24.7;3722;151;4000;4000;0.8154;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 86,8° / 101,6°;IP20;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0004.24/;19.3127.0004.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
UNIVERSAL LINE LED 4400 OPTICS-1L E 24 IP20 840 LINE-S / L-1159MM;Surface mounted luminaires;19.3127.0005.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;24.7;3722;151;4000;4000;0.8154;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 86,8° / 101,6°;IP20;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0005.24/;19.3127.0005.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
UNIVERSAL LINE LED 4400 PLX E 24 IP20 840 / L-1159MM;Surface mounted luminaires;19.3127.0006.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;24.7;3434;139;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP20;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0006.24/;19.3127.0006.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE LED 4400 PLX E 24 IP20 840 LINE-EL / L-1159MM;Surface mounted luminaires;19.3127.0007.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;24.7;3434;139;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP20;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0007.24/;19.3127.0007.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
UNIVERSAL LINE LED 4400 PLX E 24 IP20 840 LINE-EP / L-1159MM;Surface mounted luminaires;19.3127.0008.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;24.7;3434;139;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP20;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0008.24/;19.3127.0008.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
UNIVERSAL LINE LED 4400 PLX E 24 IP20 840 LINE-S / L-1159MM;Surface mounted luminaires;19.3127.0009.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;24.7;3434;139;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP20;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0009.24/;19.3127.0009.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
UNIVERSAL LINE LED 8000 MICRO-PRM E 24 IP20 840 / L-1159MM;Surface mounted luminaires;19.3127.0010.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;53;6919;131;4000;4000;0.8306;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 95,2° / 94,4°;IP20;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0010.24/;19.3127.0010.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE LED 8000 OPTICS-1L E 24 IP20 840 / L-1159MM;Surface mounted luminaires;19.3127.0011.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;53;6792;128;4000;4000;0.8154;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 86,8° / 101,6°;IP20;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0011.24/;19.3127.0011.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE LED 8000 OPTICS-1L E 24 IP20 840 LINE-EL / L-1159MM;Surface mounted luminaires;19.3127.0012.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;53;6792;128;4000;4000;0.8154;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 86,8° / 101,6°;IP20;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0012.24/;19.3127.0012.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
UNIVERSAL LINE LED 8000 OPTICS-1L E 24 IP20 840 LINE-EP / L-1159MM;Surface mounted luminaires;19.3127.0013.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;53;6792;128;4000;4000;0.8154;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 86,8° / 101,6°;IP20;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0013.24/;19.3127.0013.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
UNIVERSAL LINE LED 8000 OPTICS-1L E 24 IP20 840 LINE-S / L-1159MM;Surface mounted luminaires;19.3127.0014.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;53;6792;128;4000;4000;0.8154;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 86,8° / 101,6°;IP20;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0014.24/;19.3127.0014.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
UNIVERSAL LINE LED 8000 PLX E 24 IP20 840 / L-1159MM;Surface mounted luminaires;19.3127.0015.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;53;6266;118;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP20;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0015.24/;19.3127.0015.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE LED 8000 PLX E 24 IP20 840 LINE-EL / L-1159MM;Surface mounted luminaires;19.3127.0016.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;53;6266;118;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP20;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0016.24/;19.3127.0016.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
UNIVERSAL LINE LED 8000 PLX E 24 IP20 840 LINE-EP / L-1159MM;Surface mounted luminaires;19.3127.0017.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;53;6266;118;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP20;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0017.24/;19.3127.0017.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
UNIVERSAL LINE LED 8000 PLX E 24 IP20 840 LINE-S / L-1159MM;Surface mounted luminaires;19.3127.0018.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;53;6266;118;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP20;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0018.24/;19.3127.0018.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
UNIVERSAL LINE LED 8800 OPTICS-1L E 24 IP20 840 / L-2288MM;Surface mounted luminaires;19.3127.0019.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;49.1;7445;152;4000;4000;0.8154;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 86,8° / 101,6°;IP20;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0019.24/;19.3127.0019.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE LED 8800 OPTICS-1L E 24 IP20 840 LINE-EL / L-2288MM;Surface mounted luminaires;19.3127.0020.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;49.1;7445;152;4000;4000;0.8154;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 86,8° / 101,6°;IP20;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0020.24/;19.3127.0020.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
UNIVERSAL LINE LED 8800 OPTICS-1L E 24 IP20 840 LINE-EP / L-2288MM;Surface mounted luminaires;19.3127.0021.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;49.1;7445;152;4000;4000;0.8154;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 86,8° / 101,6°;IP20;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0021.24/;19.3127.0021.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
UNIVERSAL LINE LED 8800 OPTICS-1L E 24 IP20 840 LINE-S / L-2288MM;Surface mounted luminaires;19.3127.0022.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;49.1;7445;152;4000;4000;0.8154;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 86,8° / 101,6°;IP20;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0022.24/;19.3127.0022.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
UNIVERSAL LINE LED 8800 PLX E 24 IP20 840 / L-2288MM;Surface mounted luminaires;19.3127.0023.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;49.1;6868;140;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP20;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0023.24/;19.3127.0023.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE LED 8800 PLX E 24 IP20 840 LINE-EL / L-2288MM;Surface mounted luminaires;19.3127.0024.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;49.1;6868;140;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP20;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0024.24/;19.3127.0024.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
UNIVERSAL LINE LED 8800 PLX E 24 IP20 840 LINE-EP / L-2288MM;Surface mounted luminaires;19.3127.0025.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;49.1;6868;140;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP20;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0025.24/;19.3127.0025.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
UNIVERSAL LINE LED 8800 PLX E 24 IP20 840 LINE-S / L-2288MM;Surface mounted luminaires;19.3127.0026.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;49.1;6868;140;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP20;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0026.24/;19.3127.0026.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
UNIVERSAL LINE LED 16000 MICRO-PRM E 24 IP20 840 / L-2288MM;Surface mounted luminaires;19.3127.0027.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;106;13838;131;4000;4000;0.8306;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 95,2° / 94,4°;IP20;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0027.24/;19.3127.0027.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE LED 16000 OPTICS-1L E 24 IP20 840 / L-2288MM;Surface mounted luminaires;19.3127.0028.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;106;13585;128;4000;4000;0.8154;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 86,8° / 101,6°;IP20;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0028.24/;19.3127.0028.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE LED 16000 OPTICS-1L E 24 IP20 840 LINE-EL / L-2288MM;Surface mounted luminaires;19.3127.0029.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;106;13585;128;4000;4000;0.8154;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 86,8° / 101,6°;IP20;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0029.24/;19.3127.0029.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
UNIVERSAL LINE LED 16000 OPTICS-1L E 24 IP20 840 LINE-EP / L-2288MM;Surface mounted luminaires;19.3127.0030.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;106;13585;128;4000;4000;0.8154;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 86,8° / 101,6°;IP20;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0030.24/;19.3127.0030.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
UNIVERSAL LINE LED 16000 OPTICS-1L E 24 IP20 840 LINE-S / L-2288MM;Surface mounted luminaires;19.3127.0031.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;106;13585;128;4000;4000;0.8154;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_OPTICS;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 86,8° / 101,6°;IP20;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0031.24/;19.3127.0031.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
UNIVERSAL LINE LED 16000 PLX E 24 IP20 840 / L-2288MM;Surface mounted luminaires;19.3127.0032.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;106;12532;118;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP20;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0032.24/;19.3127.0032.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE LED 16000 PLX E 24 IP20 840 LINE-EL / L-2288MM;Surface mounted luminaires;19.3127.0033.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;106;12532;118;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP20;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0033.24/;19.3127.0033.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
UNIVERSAL LINE LED 16000 PLX E 24 IP20 840 LINE-EP / L-2288MM;Surface mounted luminaires;19.3127.0034.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;106;12532;118;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP20;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0034.24/;19.3127.0034.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
UNIVERSAL LINE LED 16000 PLX E 24 IP20 840 LINE-S / L-2288MM;Surface mounted luminaires;19.3127.0035.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;106;12532;118;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP20;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-nastropowe/universal-line-led/19.3127.0035.24/;19.3127.0035.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
UNIVERSAL LINE LED 4400 PLX E 24 IP65 840 KRW3K / L-1159MM;Industrial luminaires;19.3127.0037.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;24.7;3434;139;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP65;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/19.3127.0037.24/;19.3127.0037.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE LED 4400 PLX E 24 IP65 840 LINE-EL KRW5K / L-1159MM;Industrial luminaires;19.3127.0038.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;24.7;3434;139;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP65;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/19.3127.0038.24/;19.3127.0038.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
UNIVERSAL LINE LED 4400 PLX E 24 IP65 840 LINE-EP / L-1159MM;Industrial luminaires;19.3127.0039.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;24.7;3434;139;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP65;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/19.3127.0039.24/;19.3127.0039.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
UNIVERSAL LINE LED 4400 PLX E 24 IP65 840 LINE-S / L-1159MM;Industrial luminaires;19.3127.0040.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;24.7;3434;139;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP65;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/19.3127.0040.24/;19.3127.0040.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
UNIVERSAL LINE LED 8000 MICRO-PRM E 24 IP65 840 KRW3K / L-1159MM;Industrial luminaires;19.3127.0041.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;53;6919;131;4000;4000;0.8306;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 95,2° / 94,4°;IP65;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/19.3127.0041.24/;19.3127.0041.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE LED 8000 PLX E 24 IP65 840 KRW3K / L-1159MM;Industrial luminaires;19.3127.0042.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;53;6266;118;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP65;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/19.3127.0042.24/;19.3127.0042.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE LED 8000 PLX E 24 IP65 840 LINE-EL KRW5K / L-1159MM;Industrial luminaires;19.3127.0043.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;53;6266;118;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP65;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/19.3127.0043.24/;19.3127.0043.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
UNIVERSAL LINE LED 8000 PLX E 24 IP65 840 LINE-EP / L-1159MM;Industrial luminaires;19.3127.0044.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;53;6266;118;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP65;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/19.3127.0044.24/;19.3127.0044.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
UNIVERSAL LINE LED 8000 PLX E 24 IP65 840 LINE-S / L-1159MM;Industrial luminaires;19.3127.0045.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;53;6266;118;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP65;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/19.3127.0045.24/;19.3127.0045.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
UNIVERSAL LINE LED 8800 MICRO-PRM E 24 IP65 840 KRW3K / L-2288MM;Industrial luminaires;19.3127.0046.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;49.1;7583;154;4000;4000;0.8306;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM;LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 95,2° / 94,4°;IP65;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/19.3127.0046.24/;19.3127.0046.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE LED 8800 PLX E 24 IP65 840 KRW3K / L-2288MM;Industrial luminaires;19.3127.0047.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;49.1;6868;140;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP65;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/19.3127.0047.24/;19.3127.0047.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE LED 8800 PLX E 24 IP65 840 LINE-EL KRW5K / L-2288MM;Industrial luminaires;19.3127.0048.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;49.1;6868;140;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP65;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/19.3127.0048.24/;19.3127.0048.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
UNIVERSAL LINE LED 8800 PLX E 24 IP65 840 LINE-EP / L-2288MM;Industrial luminaires;19.3127.0049.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;49.1;6868;140;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP65;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/19.3127.0049.24/;19.3127.0049.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
UNIVERSAL LINE LED 8800 PLX E 24 IP65 840 LINE-S / L-2288MM;Industrial luminaires;19.3127.0050.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;49.1;6868;140;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP65;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/19.3127.0050.24/;19.3127.0050.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
UNIVERSAL LINE LED 16000 PLX E 24 IP65 840 KRW3K / L-2288MM;Industrial luminaires;19.3127.0051.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;106;12532;118;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP65;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/19.3127.0051.24/;19.3127.0051.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE LED 16000 PLX E 24 IP65 840 LINE-EL KRW5K / L-2288MM;Industrial luminaires;19.3127.0052.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;106;12532;118;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP65;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/19.3127.0052.24/;19.3127.0052.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;0
UNIVERSAL LINE LED 16000 PLX E 24 IP65 840 LINE-EP / L-2288MM;Industrial luminaires;19.3127.0053.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;106;12532;118;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP65;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/19.3127.0053.24/;19.3127.0053.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;1
UNIVERSAL LINE LED 16000 PLX E 24 IP65 840 LINE-S / L-2288MM;Industrial luminaires;19.3127.0054.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;106;12532;118;4000;4000;0.7522;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP65;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/;https://luxiona.pl/oferta/oprawy-przemyslowe/universal-line-led/19.3127.0054.24/;19.3127.0054.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;0;0
UNIVERSAL LINE OUTDOOR LED 2200 SHM E 24 IP55 830 KRW3K / L-595MM;Outdoor luminaires;19.3180.0007.24;595 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;13;1758;135;3000;3000;0.7982;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_SHM (hardened mat glass);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP55;IK04;I;0;0.95;595;60;75;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/19.3180.0007.24/;19.3180.0007.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE OUTDOOR LED 2200 SHM E 24 IP55 840 KRW3K / L-595MM;Outdoor luminaires;19.3180.0001.24;595 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;13;1822;140;4000;4000;0.7982;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_SHM (hardened mat glass);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP55;IK04;I;0;0.95;595;60;75;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/19.3180.0001.24/;19.3180.0001.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE OUTDOOR LED 2200 SHM EDD 24 IP55 830 KRW5K / L-595MM;Outdoor luminaires;19.3180.0008.24;595 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;13;1758;135;3000;3000;0.7982;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_SHM (hardened mat glass);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP55;IK04;I;0;0.95;595;60;75;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/19.3180.0008.24/;19.3180.0008.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE OUTDOOR LED 2200 SHM EDD 24 IP55 840 KRW5K / L-595MM;Outdoor luminaires;19.3180.0002.24;595 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;13;1822;140;4000;4000;0.7982;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_SHM (hardened mat glass);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP55;IK04;I;0;0.95;595;60;75;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/19.3180.0002.24/;19.3180.0002.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE OUTDOOR LED 4400 SHM E 24 IP55 830 KRW3K / L-1159MM;Outdoor luminaires;19.3180.0009.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;25;3517;141;3000;3000;0.7982;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_SHM (hardened mat glass);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP55;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/19.3180.0009.24/;19.3180.0009.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE OUTDOOR LED 4400 SHM E 24 IP55 840 KRW3K / L-1159MM;Outdoor luminaires;19.3180.0003.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;25;3644;146;4000;4000;0.7982;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_SHM (hardened mat glass);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP55;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/19.3180.0003.24/;19.3180.0003.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE OUTDOOR LED 4400 SHM EDD 24 IP55 830 KRW5K / L-1159MM;Outdoor luminaires;19.3180.0010.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;25;3517;141;3000;3000;0.7982;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_SHM (hardened mat glass);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP55;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/19.3180.0010.24/;19.3180.0010.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE OUTDOOR LED 4400 SHM EDD 24 IP55 840 KRW5K / L-1159MM;Outdoor luminaires;19.3180.0004.24;1159 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;25;3644;146;4000;4000;0.7982;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_SHM (hardened mat glass);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP55;IK04;I;0;0.95;1159;60;75;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/19.3180.0004.24/;19.3180.0004.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE OUTDOOR LED 8800 SHM E 24 IP55 830 KRW3K / L-2288MM;Outdoor luminaires;19.3180.0011.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;49;7033;144;3000;3000;0.7982;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_SHM (hardened mat glass);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP55;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/19.3180.0011.24/;19.3180.0011.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE OUTDOOR LED 8800 SHM E 24 IP55 840 KRW3K / L-2288MM;Outdoor luminaires;19.3180.0005.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;49;7288;149;4000;4000;0.7982;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_SHM (hardened mat glass);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP55;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/19.3180.0005.24/;19.3180.0005.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE OUTDOOR LED 8800 SHM EDD 24 IP55 830 KRW5K / L-2288MM;Outdoor luminaires;19.3180.0012.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;49;7033;144;3000;3000;0.7982;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_SHM (hardened mat glass);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP55;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/19.3180.0012.24/;19.3180.0012.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
UNIVERSAL LINE OUTDOOR LED 8800 SHM EDD 24 IP55 840 KRW5K / L-2288MM;Outdoor luminaires;19.3180.0006.24;2288 x 60 x 75;directly mounted to ceiling construction or surface mounted on slings;49;7288;149;4000;4000;0.7982;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_SHM (hardened mat glass);LED;-25 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109,6° / 109,6°;IP55;IK04;I;0;0.95;2288;60;75;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/;https://luxiona.pl/oferta/oprawy-zewnetrzne/universal-line-led/19.3180.0006.24/;19.3180.0006.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA;1;1
