;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
X-LINE LED 5200 MICRO-PRM E 24 830 LINE-S / CONNECTOR TYPE-X 600/600/600/600;Surface mounted luminaires;19.3106.0017.24;1126/1126 x 60 x 71;directly mounted to ceiling construction or surface mounted on slings;28.2;3804;135;3000;3000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP44;IK04;I;0;0.95;1126;60;71;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/19.3106.0017.24/;19.3106.0017.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE LED 5200 MICRO-PRM E 24 840 LINE-S / CONNECTOR TYPE-X 600/600/600/600;Surface mounted luminaires;19.3106.0018.24;1126/1126 x 60 x 71;directly mounted to ceiling construction or surface mounted on slings;28.2;3942;140;4000;4000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP44;IK04;I;0;0.95;1126;60;71;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/19.3106.0018.24/;19.3106.0018.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE LED 5200 MICRO-PRM EDD 24 830 LINE-1S / CONNECTOR TYPE-X 600/600/600/600;Surface mounted luminaires;19.3106.0003.24;1126/1126 x 60 x 71;directly mounted to ceiling construction or surface mounted on slings;28.2;3804;135;3000;3000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP44;IK04;I;0;0.95;1126;60;71;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/19.3106.0003.24/;19.3106.0003.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE LED 5200 MICRO-PRM EDD 24 840 LINE-1S / CONNECTOR TYPE-X 600/600/600/600;Surface mounted luminaires;19.3106.0004.24;1126/1126 x 60 x 71;directly mounted to ceiling construction or surface mounted on slings;28.2;3942;140;4000;4000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP44;IK04;I;0;0.95;1126;60;71;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/19.3106.0004.24/;19.3106.0004.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE LED 5200 PLX E 24 830 LINE-S / CONNECTOR TYPE-X 600/600/600/600;Surface mounted luminaires;19.3106.0005.24;1126/1126 x 60 x 71;directly mounted to ceiling construction or surface mounted on slings;28.2;3367;119;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP44;IK04;I;0;0.95;1126;60;71;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/19.3106.0005.24/;19.3106.0005.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE LED 5200 PLX E 24 840 LINE-S / CONNECTOR TYPE-X 600/600/600/600;Surface mounted luminaires;19.3106.0006.24;1126/1126 x 60 x 71;directly mounted to ceiling construction or surface mounted on slings;28.2;3489;124;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP44;IK04;I;0;0.95;1126;60;71;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/19.3106.0006.24/;19.3106.0006.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE LED 5200 PLX EDD 24 830 LINE-1S / CONNECTOR TYPE-X 600/600/600/600;Surface mounted luminaires;19.3106.0007.24;1126/1126 x 60 x 71;directly mounted to ceiling construction or surface mounted on slings;28.2;3367;119;3000;3000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP44;IK04;I;0;0.95;1126;60;71;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/19.3106.0007.24/;19.3106.0007.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE LED 5200 PLX EDD 24 840 LINE-1S / CONNECTOR TYPE-X 600/600/600/600;Surface mounted luminaires;19.3106.0008.24;1126/1126 x 60 x 71;directly mounted to ceiling construction or surface mounted on slings;28.2;3489;124;4000;4000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP44;IK04;I;0;0.95;1126;60;71;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/19.3106.0008.24/;19.3106.0008.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE LED 8800 MICRO-PRM E 24 830 LINE-S / CONNECTOR TYPE-X 600/600/600/600;Surface mounted luminaires;19.3106.0009.24;1126/1126 x 60 x 71;directly mounted to ceiling construction or surface mounted on slings;49.1;6636;135;3000;3000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP44;IK04;I;0;0.95;1126;60;71;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/19.3106.0009.24/;19.3106.0009.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE LED 8800 MICRO-PRM E 24 840 LINE-S / CONNECTOR TYPE-X 600/600/600/600;Surface mounted luminaires;19.3106.0010.24;1126/1126 x 60 x 71;directly mounted to ceiling construction or surface mounted on slings;49.1;6877;140;4000;4000;0.7532;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP44;IK04;I;0;0.95;1126;60;71;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/19.3106.0010.24/;19.3106.0010.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE LED 8800 MICRO-PRM EDD 24 830 LINE-1S / CONNECTOR TYPE-X 600/600/600/600;Surface mounted luminaires;19.3106.0011.24;1126/1126 x 60 x 71;directly mounted to ceiling construction or surface mounted on slings;49.1;6636;135;3000;3000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP44;IK04;I;0;0.95;1126;60;71;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/19.3106.0011.24/;19.3106.0011.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE LED 8800 MICRO-PRM EDD 24 840 LINE-1S / CONNECTOR TYPE-X 600/600/600/600;Surface mounted luminaires;19.3106.0012.24;1126/1126 x 60 x 71;directly mounted to ceiling construction or surface mounted on slings;49.1;6877;140;4000;4000;0.7532;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_Micro-PRM (micro-prismatic diffuser PMMA);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 82,8° / 97,2°;IP44;IK04;I;0;0.95;1126;60;71;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/19.3106.0012.24/;19.3106.0012.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE LED 8800 PLX E 24 830 LINE-S / CONNECTOR TYPE-X 600/600/600/600;Surface mounted luminaires;19.3106.0013.24;1126/1126 x 60 x 71;directly mounted to ceiling construction or surface mounted on slings;49.1;5873;120;3000;3000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP44;IK04;I;0;0.95;1126;60;71;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/19.3106.0013.24/;19.3106.0013.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE LED 8800 PLX E 24 840 LINE-S / CONNECTOR TYPE-X 600/600/600/600;Surface mounted luminaires;19.3106.0014.24;1126/1126 x 60 x 71;directly mounted to ceiling construction or surface mounted on slings;49.1;6086;124;4000;4000;0.6666;standard (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP44;IK04;I;0;0.95;1126;60;71;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/19.3106.0014.24/;19.3106.0014.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE LED 8800 PLX EDD 24 830 LINE-1S / CONNECTOR TYPE-X 600/600/600/600;Surface mounted luminaires;19.3106.0015.24;1126/1126 x 60 x 71;directly mounted to ceiling construction or surface mounted on slings;49.1;5873;120;3000;3000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP44;IK04;I;0;0.95;1126;60;71;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/19.3106.0015.24/;19.3106.0015.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE LED 8800 PLX EDD 24 840 LINE-1S / CONNECTOR TYPE-X 600/600/600/600;Surface mounted luminaires;19.3106.0016.24;1126/1126 x 60 x 71;directly mounted to ceiling construction or surface mounted on slings;49.1;6086;124;4000;4000;0.6666;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_anodised aluminum;LUXIONA_PLX (PMMA opal);LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B50 (2);>80;3;(C0-C180) / (C90-C270) - 109° / 107,2°;IP44;IK04;I;0;0.95;1126;60;71;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/;https://luxiona.pl/oferta/oprawy-nastropowe/x-line-led-connector-x/19.3106.0016.24/;19.3106.0016.24.IES;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
